{"text_format":"2","workbook":"xlsx","n_sheets":45,"sheets":["HAND LEVER","HAND WHEEL","PLUG VALVE_5","GLOBE VALVE_2","CHECK VALVE_1","GLOBE VALVE_1","GATE VALVE_5","GATE VALVE_4","PLUG VALVE_4","PLUG VALVE_3","BUTTERFLY VALVE_1","PLUG VALVE_2","PLUG VALVE_1","BALL VALVE_1","PLUG VALVE","BALL VALVE","BUTTERFLY VALVE","CHECK VALVE","GLOBE VALVE","GATE VALVE_3","GATE VALVE_2","GATE VALVE_1","GATE VALVE","TEE (RED)","TEE_1","TEE","REDUCER (CONC)","REDUCER (ECC)","PIPE, SEAMLESS","SOCKOLET","GASKET","GASKET, SWG","FLANGE WN","FLANGE SW","ELL 45","ELL 45 LR","ELL 90","ELL 90 LR","STREET ELL","COUPLING","CAP_1","CAP","BOLT SET_1","BOLT SET","FLANGE BLIND"],"not_rendered":{"charts":0,"images":28,"macros":0,"external_links":0,"defined_names":0,"comments":45,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"HAND LEVER","index":0,"n_rows":145,"n_cols":56,"rows_kept":145,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","L","H","DO","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","L","H","DO","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,null,"CPVX008","16","20","0","L,H,DO,","9bc59a01-dfdc-495b-bbdf-b5e876c2e233","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=20\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","20","16",null,"ValveActuator",null,"123"]
[null,null,"CPVX008","16","22","0","L,H,DO,","7320d51e-92e3-4406-946b-c2677e6bf68b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=22\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","22","16",null,"ValveActuator",null,"124"]
[null,null,"CPVX008","14","8","0","L,H,DO,","0bb4b333-0cca-4114-a794-8ef777a0aec9","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8","14",null,"ValveActuator",null,"125"]
[null,null,"CPVX008","14","12","0","L,H,DO,","0d9b5135-4fc3-40db-b8cc-9955f70d82f5","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=12\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","12","14",null,"ValveActuator",null,"126"]
[null,null,"CPVX008","10.5","5.5","0","L,H,DO,","81d8de36-487e-43e8-a118-bee64679be4f","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 1/2\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.5","10.5",null,"ValveActuator",null,"127"]
[null,null,"CPVX008","14","11","0","L,H,DO,","df388247-531c-47ef-bbe7-b63d17abdead","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11","14",null,"ValveActuator",null,"129"]
[null,null,"CPVX008","16","19","0","L,H,DO,","a811db4b-e49b-4978-a35f-cb9c19558fd1","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=19\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","19","16",null,"ValveActuator",null,"130"]
[null,null,"CPVX008","14","14","0","L,H,DO,","98899958-b00c-419a-b9a9-1be7902cd941","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=14\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","14","14",null,"ValveActuator",null,"131"]
[null,null,"CPVX008","6.5","4.75","0","L,H,DO,","b1f8b162-a8db-43b9-bf35-537ed298e07a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4 3/4\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4.75","6.5",null,"ValveActuator",null,"132"]
[null,null,"CPVX008","14","9","0","L,H,DO,","dcb67e85-ba74-4252-8d70-c13a0eb17c1c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=9\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","9","14",null,"ValveActuator",null,"133"]
[null,null,"CPVX008","14","13","0","L,H,DO,","7d07ce87-7155-4217-a375-e784f9501de6","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","14",null,"ValveActuator",null,"134"]
[null,null,"CPVX008","14","10","0","L,H,DO,","c9366c8b-c436-460a-97c5-ae5419e5aa2d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=10\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","10","14",null,"ValveActuator",null,"135"]
[null,null,"CPVX008","10.5","7","0","L,H,DO,","0b48c097-258b-4e07-99a2-75ab6e1de5a2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7","10.5",null,"ValveActuator",null,"136"]
[null,null,"CPVX008","16","17","0","L,H,DO,","140daba8-eca6-4b10-8453-23e47ffa713d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=17\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","17","16",null,"ValveActuator",null,"137"]
[null,null,"CPVX008","10.5","5","0","L,H,DO,","de0125b4-373e-464d-b3fb-1c3d13be8ba9","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5","10.5",null,"ValveActuator",null,"138"]
[null,null,"CPVX008","14","16","0","L,H,DO,","c6cb6dce-1151-4467-bc57-ebe08050091c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16","14",null,"ValveActuator",null,"139"]
[null,null,"CPVX008","16","18","0","L,H,DO,","a4005ed0-298d-4584-ba75-a08e057a73bf","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=18\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","18","16",null,"ValveActuator",null,"140"]
[null,null,"CPVX008","6.5","4.5","0","L,H,DO,","d81efdd5-2420-4cfc-9293-bd52bdc68339","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4 1/2\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4.5","6.5",null,"ValveActuator",null,"141"]
[null,null,"CPVX008","16","21","0","L,H,DO,","801bc4ee-daeb-4b63-8e9a-0072064e67e2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21","16",null,"ValveActuator",null,"142"]
[null,null,"CPVX008","16","20","0","L,H,DO,","9bc59a01-dfdc-495b-bbdf-b5e876c2e233","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=20\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","20","16",null,"ValveActuator",null,"205"]
[null,null,"CPVX008","16","22","0","L,H,DO,","7320d51e-92e3-4406-946b-c2677e6bf68b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=22\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","22","16",null,"ValveActuator",null,"206"]
[null,null,"CPVX008","14","8","0","L,H,DO,","0bb4b333-0cca-4114-a794-8ef777a0aec9","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8","14",null,"ValveActuator",null,"207"]
[null,null,"CPVX008","14","12","0","L,H,DO,","0d9b5135-4fc3-40db-b8cc-9955f70d82f5","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=12\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","12","14",null,"ValveActuator",null,"208"]
[null,null,"CPVX008","10.5","5.5","0","L,H,DO,","81d8de36-487e-43e8-a118-bee64679be4f","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 1/2\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.5","10.5",null,"ValveActuator",null,"209"]
[null,null,"CPVX008","14","11","0","L,H,DO,","df388247-531c-47ef-bbe7-b63d17abdead","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11","14",null,"ValveActuator",null,"210"]
[null,null,"CPVX008","16","19","0","L,H,DO,","a811db4b-e49b-4978-a35f-cb9c19558fd1","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=19\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","19","16",null,"ValveActuator",null,"211"]
[null,null,"CPVX008","14","14","0","L,H,DO,","98899958-b00c-419a-b9a9-1be7902cd941","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=14\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","14","14",null,"ValveActuator",null,"212"]
[null,null,"CPVX008","6.5","4.75","0","L,H,DO,","b1f8b162-a8db-43b9-bf35-537ed298e07a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4 3/4\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4.75","6.5",null,"ValveActuator",null,"213"]
[null,null,"CPVX008","14","9","0","L,H,DO,","dcb67e85-ba74-4252-8d70-c13a0eb17c1c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=9\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","9","14",null,"ValveActuator",null,"214"]
[null,null,"CPVX008","14","13","0","L,H,DO,","7d07ce87-7155-4217-a375-e784f9501de6","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","14",null,"ValveActuator",null,"215"]
[null,null,"CPVX008","14","10","0","L,H,DO,","c9366c8b-c436-460a-97c5-ae5419e5aa2d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=10\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","10","14",null,"ValveActuator",null,"216"]
[null,null,"CPVX008","10.5","7","0","L,H,DO,","0b48c097-258b-4e07-99a2-75ab6e1de5a2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7","10.5",null,"ValveActuator",null,"217"]
[null,null,"CPVX008","16","17","0","L,H,DO,","140daba8-eca6-4b10-8453-23e47ffa713d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=17\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","17","16",null,"ValveActuator",null,"218"]
[null,null,"CPVX008","10.5","5","0","L,H,DO,","de0125b4-373e-464d-b3fb-1c3d13be8ba9","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5","10.5",null,"ValveActuator",null,"219"]
[null,null,"CPVX008","14","16","0","L,H,DO,","c6cb6dce-1151-4467-bc57-ebe08050091c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16","14",null,"ValveActuator",null,"220"]
[null,null,"CPVX008","16","18","0","L,H,DO,","a4005ed0-298d-4584-ba75-a08e057a73bf","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=18\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","18","16",null,"ValveActuator",null,"221"]
[null,null,"CPVX008","6.5","4.5","0","L,H,DO,","d81efdd5-2420-4cfc-9293-bd52bdc68339","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4 1/2\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4.5","6.5",null,"ValveActuator",null,"222"]
[null,null,"CPVX008","16","21","0","L,H,DO,","801bc4ee-daeb-4b63-8e9a-0072064e67e2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21","16",null,"ValveActuator",null,"223"]
[null,null,"CPVX008","16","20","0","L,H,DO,","9bc59a01-dfdc-495b-bbdf-b5e876c2e233","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=20\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","20","16",null,"ValveActuator",null,"3406"]
[null,null,"CPVX008","16","22","0","L,H,DO,","7320d51e-92e3-4406-946b-c2677e6bf68b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=22\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","22","16",null,"ValveActuator",null,"3407"]
[null,null,"CPVX008","14","8","0","L,H,DO,","0bb4b333-0cca-4114-a794-8ef777a0aec9","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8","14",null,"ValveActuator",null,"3408"]
[null,null,"CPVX008","14","12","0","L,H,DO,","0d9b5135-4fc3-40db-b8cc-9955f70d82f5","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=12\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","12","14",null,"ValveActuator",null,"3409"]
[null,null,"CPVX008","10.5","5.5","0","L,H,DO,","81d8de36-487e-43e8-a118-bee64679be4f","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 1/2\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.5","10.5",null,"ValveActuator",null,"3410"]
[null,null,"CPVX008","14","11","0","L,H,DO,","df388247-531c-47ef-bbe7-b63d17abdead","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11","14",null,"ValveActuator",null,"3411"]
[null,null,"CPVX008","16","19","0","L,H,DO,","a811db4b-e49b-4978-a35f-cb9c19558fd1","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=19\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","19","16",null,"ValveActuator",null,"3412"]
[null,null,"CPVX008","14","14","0","L,H,DO,","98899958-b00c-419a-b9a9-1be7902cd941","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=14\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","14","14",null,"ValveActuator",null,"3413"]
[null,null,"CPVX008","6.5","4.75","0","L,H,DO,","b1f8b162-a8db-43b9-bf35-537ed298e07a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4 3/4\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4.75","6.5",null,"ValveActuator",null,"3414"]
[null,null,"CPVX008","14","9","0","L,H,DO,","dcb67e85-ba74-4252-8d70-c13a0eb17c1c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=9\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","9","14",null,"ValveActuator",null,"3415"]
[null,null,"CPVX008","14","13","0","L,H,DO,","7d07ce87-7155-4217-a375-e784f9501de6","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","14",null,"ValveActuator",null,"3416"]
[null,null,"CPVX008","14","10","0","L,H,DO,","c9366c8b-c436-460a-97c5-ae5419e5aa2d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=10\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","10","14",null,"ValveActuator",null,"3417"]
[null,null,"CPVX008","10.5","7","0","L,H,DO,","0b48c097-258b-4e07-99a2-75ab6e1de5a2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7","10.5",null,"ValveActuator",null,"3418"]
[null,null,"CPVX008","16","17","0","L,H,DO,","140daba8-eca6-4b10-8453-23e47ffa713d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=17\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","17","16",null,"ValveActuator",null,"3419"]
[null,null,"CPVX008","10.5","5","0","L,H,DO,","de0125b4-373e-464d-b3fb-1c3d13be8ba9","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5","10.5",null,"ValveActuator",null,"3420"]
[null,null,"CPVX008","14","16","0","L,H,DO,","c6cb6dce-1151-4467-bc57-ebe08050091c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16","14",null,"ValveActuator",null,"3421"]
[null,null,"CPVX008","16","18","0","L,H,DO,","a4005ed0-298d-4584-ba75-a08e057a73bf","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=18\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","18","16",null,"ValveActuator",null,"3422"]
[null,null,"CPVX008","6.5","4.5","0","L,H,DO,","d81efdd5-2420-4cfc-9293-bd52bdc68339","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4 1/2\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4.5","6.5",null,"ValveActuator",null,"3423"]
[null,null,"CPVX008","16","21","0","L,H,DO,","801bc4ee-daeb-4b63-8e9a-0072064e67e2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21\", W=16\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21","16",null,"ValveActuator",null,"3424"]
[null,null,"CPVX008","10.5","5.69","0","L,H,DO,","f40acc41-aa31-4dd1-9428-c99dda8d6c23","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 69/100\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.69","10.5",null,"ValveActuator",null,"3478"]
[null,null,"CPVX008","14","11.5","0","L,H,DO,","ddcb694e-a0f1-411a-b499-42359fc626dc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","14",null,"ValveActuator",null,"3479"]
[null,null,"CPVX008","14","13.5","0","L,H,DO,","7ad52f56-e93d-4c01-9400-093773391624","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","14",null,"ValveActuator",null,"3480"]
[null,null,"CPVX008","14","15.25","0","L,H,DO,","9a0dc275-cb55-4643-b2f3-af5e55bae7f6","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 1/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.25","14",null,"ValveActuator",null,"3481"]
[null,null,"CPVX008","14","16.25","0","L,H,DO,","4fc00a7c-91b6-4d8c-9542-a57ce77d839d","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.25","14",null,"ValveActuator",null,"3482"]
[null,null,"CPVX008","6.5","4","0","L,H,DO,","02c4c27f-4ae3-4bd2-9e91-ae3be54d166a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4","6.5",null,"ValveActuator",null,"3483"]
[null,null,"CPVX008","14","8.75","0","L,H,DO,","c27da085-ef36-4e79-86d1-0af7d4ad54a7","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","14",null,"ValveActuator",null,"3484"]
[null,null,"CPVX008","6.5","3.63","0","L,H,DO,","351cdd93-c271-4bac-b995-050a67fdf152","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=3 63/100\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","3.63","6.5",null,"ValveActuator",null,"3485"]
[null,null,"CPVX008","10.5","7","0","L,H,DO,","0b48c097-258b-4e07-99a2-75ab6e1de5a2","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7","10.5",null,"ValveActuator",null,"3486"]
[null,null,"CPVX008","14","21.5","0","L,H,DO,","9b9df8f6-06f0-44a4-8291-961395f9ca60","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21.5","14",null,"ValveActuator",null,"3487"]
[null,null,"CPVX008","14","16.5","0","L,H,DO,","e3817f3d-3795-461a-9d63-f89ce6a43eba","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.5","14",null,"ValveActuator",null,"3537"]
[null,null,"CPVX008","14","10.25","0","L,H,DO,","5a101043-71bb-43ee-b8b1-f88ffc9fd7b0","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=10 1/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","10.25","14",null,"ValveActuator",null,"3538"]
[null,null,"CPVX008","14","11.5","0","L,H,DO,","ddcb694e-a0f1-411a-b499-42359fc626dc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","14",null,"ValveActuator",null,"3539"]
[null,null,"CPVX008","10.5","8.75","0","L,H,DO,","5559017f-64c8-4534-a5ec-c0c8fa2b960b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","10.5",null,"ValveActuator",null,"3540"]
[null,null,"CPVX008","6.5","7","0","L,H,DO,","14a38483-5252-44c9-b313-4af077f430a4","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7","6.5",null,"ValveActuator",null,"3541"]
[null,null,"CPVX008","10.5","8.25","0","L,H,DO,","d314328f-b36d-4733-b422-f6f5023d8a90","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 1/4\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.25","10.5",null,"ValveActuator",null,"3542"]
[null,null,"CPVX008","10.5","7.75","0","L,H,DO,","3eafb794-44d6-4307-81eb-bfb9b676421e","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7 3/4\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7.75","10.5",null,"ValveActuator",null,"3543"]
[null,null,"CPVX008","14","14.5","0","L,H,DO,","e681b696-660d-46c3-a52d-02765ba90bec","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=14 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","14.5","14",null,"ValveActuator",null,"3544"]
[null,null,"CPVX008","14","15.75","0","L,H,DO,","45730dd4-988d-48e3-978e-5de04277f5dc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 3/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.75","14",null,"ValveActuator",null,"3545"]
[null,null,"CPVX008","14","21","0","L,H,DO,","b72129de-f087-4db9-9c9b-3793a4ce05bf","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21","14",null,"ValveActuator",null,"3546"]
[null,null,"CPVX008","14","18.75","0","L,H,DO,","27092ef5-afd7-4ded-987f-99fce4e691cc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=18 3/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","18.75","14",null,"ValveActuator",null,"3547"]
[null,null,"CPVX008","14","13.25","0","L,H,DO,","cea247f5-355c-40af-84eb-eddcd1f98df3","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.25","14",null,"ValveActuator",null,"3548"]
[null,null,"CPVX008","14","16.5","0","L,H,DO,","e3817f3d-3795-461a-9d63-f89ce6a43eba","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.5","14",null,"ValveActuator",null,"3583"]
[null,null,"CPVX008","14","10.25","0","L,H,DO,","5a101043-71bb-43ee-b8b1-f88ffc9fd7b0","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=10 1/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","10.25","14",null,"ValveActuator",null,"3584"]
[null,null,"CPVX008","14","11.5","0","L,H,DO,","ddcb694e-a0f1-411a-b499-42359fc626dc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","14",null,"ValveActuator",null,"3585"]
[null,null,"CPVX008","10.5","8.75","0","L,H,DO,","5559017f-64c8-4534-a5ec-c0c8fa2b960b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","10.5",null,"ValveActuator",null,"3586"]
[null,null,"CPVX008","6.5","7","0","L,H,DO,","14a38483-5252-44c9-b313-4af077f430a4","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7\", W=6 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7","6.5",null,"ValveActuator",null,"3587"]
[null,null,"CPVX008","10.5","8.25","0","L,H,DO,","d314328f-b36d-4733-b422-f6f5023d8a90","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 1/4\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.25","10.5",null,"ValveActuator",null,"3588"]
[null,null,"CPVX008","10.5","7.75","0","L,H,DO,","3eafb794-44d6-4307-81eb-bfb9b676421e","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7 3/4\", W=10 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7.75","10.5",null,"ValveActuator",null,"3589"]
[null,null,"CPVX008","14","14.5","0","L,H,DO,","e681b696-660d-46c3-a52d-02765ba90bec","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=14 1/2\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","14.5","14",null,"ValveActuator",null,"3590"]
[null,null,"CPVX008","14","15.75","0","L,H,DO,","45730dd4-988d-48e3-978e-5de04277f5dc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 3/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.75","14",null,"ValveActuator",null,"3591"]
[null,null,"CPVX008","14","21","0","L,H,DO,","b72129de-f087-4db9-9c9b-3793a4ce05bf","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21","14",null,"ValveActuator",null,"3592"]
[null,null,"CPVX008","14","18.75","0","L,H,DO,","27092ef5-afd7-4ded-987f-99fce4e691cc","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=18 3/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","18.75","14",null,"ValveActuator",null,"3593"]
[null,null,"CPVX008","14","13.25","0","L,H,DO,","cea247f5-355c-40af-84eb-eddcd1f98df3","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/4\", W=14\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.25","14",null,"ValveActuator",null,"3594"]
[null,null,"CPVX008","18","4","0","L,H,DO,","ba14331c-3cfe-463c-abca-3a629699735a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4\", W=18\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4","18",null,"ValveActuator",null,"4158"]
[null,null,"CPVX008","30","16.25","0","L,H,DO,","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.25","30",null,"ValveActuator",null,"4159"]
[null,null,"CPVX008","30","13.5","0","L,H,DO,","5c04ba24-a4ed-4794-a425-069eb5c978ed","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","30",null,"ValveActuator",null,"4160"]
[null,null,"CPVX008","30","8.75","0","L,H,DO,","3b428250-2347-4a52-9bb5-8497ecb0f6dd","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","30",null,"ValveActuator",null,"4161"]
[null,null,"CPVX008","8.75","2.88","0","L,H,DO,","37894da0-c8af-467e-ad0c-c1b2f6e65219","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=2 22/25\", W=8 3/4\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","2.88","8.75",null,"ValveActuator",null,"4162"]
[null,null,"CPVX008","12.5","3.6","0","L,H,DO,","95f070a6-4fd5-4323-a634-1ba9ed7e13fb","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=3 3/5\", W=12 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","3.6","12.5",null,"ValveActuator",null,"4163"]
[null,null,"CPVX008","24","5.7","0","L,H,DO,","bae61cb2-cd55-422f-b094-cbcf4aec2474","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 7/10\", W=24\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.7","24",null,"ValveActuator",null,"4164"]
[null,null,"CPVX008","30","11.5","0","L,H,DO,","b985b3ec-3421-4a14-b498-3d5f49b52589","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","30",null,"ValveActuator",null,"4165"]
[null,null,"CPVX008","26.5354","8.7402","0","L,H,DO,","d81badf1-6af2-4061-a972-33a3924e8242","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 161/217\", W=26 127/238\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.7402","26.5354",null,"ValveActuator",null,"4166"]
[null,null,"CPVX008","30","15.25","0","L,H,DO,","4011aff6-fa15-409c-a0d0-5cc7734c9887","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.25","30",null,"ValveActuator",null,"4167"]
[null,null,"CPVX008","18","4","0","L,H,DO,","ba14331c-3cfe-463c-abca-3a629699735a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4\", W=18\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4","18",null,"ValveActuator",null,"4190"]
[null,null,"CPVX008","30","16.25","0","L,H,DO,","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.25","30",null,"ValveActuator",null,"4191"]
[null,null,"CPVX008","30","13.5","0","L,H,DO,","5c04ba24-a4ed-4794-a425-069eb5c978ed","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","30",null,"ValveActuator",null,"4192"]
[null,null,"CPVX008","30","8.75","0","L,H,DO,","3b428250-2347-4a52-9bb5-8497ecb0f6dd","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","30",null,"ValveActuator",null,"4193"]
[null,null,"CPVX008","8.75","2.88","0","L,H,DO,","37894da0-c8af-467e-ad0c-c1b2f6e65219","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=2 22/25\", W=8 3/4\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","2.88","8.75",null,"ValveActuator",null,"4194"]
[null,null,"CPVX008","12.5","3.6","0","L,H,DO,","95f070a6-4fd5-4323-a634-1ba9ed7e13fb","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=3 3/5\", W=12 1/2\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","3.6","12.5",null,"ValveActuator",null,"4195"]
[null,null,"CPVX008","24","5.7","0","L,H,DO,","bae61cb2-cd55-422f-b094-cbcf4aec2474","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 7/10\", W=24\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.7","24",null,"ValveActuator",null,"4196"]
[null,null,"CPVX008","30","11.5","0","L,H,DO,","b985b3ec-3421-4a14-b498-3d5f49b52589","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","30",null,"ValveActuator",null,"4197"]
[null,null,"CPVX008","26.5354","8.7402","0","L,H,DO,","d81badf1-6af2-4061-a972-33a3924e8242","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 161/217\", W=26 127/238\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.7402","26.5354",null,"ValveActuator",null,"4198"]
[null,null,"CPVX008","30","15.25","0","L,H,DO,","4011aff6-fa15-409c-a0d0-5cc7734c9887","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.25","30",null,"ValveActuator",null,"4199"]
[null,null,"CPVX008","16.1417","7.0472","0","L,H,DO,","92178400-e304-4a42-a01e-83ad89385bb8","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7 20/417\", W=16 35/250\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7.0472","16.1417",null,"ValveActuator",null,"4231"]
[null,null,"CPVX008","30","5.5","0","L,H,DO,","40405c3d-0651-468e-a192-4946a91c87e7","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.5","30",null,"ValveActuator",null,"4232"]
[null,null,"CPVX008","16.1417","6.4961","0","L,H,DO,","6ac4b970-aa35-435b-84b4-bf5e7d2ac2b5","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=6 331/667\", W=16 35/250\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","6.4961","16.1417",null,"ValveActuator",null,"4233"]
[null,null,"CPVX008","44","13.875","0","L,H,DO,","2990e987-6c60-4251-b2a0-4e27c78dc135","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 7/8\", W=44\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.875","44",null,"ValveActuator",null,"4234"]
[null,null,"CPVX008","44","13.875","0","L,H,DO,","2a1e71a8-cea2-469a-af13-672596bc151a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 7/8\", W=44\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.875","44",null,"ValveActuator",null,"4235"]
[null,null,"CPVX008","30","6","0","L,H,DO,","b3e5a1b5-7e06-4790-a12d-60836ca245a7","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=6\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","6","30",null,"ValveActuator",null,"4236"]
[null,null,"CPVX008","44","13.875","0","L,H,DO,","328f39de-736a-4dd4-b79c-2f84deb1ec9c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 7/8\", W=44\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.875","44",null,"ValveActuator",null,"4237"]
[null,null,"CPVX008","26.5354","8.7402","0","L,H,DO,","d81badf1-6af2-4061-a972-33a3924e8242","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 161/217\", W=26 127/238\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.7402","26.5354",null,"ValveActuator",null,"4238"]
[null,null,"CPVX008","18","4","0","L,H,DO,","ba14331c-3cfe-463c-abca-3a629699735a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=4\", W=18\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","4","18",null,"ValveActuator",null,"4266"]
[null,null,"CPVX008","30","16.25","0","L,H,DO,","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.25","30",null,"ValveActuator",null,"4267"]
[null,null,"CPVX008","30","13.5","0","L,H,DO,","5c04ba24-a4ed-4794-a425-069eb5c978ed","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","30",null,"ValveActuator",null,"4268"]
[null,null,"CPVX008","30","8.75","0","L,H,DO,","3b428250-2347-4a52-9bb5-8497ecb0f6dd","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","30",null,"ValveActuator",null,"4269"]
[null,null,"CPVX008","30","21.5","0","L,H,DO,","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21.5","30",null,"ValveActuator",null,"4270"]
[null,null,"CPVX008","24","5.7","0","L,H,DO,","bae61cb2-cd55-422f-b094-cbcf4aec2474","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 7/10\", W=24\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.7","24",null,"ValveActuator",null,"4271"]
[null,null,"CPVX008","30","11.5","0","L,H,DO,","b985b3ec-3421-4a14-b498-3d5f49b52589","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","30",null,"ValveActuator",null,"4272"]
[null,null,"CPVX008","26.5354","8.7402","0","L,H,DO,","d81badf1-6af2-4061-a972-33a3924e8242","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 161/217\", W=26 127/238\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.7402","26.5354",null,"ValveActuator",null,"4273"]
[null,null,"CPVX008","30","15.25","0","L,H,DO,","4011aff6-fa15-409c-a0d0-5cc7734c9887","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.25","30",null,"ValveActuator",null,"4274"]
[null,null,"CPVX008","16.1417","7.0472","0","L,H,DO,","92178400-e304-4a42-a01e-83ad89385bb8","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=7 20/417\", W=16 35/250\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","7.0472","16.1417",null,"ValveActuator",null,"4308"]
[null,null,"CPVX008","30","5","0","L,H,DO,","3512211a-086e-4c9d-8ec4-24b7a97db83a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5","30",null,"ValveActuator",null,"4309"]
[null,null,"CPVX008","30","5.5","0","L,H,DO,","40405c3d-0651-468e-a192-4946a91c87e7","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=5 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","5.5","30",null,"ValveActuator",null,"4310"]
[null,null,"CPVX008","16.1417","6.4961","0","L,H,DO,","6ac4b970-aa35-435b-84b4-bf5e7d2ac2b5","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=6 331/667\", W=16 35/250\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","6.4961","16.1417",null,"ValveActuator",null,"4311"]
[null,null,"CPVX008","44","13.875","0","L,H,DO,","2990e987-6c60-4251-b2a0-4e27c78dc135","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 7/8\", W=44\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.875","44",null,"ValveActuator",null,"4312"]
[null,null,"CPVX008","30","6","0","L,H,DO,","b3e5a1b5-7e06-4790-a12d-60836ca245a7","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=6\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","6","30",null,"ValveActuator",null,"4313"]
[null,null,"CPVX008","44","13.875","0","L,H,DO,","328f39de-736a-4dd4-b79c-2f84deb1ec9c","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 7/8\", W=44\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.875","44",null,"ValveActuator",null,"4314"]
[null,null,"CPVX008","26.5354","8.7402","0","L,H,DO,","d81badf1-6af2-4061-a972-33a3924e8242","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 161/217\", W=26 127/238\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.7402","26.5354",null,"ValveActuator",null,"4315"]
[null,null,"CPVX008","30","16.25","0","L,H,DO,","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=16 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","16.25","30",null,"ValveActuator",null,"4341"]
[null,null,"CPVX008","30","13.5","0","L,H,DO,","5c04ba24-a4ed-4794-a425-069eb5c978ed","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.5","30",null,"ValveActuator",null,"4342"]
[null,null,"CPVX008","30","8.75","0","L,H,DO,","3b428250-2347-4a52-9bb5-8497ecb0f6dd","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=8 3/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","8.75","30",null,"ValveActuator",null,"4343"]
[null,null,"CPVX008","30","21.5","0","L,H,DO,","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=21 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","21.5","30",null,"ValveActuator",null,"4344"]
[null,null,"CPVX008","44","13.875","0","L,H,DO,","2a1e71a8-cea2-469a-af13-672596bc151a","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=13 7/8\", W=44\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","13.875","44",null,"ValveActuator",null,"4345"]
[null,null,"CPVX008","30","11.5","0","L,H,DO,","b985b3ec-3421-4a14-b498-3d5f49b52589","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=11 1/2\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","11.5","30",null,"ValveActuator",null,"4346"]
[null,null,"CPVX008","30","15.25","0","L,H,DO,","4011aff6-fa15-409c-a0d0-5cc7734c9887","ALL","0","in",{"$nulls":10},"in","Hand Lever",null,null,"Hand Lever","HAND LEVER, H=15 1/4\", W=30\"",{"$nulls":6},"dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dfba20f9-ae50-4ccc-aaef-796bf7a5767e",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandLever","15.25","30",null,"ValveActuator",null,"4347"]

{"sheet":"HAND WHEEL","index":1,"n_rows":89,"n_cols":55,"rows_kept":89,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","L","D","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","L","D","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,null,"CPVX002","29.5","23.5","L,D,","cac83439-30eb-48c8-8a47-af608ed06509","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=29 1/2\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","29.5","23.5",null,"ValveActuator",null,"128"]
[null,null,"CPVX002","133.5","78.5","L,D,","1f967a14-50de-418a-9806-0f90316e6e17","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=133 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","133.5","78.5",null,"ValveActuator",null,"3731"]
[null,null,"CPVX002","49.75","23.5","L,D,","af90cd55-9525-410b-b2b6-c67760d26276","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=49 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","49.75","23.5",null,"ValveActuator",null,"3732"]
[null,null,"CPVX002","140","36","L,D,","23d3e45c-5718-406d-9b1d-96f1951e80a5","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=140\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","140","36",null,"ValveActuator",null,"3733"]
[null,null,"CPVX002","66.5","31.5","L,D,","95186260-05ab-4f34-9f3b-a9e4661430dd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=66 1/2\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","66.5","31.5",null,"ValveActuator",null,"3734"]
[null,null,"CPVX002","33.25","15.75","L,D,","7f821266-6705-432f-9d82-62fb1dc61b9b","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=33 1/4\", W=15 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","33.25","15.75",null,"ValveActuator",null,"3735"]
[null,null,"CPVX002","15","8","L,D,","09af6d70-66a4-4d3c-a8e1-15c344690baf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=15\", W=8\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","15","8",null,"ValveActuator",null,"3736"]
[null,null,"CPVX002","166","78.5","L,D,","50447195-3edf-4ced-9e1b-299b3b6464e1","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=166\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","166","78.5",null,"ValveActuator",null,"3737"]
[null,null,"CPVX002","56.75","23.5","L,D,","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=56 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","56.75","23.5",null,"ValveActuator",null,"3738"]
[null,null,"CPVX002","21.75","11.75","L,D,","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=21 3/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","21.75","11.75",null,"ValveActuator",null,"3739"]
[null,null,"CPVX002","131","78.5","L,D,","3aca9ba6-cada-4b93-998b-9ae0d21028fd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=131\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","131","78.5",null,"ValveActuator",null,"3740"]
[null,null,"CPVX002","115.5","78.5","L,D,","1df90dcc-8aed-4df7-9625-1161fe156ec4","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=115 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","115.5","78.5",null,"ValveActuator",null,"3741"]
[null,null,"CPVX002","73.25","31.5","L,D,","e7b757cd-087d-47b7-9775-a17b2e752794","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=73 1/4\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","73.25","31.5",null,"ValveActuator",null,"3742"]
[null,null,"CPVX002","107.5","78.5","L,D,","879658da-2bb0-4344-a874-3edf9988d3e0","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=107 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","107.5","78.5",null,"ValveActuator",null,"3743"]
[null,null,"CPVX002","148","78.5","L,D,","aab3b7da-7cee-42c1-b7cc-ede34fcd62c3","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=148\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","148","78.5",null,"ValveActuator",null,"3744"]
[null,null,"CPVX002","82","43.25","L,D,","ea29d9dc-eac3-422f-8b07-2a851d4650c6","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=82\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","82","43.25",null,"ValveActuator",null,"3745"]
[null,null,"CPVX002","42","19.5","L,D,","1f9150dd-0ada-454c-a5a8-f02b683b4441","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=42\", W=19 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","42","19.5",null,"ValveActuator",null,"3746"]
[null,null,"CPVX002","27","11.75","L,D,","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=27\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","27","11.75",null,"ValveActuator",null,"3747"]
[null,null,"CPVX002","92","43.25","L,D,","60165ae9-ac00-4b7f-bd73-40e4094b7ace","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=92\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","92","43.25",null,"ValveActuator",null,"3748"]
[null,null,"CPVX002","133.5","78.5","L,D,","1f967a14-50de-418a-9806-0f90316e6e17","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=133 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","133.5","78.5",null,"ValveActuator",null,"3816"]
[null,null,"CPVX002","49.75","23.5","L,D,","af90cd55-9525-410b-b2b6-c67760d26276","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=49 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","49.75","23.5",null,"ValveActuator",null,"3817"]
[null,null,"CPVX002","140","36","L,D,","23d3e45c-5718-406d-9b1d-96f1951e80a5","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=140\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","140","36",null,"ValveActuator",null,"3818"]
[null,null,"CPVX002","66.5","31.5","L,D,","95186260-05ab-4f34-9f3b-a9e4661430dd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=66 1/2\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","66.5","31.5",null,"ValveActuator",null,"3819"]
[null,null,"CPVX002","33.25","15.75","L,D,","7f821266-6705-432f-9d82-62fb1dc61b9b","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=33 1/4\", W=15 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","33.25","15.75",null,"ValveActuator",null,"3820"]
[null,null,"CPVX002","15","8","L,D,","09af6d70-66a4-4d3c-a8e1-15c344690baf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=15\", W=8\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","15","8",null,"ValveActuator",null,"3821"]
[null,null,"CPVX002","166","78.5","L,D,","50447195-3edf-4ced-9e1b-299b3b6464e1","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=166\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","166","78.5",null,"ValveActuator",null,"3822"]
[null,null,"CPVX002","56.75","23.5","L,D,","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=56 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","56.75","23.5",null,"ValveActuator",null,"3823"]
[null,null,"CPVX002","21.75","11.75","L,D,","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=21 3/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","21.75","11.75",null,"ValveActuator",null,"3824"]
[null,null,"CPVX002","131","78.5","L,D,","3aca9ba6-cada-4b93-998b-9ae0d21028fd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=131\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","131","78.5",null,"ValveActuator",null,"3825"]
[null,null,"CPVX002","115.5","78.5","L,D,","1df90dcc-8aed-4df7-9625-1161fe156ec4","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=115 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","115.5","78.5",null,"ValveActuator",null,"3826"]
[null,null,"CPVX002","73.25","31.5","L,D,","e7b757cd-087d-47b7-9775-a17b2e752794","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=73 1/4\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","73.25","31.5",null,"ValveActuator",null,"3827"]
[null,null,"CPVX002","107.5","78.5","L,D,","879658da-2bb0-4344-a874-3edf9988d3e0","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=107 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","107.5","78.5",null,"ValveActuator",null,"3828"]
[null,null,"CPVX002","148","78.5","L,D,","aab3b7da-7cee-42c1-b7cc-ede34fcd62c3","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=148\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","148","78.5",null,"ValveActuator",null,"3829"]
[null,null,"CPVX002","82","43.25","L,D,","ea29d9dc-eac3-422f-8b07-2a851d4650c6","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=82\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","82","43.25",null,"ValveActuator",null,"3830"]
[null,null,"CPVX002","42","19.5","L,D,","1f9150dd-0ada-454c-a5a8-f02b683b4441","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=42\", W=19 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","42","19.5",null,"ValveActuator",null,"3831"]
[null,null,"CPVX002","27","11.75","L,D,","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=27\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","27","11.75",null,"ValveActuator",null,"3832"]
[null,null,"CPVX002","92","43.25","L,D,","60165ae9-ac00-4b7f-bd73-40e4094b7ace","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=92\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","92","43.25",null,"ValveActuator",null,"3833"]
[null,null,"CPVX002","133.5","78.5","L,D,","1f967a14-50de-418a-9806-0f90316e6e17","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=133 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","133.5","78.5",null,"ValveActuator",null,"3896"]
[null,null,"CPVX002","49.75","23.5","L,D,","af90cd55-9525-410b-b2b6-c67760d26276","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=49 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","49.75","23.5",null,"ValveActuator",null,"3897"]
[null,null,"CPVX002","140","36","L,D,","23d3e45c-5718-406d-9b1d-96f1951e80a5","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=140\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","140","36",null,"ValveActuator",null,"3898"]
[null,null,"CPVX002","66.5","31.5","L,D,","95186260-05ab-4f34-9f3b-a9e4661430dd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=66 1/2\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","66.5","31.5",null,"ValveActuator",null,"3899"]
[null,null,"CPVX002","33.25","15.75","L,D,","7f821266-6705-432f-9d82-62fb1dc61b9b","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=33 1/4\", W=15 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","33.25","15.75",null,"ValveActuator",null,"3901"]
[null,null,"CPVX002","15","8","L,D,","09af6d70-66a4-4d3c-a8e1-15c344690baf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=15\", W=8\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","15","8",null,"ValveActuator",null,"3902"]
[null,null,"CPVX002","166","78.5","L,D,","50447195-3edf-4ced-9e1b-299b3b6464e1","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=166\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","166","78.5",null,"ValveActuator",null,"3903"]
[null,null,"CPVX002","56.75","23.5","L,D,","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=56 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","56.75","23.5",null,"ValveActuator",null,"3904"]
[null,null,"CPVX002","21.75","11.75","L,D,","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=21 3/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","21.75","11.75",null,"ValveActuator",null,"3905"]
[null,null,"CPVX002","131","78.5","L,D,","3aca9ba6-cada-4b93-998b-9ae0d21028fd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=131\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","131","78.5",null,"ValveActuator",null,"3906"]
[null,null,"CPVX002","115.5","78.5","L,D,","1df90dcc-8aed-4df7-9625-1161fe156ec4","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=115 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","115.5","78.5",null,"ValveActuator",null,"3907"]
[null,null,"CPVX002","73.25","31.5","L,D,","e7b757cd-087d-47b7-9775-a17b2e752794","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=73 1/4\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","73.25","31.5",null,"ValveActuator",null,"3908"]
[null,null,"CPVX002","107.5","78.5","L,D,","879658da-2bb0-4344-a874-3edf9988d3e0","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=107 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","107.5","78.5",null,"ValveActuator",null,"3909"]
[null,null,"CPVX002","148","78.5","L,D,","aab3b7da-7cee-42c1-b7cc-ede34fcd62c3","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=148\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","148","78.5",null,"ValveActuator",null,"3910"]
[null,null,"CPVX002","82","43.25","L,D,","ea29d9dc-eac3-422f-8b07-2a851d4650c6","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=82\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","82","43.25",null,"ValveActuator",null,"3911"]
[null,null,"CPVX002","42","19.5","L,D,","1f9150dd-0ada-454c-a5a8-f02b683b4441","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=42\", W=19 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","42","19.5",null,"ValveActuator",null,"3912"]
[null,null,"CPVX002","27","11.75","L,D,","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=27\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","27","11.75",null,"ValveActuator",null,"3913"]
[null,null,"CPVX002","92","43.25","L,D,","60165ae9-ac00-4b7f-bd73-40e4094b7ace","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=92\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","92","43.25",null,"ValveActuator",null,"3914"]
[null,null,"CPVX002","133.5","78.5","L,D,","1f967a14-50de-418a-9806-0f90316e6e17","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=133 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","133.5","78.5",null,"ValveActuator",null,"3977"]
[null,null,"CPVX002","49.75","23.5","L,D,","af90cd55-9525-410b-b2b6-c67760d26276","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=49 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","49.75","23.5",null,"ValveActuator",null,"3978"]
[null,null,"CPVX002","140","36","L,D,","23d3e45c-5718-406d-9b1d-96f1951e80a5","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=140\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","140","36",null,"ValveActuator",null,"3979"]
[null,null,"CPVX002","66.5","31.5","L,D,","95186260-05ab-4f34-9f3b-a9e4661430dd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=66 1/2\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","66.5","31.5",null,"ValveActuator",null,"3980"]
[null,null,"CPVX002","33.25","15.75","L,D,","7f821266-6705-432f-9d82-62fb1dc61b9b","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=33 1/4\", W=15 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","33.25","15.75",null,"ValveActuator",null,"3981"]
[null,null,"CPVX002","15","8","L,D,","09af6d70-66a4-4d3c-a8e1-15c344690baf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=15\", W=8\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","15","8",null,"ValveActuator",null,"3982"]
[null,null,"CPVX002","166","78.5","L,D,","50447195-3edf-4ced-9e1b-299b3b6464e1","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=166\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","166","78.5",null,"ValveActuator",null,"3983"]
[null,null,"CPVX002","56.75","23.5","L,D,","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=56 3/4\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","56.75","23.5",null,"ValveActuator",null,"3984"]
[null,null,"CPVX002","21.75","11.75","L,D,","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=21 3/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","21.75","11.75",null,"ValveActuator",null,"3985"]
[null,null,"CPVX002","131","78.5","L,D,","3aca9ba6-cada-4b93-998b-9ae0d21028fd","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=131\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","131","78.5",null,"ValveActuator",null,"3986"]
[null,null,"CPVX002","115.5","78.5","L,D,","1df90dcc-8aed-4df7-9625-1161fe156ec4","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=115 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","115.5","78.5",null,"ValveActuator",null,"3987"]
[null,null,"CPVX002","73.25","31.5","L,D,","e7b757cd-087d-47b7-9775-a17b2e752794","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=73 1/4\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","73.25","31.5",null,"ValveActuator",null,"3988"]
[null,null,"CPVX002","107.5","78.5","L,D,","879658da-2bb0-4344-a874-3edf9988d3e0","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=107 1/2\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","107.5","78.5",null,"ValveActuator",null,"3989"]
[null,null,"CPVX002","148","78.5","L,D,","aab3b7da-7cee-42c1-b7cc-ede34fcd62c3","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=148\", W=78 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","148","78.5",null,"ValveActuator",null,"3990"]
[null,null,"CPVX002","82","43.25","L,D,","ea29d9dc-eac3-422f-8b07-2a851d4650c6","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=82\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","82","43.25",null,"ValveActuator",null,"3991"]
[null,null,"CPVX002","42","19.5","L,D,","1f9150dd-0ada-454c-a5a8-f02b683b4441","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=42\", W=19 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","42","19.5",null,"ValveActuator",null,"3992"]
[null,null,"CPVX002","27","11.75","L,D,","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=27\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","27","11.75",null,"ValveActuator",null,"3993"]
[null,null,"CPVX002","92","43.25","L,D,","60165ae9-ac00-4b7f-bd73-40e4094b7ace","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=92\", W=43 1/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","92","43.25",null,"ValveActuator",null,"3994"]
[null,null,"CPVX002","15","8","L,D,","09af6d70-66a4-4d3c-a8e1-15c344690baf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=15\", W=8\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","15","8",null,"ValveActuator",null,"4033"]
[null,null,"CPVX002","15","8","L,D,","09af6d70-66a4-4d3c-a8e1-15c344690baf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=15\", W=8\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","15","8",null,"ValveActuator",null,"4047"]
[null,null,"CPVX002","32.75","31.5","L,D,","6d8f1304-9c6c-491d-86fc-0c515d932df8","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=32 3/4\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","32.75","31.5",null,"ValveActuator",null,"4071"]
[null,null,"CPVX002","57.25","36","L,D,","ecbd0507-87e8-4762-b5ee-b115b5f692a6","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=57 1/4\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","57.25","36",null,"ValveActuator",null,"4072"]
[null,null,"CPVX002","60","36","L,D,","c31fde0b-b209-4f78-9bd4-77b9181a2ae4","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=60\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","60","36",null,"ValveActuator",null,"4073"]
[null,null,"CPVX002","22","11.75","L,D,","f4e58e13-57f6-4cd4-ad9e-42d26e3a79e8","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=22\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","22","11.75",null,"ValveActuator",null,"4074"]
[null,null,"CPVX002","18.75","11.75","L,D,","9481a326-f55f-42ec-8cce-0a653c6c56ff","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=18 3/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","18.75","11.75",null,"ValveActuator",null,"4075"]
[null,null,"CPVX002","40.75","31.5","L,D,","7e71cf34-0825-48c0-ad6b-9426e6387717","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=40 3/4\", W=31 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","40.75","31.5",null,"ValveActuator",null,"4076"]
[null,null,"CPVX002","16.25","11.75","L,D,","7779af35-d169-432a-a897-31b7b304b299","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=16 1/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","16.25","11.75",null,"ValveActuator",null,"4077"]
[null,null,"CPVX002","29.5","23.5","L,D,","cac83439-30eb-48c8-8a47-af608ed06509","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=29 1/2\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","29.5","23.5",null,"ValveActuator",null,"4078"]
[null,null,"CPVX002","24.5","23.5","L,D,","ab498d70-6c32-485f-a670-95a97fc2a2b9","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=24 1/2\", W=23 1/2\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","24.5","23.5",null,"ValveActuator",null,"4079"]
[null,null,"CPVX002","57.25","36","L,D,","492a43ce-edca-4cef-8c6a-4838390906cf","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=57 1/4\", W=36\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","57.25","36",null,"ValveActuator",null,"4080"]
[null,null,"CPVX002","16.25","11.75","L,D,","7779af35-d169-432a-a897-31b7b304b299","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=16 1/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","16.25","11.75",null,"ValveActuator",null,"4121"]
[null,null,"CPVX002","16.25","11.75","L,D,","7779af35-d169-432a-a897-31b7b304b299","ALL","0","in",{"$nulls":10},"in","Hand Wheel",null,null,"Hand Wheel","HAND WHEEL, H=16 1/4\", W=11 3/4\"",{"$nulls":6},"1bc8e695-b9f3-47bd-beff-382ef635b7f6","1bc8e695-b9f3-47bd-beff-382ef635b7f6",{"$nulls":4},"1",null,"Actuators",null,null,"ASME Valves Catalog","4_0",null,null,"Manual","HandWheel","16.25","11.75",null,"ValveActuator",null,"4135"]

{"sheet":"PLUG VALVE_5","index":2,"n_rows":11,"n_cols":81,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"2\"","CPVI010000","0.01","0.01","10.5","0","2.375","2.375","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","4e183549-9d50-e375-c5af-e3afa4049c72","ALL","2","in","2.375","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 2\" ND, 150 LB, BW, ASME B16.10, 10 1/2\" LG",null,null,"44.09","LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10.5","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","cb868361-9d2b-5d1d-a03d-40f0840ce8e3","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","6ac4b970-aa35-435b-84b4-bf5e7d2ac2b5","Manual","HandLever","6.4961","16.1417","False",{"$nulls":6},"Valve",null,"4221"]
[null,"2 1/2\"","CPVI010000","0.01","0.01","12","0","2.875","2.875","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","4023859c-8c65-5e87-a17e-16b4a56de0d2","ALL","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 2 1/2\" ND, 150 LB, BW, ASME B16.10, 12\" LG",null,null,"66.14","LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"12","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","1fb6f4a1-a091-5d8d-a6a1-2daff39e06ec","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","92178400-e304-4a42-a01e-83ad89385bb8","Manual","HandLever","7.0472","16.1417","False",{"$nulls":6},"Valve",null,"4239"]
[null,"3\"","CPVI010000","0.01","0.01","13","0","3.5","3.5","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5f943b2c-ac64-f330-0382-b4c3414122e4","ALL","3","in","3.5","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 3\" ND, 150 LB, BW, ASME B16.10, 13\" LG",null,null,"88.19","LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","770ce484-9352-5eb2-95ad-104407b121da","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","92178400-e304-4a42-a01e-83ad89385bb8","Manual","HandLever","7.0472","16.1417","False",{"$nulls":6},"Valve",null,"4241"]
[null,"4\"","CPVI010000","0.01","0.01","14","0","4.5","4.5","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","70768478-c7a2-3b44-0952-4bedea0fbea7","ALL","4","in","4.5","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 4\" ND, 150 LB, BW, ASME B16.10, 14\" LG",null,null,"132.28","LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","afa6e61d-9f96-576f-83d1-e9efe96d4be3","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","40405c3d-0651-468e-a192-4946a91c87e7","Manual","HandLever","5.5","30","False",{"$nulls":6},"Valve",null,"4243"]
[null,"5\"","CPVI010000","0.01","0.01","15","0","5.563","5.563","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","95eb5dfe-9dfd-01ae-9d02-047782036605","ALL","5","in","5.563","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 5\" ND, 150 LB, BW, ASME B16.10, 15\" LG",null,null,null,"LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","32730d94-636f-5871-bbd8-b4422a05d637","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b3e5a1b5-7e06-4790-a12d-60836ca245a7","Manual","HandLever","6","30","False",{"$nulls":6},"Valve",null,"4245"]
[null,"6\"","CPVI010000","0.01","0.01","18","0","6.625","6.625","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","ba340c03-2cf9-8096-466a-97cd5bc9ca5e","ALL","6","in","6.625","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 6\" ND, 150 LB, BW, ASME B16.10, 18\" LG",null,null,"242.51","LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","38f31171-e3c7-5665-b87a-2afdc7eb960a","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81badf1-6af2-4061-a972-33a3924e8242","Manual","HandLever","8.7402","26.5354","False",{"$nulls":6},"Valve",null,"4247"]
[null,"8\"","CPVI010000","0.01","0.01","20.5","0","8.625","8.625","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","86f13b90-4663-38a8-dfd1-638f6bd09f23","ALL","8","in","8.625","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 8\" ND, 150 LB, BW, ASME B16.10, 20 1/2\" LG",null,null,null,"LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"20.5","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","2a4ee6ac-756b-5624-97fb-96c92bb19716","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","2990e987-6c60-4251-b2a0-4e27c78dc135","Manual","HandLever","13.875","44","False",{"$nulls":6},"Valve",null,"4249"]
[null,"10\"","CPVI010000","0.01","0.01","22","0","10.75","10.75","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","473b775a-b927-6023-804d-87283c56f607","ALL","10","in","10.75","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 10\" ND, 150 LB, BW, ASME B16.10, 22\" LG",null,null,null,"LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","70e4b401-b316-5dbe-977e-9d5ae08dfd62","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","328f39de-736a-4dd4-b79c-2f84deb1ec9c","Manual","HandLever","13.875","44","False",{"$nulls":6},"Valve",null,"4251"]
[null,"12\"","CPVI010000","0.01","0.01","25","0","12.75","12.75","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","a14e0a14-bdee-c7fd-b57a-0cf388da6182","ALL","12","in","12.75","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 12\" ND, 150 LB, BW, ASME B16.10, 25\" LG",null,null,null,"LB","VPBW","VALVE","f827cde5-8c2d-4e14-940d-909547b6fb4b","f9fa65b2-ad8a-46de-ab51-653a2645e223",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"25","Inline","Continuous","Plug","False","False","f9fa65b2-ad8a-46de-ab51-653a2645e223","b3dd4d46-6183-5383-8705-c9443e2c6094","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","2a1e71a8-cea2-469a-af13-672596bc151a","Manual","HandLever","13.875","44","False",{"$nulls":6},"Valve",null,"4253"]

{"sheet":"GLOBE VALVE_2","index":3,"n_rows":8,"n_cols":86,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI004000_OFOF","0.84","0.84","4.25","0","-2","-2","1.4",null,null,"0","0.418","0.418","0.38","0.38","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","94cea3cf-d567-30f3-8fbe-cedd35e776d3","ALL","0.5","in","0.84","THDF",{"$nulls":4},"150",null,null,"0.38","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1/2\" ND, 150 LB, FPT, ASME B16.10, 4 1/4\" LG",{"$nulls":4},"VGSC","VALVE","e857e6c8-2140-4cc8-bdb7-3d3747fb237b","ad8f8d37-457d-48c5-baf6-6d5617d7ba56",{"$nulls":4},"2",null,"Valves","SKEY=VGSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Globe","False","False","ad8f8d37-457d-48c5-baf6-6d5617d7ba56","4a319953-ab98-5090-be39-f80d4964bfc5","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4118"]
[null,"3/4\"","CPVI004000_OFOF","1.05","1.05","4.625","0","-2","-2","1.552",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","a31ef362-b5fc-0457-8bdd-859f1f65abce","ALL","0.75","in","1.05","THDF",{"$nulls":4},"150",null,null,"0.5","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 3/4\" ND, 150 LB, FPT, ASME B16.10, 4 5/8\" LG",{"$nulls":4},"VGSC","VALVE","e857e6c8-2140-4cc8-bdb7-3d3747fb237b","ad8f8d37-457d-48c5-baf6-6d5617d7ba56",{"$nulls":4},"2",null,"Valves","SKEY=VGSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.625","Inline","Continuous","Globe","False","False","ad8f8d37-457d-48c5-baf6-6d5617d7ba56","a4ad0249-1f1f-519a-8c6b-7e8021441064","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4122"]
[null,"1\"","CPVI004000_OFOF","1.315","1.315","5","0","-2","-2","1.7",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","b39f7140-dc56-6cb8-8bb9-f02759b297f8","ALL","1","in","1.315","THDF",{"$nulls":4},"150",null,null,"0.5","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1\" ND, 150 LB, FPT, ASME B16.10, 5\" LG",{"$nulls":4},"VGSC","VALVE","e857e6c8-2140-4cc8-bdb7-3d3747fb237b","ad8f8d37-457d-48c5-baf6-6d5617d7ba56",{"$nulls":4},"2",null,"Valves","SKEY=VGSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Globe","False","False","ad8f8d37-457d-48c5-baf6-6d5617d7ba56","25d6b826-fa13-5cce-bf65-66122fcd1c0b","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4124"]
[null,"1 1/4\"","CPVI004000_OFOF","1.66","1.66","5.5","0","-2","-2","1.848",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","a7af0ec2-8a7d-b543-d647-5086dc0c552f","ALL","1.25","in","1.66","THDF",{"$nulls":4},"150",null,null,"0.5","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1 1/4\" ND, 150 LB, FPT, ASME B16.10, 5 1/2\" LG",{"$nulls":4},"VGSC","VALVE","e857e6c8-2140-4cc8-bdb7-3d3747fb237b","ad8f8d37-457d-48c5-baf6-6d5617d7ba56",{"$nulls":4},"2",null,"Valves","SKEY=VGSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Globe","False","False","ad8f8d37-457d-48c5-baf6-6d5617d7ba56","1cb0f50a-b596-5a7b-aa00-07abd92a1877","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4126"]
[null,"1 1/2\"","CPVI004000_OFOF","1.91","1.91","6.5","0","-2","-2","2",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","a68f4b90-9b39-13f0-e5a6-890551691116","ALL","1.5","in","1.91","THDF",{"$nulls":4},"150",null,null,"0.5","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1 1/2\" ND, 150 LB, FPT, ASME B16.10, 6 1/2\" LG",{"$nulls":4},"VGSC","VALVE","e857e6c8-2140-4cc8-bdb7-3d3747fb237b","ad8f8d37-457d-48c5-baf6-6d5617d7ba56",{"$nulls":4},"2",null,"Valves","SKEY=VGSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Globe","False","False","ad8f8d37-457d-48c5-baf6-6d5617d7ba56","a132ab8a-1633-5046-bf2d-3ffbe8d5b0e1","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4128"]
[null,"2\"","CPVI004000_OFOF","2.375","2.375","8","0","-2","-2","2.4",null,null,"0","0.682","0.682","0.62","0.62","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","8b82967a-af85-989d-15f4-bf0a17b1ac16","ALL","2","in","2.375","THDF",{"$nulls":4},"150",null,null,"0.62","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 2\" ND, 150 LB, FPT, ASME B16.10, 8\" LG",{"$nulls":4},"VGSC","VALVE","e857e6c8-2140-4cc8-bdb7-3d3747fb237b","ad8f8d37-457d-48c5-baf6-6d5617d7ba56",{"$nulls":4},"2",null,"Valves","SKEY=VGSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Globe","False","False","ad8f8d37-457d-48c5-baf6-6d5617d7ba56","d8a01571-6145-51b9-a9d6-8cfd3873615f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4130"]

{"sheet":"CHECK VALVE_1","index":4,"n_rows":25,"n_cols":81,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI011000","0.84","0.84","4.25","0","3.5","3.5","0","0","-1","0.44","0.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","19f4f95e-d354-4bc1-9be1-ce3c8bd37bf6","ALL","0.5","in","0.84","FL",null,null,"RF","0.44","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1/2\" ND, 150 LB, RF, ASME B16.10, 4 1/4\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","8793481b-b3f5-5484-aa49-59d2fd3ceb33",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3664"]
[null,"3/4\"","CPVI011000","1.05","1.05","4.62","0","3.88","3.88","0","0","-1","0.5","0.5","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","de199cd4-f63b-4b3c-9124-d6b386c87ec1","ALL","0.75","in","1.05","FL",null,null,"RF","0.5","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 3/4\" ND, 150 LB, RF, ASME B16.10, 4 31/50\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.62","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","c28e7c3a-2214-5708-94e7-cf6b562f5d17",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3666"]
[null,"1\"","CPVI011000","1.32","1.32","5","0","4.25","4.25","0","0","-1","0.56","0.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b9f8fcd1-ae25-4c65-b007-8bab1a8806c8","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1\" ND, 150 LB, RF, ASME B16.10, 5\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","238b20b3-225c-55a2-b2f9-9b6d23678532",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3668"]
[null,"1 1/4\"","CPVI011000","1.66","1.66","5.5","0","4.62","4.62","0","0","-1","0.62","0.62","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","62a76d42-084a-43bd-ae57-ac74cb6f8e02","ALL","1.25","in","1.66","FL",null,null,"RF","0.62","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1 1/4\" ND, 150 LB, RF, ASME B16.10, 5 1/2\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","1edce6b2-1cb0-5a72-917d-1cfaadf474d6",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3670"]
[null,"1 1/2\"","CPVI011000","1.91","1.91","6.5","0","5","5","0","0","-1","0.68","0.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","22252603-670a-449b-a5fc-1f53ae3b53bf","ALL","1.5","in","1.91","FL",null,null,"RF","0.68","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 6 1/2\" LG",null,null,"24.25","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","6fcf7106-5aca-51f8-8e76-d9ee73ce5b19",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3672"]
[null,"2\"","CPVI011000","2.38","2.38","8","0","6","6","0","0","-1","0.75","0.75","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3c081faf-e65f-487a-9266-ac10351c7338","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 2\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,"33.07","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","e60b0990-7071-5e4d-9549-36422f4f6a7e",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3674"]
[null,"2 1/2\"","CPVI011000","2.88","2.88","8.5","0","7","7","0","0","-1","0.87","0.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","c2af1cd0-4e7c-449c-bee6-df6cf96c8709","ALL","2.5","in","2.875","FL",null,null,"RF","0.87","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 8 1/2\" LG",null,null,"57.32","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","aead79f0-ada9-5b7c-b9ad-99bed7b07a3c",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3676"]
[null,"3\"","CPVI011000","3.5","3.5","9.5","0","7.5","7.5","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","0119a20f-2cc7-4b38-a05d-c91342a89e75","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 3\" ND, 150 LB, RF, ASME B16.10, 9 1/2\" LG",null,null,"59.52","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","2f96154d-afde-5a20-ad2a-2325d48b4884",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3678"]
[null,"4\"","CPVI011000","4.5","4.5","11.5","0","9","9","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3ac5849d-a9db-4f08-b59b-d42e862153f5","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 4\" ND, 150 LB, RF, ASME B16.10, 11 1/2\" LG",null,null,"92.59","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","41eed52d-f137-5657-8988-3166484900aa",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3680"]
[null,"5\"","CPVI011000","5.56","5.56","13","0","10","10","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","988e4fe5-ce6f-4648-bb77-b77a80c05a62","ALL","5","in","5.563","FL",null,null,"RF","0.94","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 5\" ND, 150 LB, RF, ASME B16.10, 13\" LG",null,null,"152.12","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","661fa173-3f4f-56ca-b78d-a7262d990295",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3682"]
[null,"6\"","CPVI011000","6.63","6.63","14","0","11","11","0","0","-1","1","1","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3ab9282d-f3f8-446b-834f-3b4e75718e37","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 6\" ND, 150 LB, RF, ASME B16.10, 14\" LG",null,null,"165.35","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","fcac7e10-b8a5-5dcf-a2c7-b55e7a2945bd",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3684"]
[null,"8\"","CPVI011000","8.63","8.63","19.5","0","13.5","13.5","0","0","-1","1.12","1.12","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","83fe5cb2-7547-44e0-bfdb-1b9fcdb29090","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 8\" ND, 150 LB, RF, ASME B16.10, 19 1/2\" LG",null,null,"273.37","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"19.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","d3a6a4aa-44bb-572f-8994-7967146b1c34",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3686"]
[null,"10\"","CPVI011000","10.75","10.75","24.5","0","16","16","0","0","-1","1.18","1.18","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","cc185461-bd22-4b97-b9de-3ff143ac4eb6","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 10\" ND, 150 LB, RF, ASME B16.10, 24 1/2\" LG",null,null,"440.92","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","bc14dfce-6a78-569f-b760-6922e953a8f1",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3688"]
[null,"12\"","CPVI011000","12.75","12.75","27.5","0","19","19","0","0","-1","1.25","1.25","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3430a36c-71c3-45ad-b116-db8c895a804a","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 12\" ND, 150 LB, RF, ASME B16.10, 27 1/2\" LG",null,null,"683.43","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"27.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","c550f0e8-d343-569c-b389-297b21a444cf",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3690"]
[null,"14\"","CPVI011000","14","14","21","0","21","21","0","0","-1","1.37","1.37","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","71b4c25f-5a9b-430c-9dfa-8465e35423c6","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 14\" ND, 150 LB, RF, ASME B16.10, 21\" LG",null,null,"943.58","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"21","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","71ba70bf-c953-5d4d-989e-43ef42a93bd0",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3692"]
[null,"16\"","CPVI011000","16","16","36","0","23.5","23.5","0","0","-1","1.44","1.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","a3d28979-42e7-41be-98ef-e7d7b15f923b","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 16\" ND, 150 LB, RF, ASME B16.10, 36\" LG",null,null,"1223.56","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","4b151fb4-d102-5324-8ff8-134781349b0e",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3694"]
[null,"18\"","CPVI011000","18","18","38.5","0","25","25","0","0","-1","1.56","1.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d81fadaf-1bbe-40dd-a86d-edb64c75edf8","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 18\" ND, 150 LB, RF, ASME B16.10, 38 1/2\" LG",null,null,"1708.58","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"38.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","3bc26ce3-62bd-59e5-8726-3722222679ac",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3696"]
[null,"20\"","CPVI011000","20","20","38.5","0","27.5","27.5","0","0","-1","1.68","1.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","8c33e621-9e1c-4c22-9419-887167e1651c","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 20\" ND, 150 LB, RF, ASME B16.10, 38 1/2\" LG",null,null,"1840.86","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"38.5","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","65e16abd-c50b-5a41-8667-0ea90e6e2e63",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3698"]
[null,"24\"","CPVI011000","24","24","51","0","32","32","0","0","-1","1.87","1.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","82a5711c-43ef-4824-86fe-dde5c86dfcdc","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 24\" ND, 150 LB, RF, ASME B16.10, 51\" LG",null,null,"2866.01","LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"51","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","6b960538-7f8b-5156-9737-2d8b3f99d251",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3701"]
[null,"26\"","CPVI011000","26","26","51","0","34.25","34.25","0","0","-1","2.69","2.69","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","14b0fe4f-14f4-4378-9484-9b8078f5129e","ALL","26","in","26","FL","Series A",null,"RF","2.69","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 26\" ND, 150 LB, RF, ASME B16.10, 51\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"51","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","d7d9b228-c50c-537e-b5bd-232684c31e52",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3703"]
[null,"28\"","CPVI011000","28","28","57","0","36.5","36.5","0","0","-1","2.81","2.81","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","50ef75df-e012-4d2e-9b5f-e0e7cd413551","ALL","28","in","28","FL","Series A",null,"RF","2.81","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 28\" ND, 150 LB, RF, ASME B16.10, 57\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"57","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","1378d695-8055-5448-9f2e-5940dc068918",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3705"]
[null,"30\"","CPVI011000","30","30","60","0","38.75","38.75","0","0","-1","2.94","2.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","cfc9c496-b5d5-4403-8146-46f478191482","ALL","30","in","30","FL","Series A",null,"RF","2.94","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 30\" ND, 150 LB, RF, ASME B16.10, 60\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"60","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","d9af01c5-fa99-5a8d-9619-7cd2eb4618e3",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3707"]
[null,"36\"","CPVI011000","36","36","77","0","46","46","0","0","-1","3.56","3.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","cec64889-879e-40e9-8bc8-f846d8ec6065","ALL","36","in","36","FL","Series A",null,"RF","3.56","150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 36\" ND, 150 LB, RF, ASME B16.10, 77\" LG",null,null,null,"LB","VCFL","VALVE","2a202298-08db-4487-8a57-43106c15fd02","9741e95c-2918-4cff-bc4d-ff09d2852bd3",{"$nulls":4},"2",null,"Valves","SKEY=VCFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"77","Inline","Continuous","Check","True","False","9741e95c-2918-4cff-bc4d-ff09d2852bd3","aeb5bd40-5726-599e-ae9e-5cd4288137c2",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3709"]

{"sheet":"GLOBE VALVE_1","index":5,"n_rows":17,"n_cols":82,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI004000","0.84","0.84","4.25","0","3.5","3.5","0","0","0","-1","0.38","0.38","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","9d3aedd9-1ef8-9211-7d81-3847e466bb2f","ALL","0.5","in","0.84","FL",null,null,"RF","0.38","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1/2\" ND, 150 LB, RF, ASME B16.10, 4 1/4\" LG",null,null,"11.02","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","88037d17-6442-59f4-a1e6-8fc70dd62fa5","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4058"]
[null,"3/4\"","CPVI004000","1.05","1.05","4.62","0","3.88","3.88","0","0","0","-1","0.44","0.44","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","3b89265c-ea72-d274-2d28-8c62e98f9f3b","ALL","0.75","in","1.05","FL",null,null,"RF","0.44","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 3/4\" ND, 150 LB, RF, ASME B16.10, 4 31/50\" LG",null,null,"15.43","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.62","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","bf1c4276-f080-55ef-afc8-5ee0a4b90eaf","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4081"]
[null,"1\"","CPVI004000","1.315","1.315","5","0","4.25","4.25","0","0","0","-1","0.5","0.5","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","8aeffcf6-c7a3-14b9-b1c3-b173cee64712","ALL","1","in","1.315","FL",null,null,"RF","0.5","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1\" ND, 150 LB, RF, ASME B16.10, 5\" LG",null,null,"22.04","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","031ef717-a2d1-52ba-925a-68e707e66b2a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4083"]
[null,"1 1/4\"","CPVI004000","1.66","1.66","5.5","0","4.62","4.62","0","0","0","-1","0.56","0.56","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","4a041862-6c2c-4bcf-fab1-156eb197679c","ALL","1.25","in","1.66","FL",null,null,"RF","0.56","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1 1/4\" ND, 150 LB, RF, ASME B16.10, 5 1/2\" LG",null,null,"33.06","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","cb219b68-4cea-552c-9b49-13ec015b1f7d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4085"]
[null,"1 1/2\"","CPVI004000","1.9","1.9","6.5","0","5","5","0","0","0","-1","0.62","0.62","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","05121590-e215-15fd-f801-7425b0432eb8","ALL","1.5","in","1.9","FL",null,null,"RF","0.62","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 6 1/2\" LG",null,null,"39.68","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","9d5166b9-30c7-5f94-8f81-ecab3d44c0a5","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4087"]
[null,"2\"","CPVI004000","2.375","2.375","8","0","6","6","0","0","0","-1","0.69","0.69","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","1c4a41f4-ad98-c631-d2de-1aac3094d085","ALL","2","in","2.375","FL",null,null,"RF","0.69","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 2\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,"48.5","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","8df4d253-1fcb-5961-8b49-eda0a0baaef0","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4089"]
[null,"2 1/2\"","CPVI004000","2.875","2.875","8.5","0","7","7","0","0","0","-1","0.81","0.81","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","afc6424a-73f2-ca3b-ef1b-d166cf1714fe","ALL","2.5","in","2.875","FL",null,null,"RF","0.81","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 8 1/2\" LG",null,null,"66.13","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","43d54ada-6ebe-5c16-b72c-9400ea77e4e3","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4091"]
[null,"3\"","CPVI004000","3.5","3.5","9.5","0","7.5","7.5","0","0","0","-1","0.88","0.88","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","1705f4ef-2b98-7203-d094-db16b60b71fe","ALL","3","in","3.5","FL",null,null,"RF","0.88","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 3\" ND, 150 LB, RF, ASME B16.10, 9 1/2\" LG",null,null,"92.59","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","12a76dbb-b646-5ff7-963c-4bd80087a88c","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","9481a326-f55f-42ec-8cce-0a653c6c56ff","Manual","HandWheel","18.75","11.75","False",{"$nulls":6},"Valve",null,"4093"]
[null,"4\"","CPVI004000","4.5","4.5","11.5","0","9","9","0","0","0","-1","0.88","0.88","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","e7f96959-4d34-7b58-ae39-bcb79bca74ba","ALL","4","in","4.5","FL",null,null,"RF","0.88","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 4\" ND, 150 LB, RF, ASME B16.10, 11 1/2\" LG",null,null,"132.27","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","4ae07793-106e-5425-aa62-cd4257d492ea","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","f4e58e13-57f6-4cd4-ad9e-42d26e3a79e8","Manual","HandWheel","22","11.75","False",{"$nulls":6},"Valve",null,"4095"]
[null,"6\"","CPVI004000","6.625","6.625","16","0","11","11","0","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","d826786e-1aa8-ecc4-f9f0-01319949c0cc","ALL","6","in","6.625","FL",null,null,"RF","0.94","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 6\" ND, 150 LB, RF, ASME B16.10, 16\" LG",null,null,"222.66","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"16","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","ca6047cd-883a-528b-b80d-4dd13b652ed0","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","ab498d70-6c32-485f-a670-95a97fc2a2b9","Manual","HandWheel","24.5","23.5","False",{"$nulls":6},"Valve",null,"4099"]
[null,"8\"","CPVI004000","8.625","8.625","19.5","0","13.5","13.5","0","0","0","-1","1.06","1.06","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","0909a57b-186f-1366-ec97-007f562375af","ALL","8","in","8.625","FL",null,null,"RF","1.06","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 8\" ND, 150 LB, RF, ASME B16.10, 19 1/2\" LG",null,null,"354.94","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"19.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","0f63e206-cec1-5f35-83c6-0c19caa9c178","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","cac83439-30eb-48c8-8a47-af608ed06509","Manual","HandWheel","29.5","23.5","False",{"$nulls":6},"Valve",null,"4102"]
[null,"10\"","CPVI004000","10.75","10.75","24.5","0","16","16","0","0","0","-1","1.12","1.12","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","2c311483-ab96-255a-c349-d01c57c15692","ALL","10","in","10.75","FL",null,null,"RF","1.12","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 10\" ND, 150 LB, RF, ASME B16.10, 24 1/2\" LG",null,null,"679.02","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","d09ab95c-ef37-5918-b3b2-b66427be37ff","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","6d8f1304-9c6c-491d-86fc-0c515d932df8","Manual","HandWheel","32.75","31.5","False",{"$nulls":6},"Valve",null,"4104"]
[null,"12\"","CPVI004000","12.75","12.75","27.5","0","19","19","0","0","0","-1","1.19","1.19","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","e4853c24-1a66-21d1-9360-64b258fb4ba5","ALL","12","in","12.75","FL",null,null,"RF","1.19","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 12\" ND, 150 LB, RF, ASME B16.10, 27 1/2\" LG",null,null,"903.89","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"27.5","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","6be9579b-ff5f-510b-b839-fd32a797d185","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7e71cf34-0825-48c0-ad6b-9426e6387717","Manual","HandWheel","40.75","31.5","False",{"$nulls":6},"Valve",null,"4106"]
[null,"14\"","CPVI004000","14","14","31","0","21","21","0","0","0","-1","1.31","1.31","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","2b6190bb-da40-2f1b-6480-446a01663823","ALL","14","in","14","FL",null,null,"RF","1.31","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 14\" ND, 150 LB, RF, ASME B16.10, 31\" LG",null,null,"1344.81","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"31","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","91bd2438-c45e-5742-bc70-d80de8f2952b","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","ecbd0507-87e8-4762-b5ee-b115b5f692a6","Manual","HandWheel","57.25","36","False",{"$nulls":6},"Valve",null,"4108"]
[null,"16\"","CPVI004000","16","16","36","0","23.5","23.5","0","0","0","-1","1.38","1.38","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","f579a000-7f6c-bc39-50be-79c3b68fde85","ALL","16","in","16","FL",null,null,"RF","1.38","150",null,null,null,"in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 16\" ND, 150 LB, RF, ASME B16.10, 36\" LG",null,null,"1940.06","LB","VGFL","VALVE","43bd3689-eaa9-4e26-9141-a78de8c84936","3f635f12-4d41-450b-bcad-21be1e7eb691",{"$nulls":4},"2",null,"Valves","SKEY=VGFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Globe","False","False","3f635f12-4d41-450b-bcad-21be1e7eb691","442fe9b8-f8b3-5575-85ce-70c36a70f3ac","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","492a43ce-edca-4cef-8c6a-4838390906cf","Manual","HandWheel","57.25","36","False",{"$nulls":6},"Valve",null,"4110"]

{"sheet":"GATE VALVE_5","index":6,"n_rows":24,"n_cols":81,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI001000","0.84","0.84","4.25","0","3.5","3.5","0","0","0","0.44","0.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e1d7f60c-c856-9a06-d2b1-cc06b7bcec3f","ALL","0.5","in","0.84","FL",null,null,"RF","0.44","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1/2\" ND, 150 LB, RF, ASME B16.10, 4 1/4\" LG",null,null,"11.02","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","8e666205-48f7-5323-ac93-fcc6542b2f78","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3795"]
[null,"3/4\"","CPVI001000","1.05","1.05","4.625","0","3.88","3.88","0","0","0","0.5","0.5","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","96214201-f23c-cf3d-0dc6-75f5f62630cc","ALL","0.75","in","1.05","FL",null,null,"RF","0.5","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 3/4\" ND, 150 LB, RF, ASME B16.10, 4 5/8\" LG",null,null,"15.43","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.625","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","55f8a19b-2440-55df-a40b-fff3ce09c4e6","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3834"]
[null,"1\"","CPVI001000","1.315","1.315","5","0","4.25","4.25","0","0","0","0.56","0.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","106b3f60-145a-5569-88b2-b0bf802ec51b","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1\" ND, 150 LB, RF, ASME B16.10, 5\" LG",null,null,"22.04","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","1f21acaa-4310-50f6-9b41-96c00ec49198","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3836"]
[null,"1 1/4\"","CPVI001000","1.66","1.66","5.5","0","4.62","4.62","0","0","0","0.62","0.62","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e8995d22-00a2-2463-ce2f-f91afb0302a7","ALL","1.25","in","1.66","FL",null,null,"RF","0.62","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1 1/4\" ND, 150 LB, RF, ASME B16.10, 5 1/2\" LG",null,null,"33.06","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","cf2fda7a-e311-5056-8237-7714c5cd6fc4","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3838"]
[null,"1 1/2\"","CPVI001000","1.91","1.91","6.5","0","5","5","0","0","0","0.68","0.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d4f18e68-f753-1364-2740-702d67f0a487","ALL","1.5","in","1.91","FL",null,null,"RF","0.68","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 6 1/2\" LG",null,null,"39.68","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","90b5e0b7-f54b-5f27-9479-aaf7fc472d68","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3840"]
[null,"2\"","CPVI001000","2.375","2.375","7","0","6","6","0","0","0","0.75","0.75","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","c701bcfb-21d5-d97a-305f-68b09453d6fa","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 2\" ND, 150 LB, RF, ASME B16.10, 7\" LG",null,null,"39.68","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","1d91d731-b0bc-5840-8849-23a798806091","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3842"]
[null,"2 1/2\"","CPVI001000","2.875","2.875","7.5","0","7","7","0","0","0","0.87","0.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","2e89c4cd-0681-3e57-cd0d-2cc5c5502fe3","ALL","2.5","in","2.875","FL",null,null,"RF","0.87","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 7 1/2\" LG",null,null,"61.72","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7.5","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","684655b0-4e5e-5c52-bcb7-1ee8a5f4a80f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3844"]
[null,"3\"","CPVI001000","3.5","3.5","8","0","7.5","7.5","0","0","0","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","99fd86e7-2c35-2a22-3478-bec003ea2cda","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 3\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,"74.95","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","736ef22f-60e9-511b-9895-a60e1713b989","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","Manual","HandWheel","21.75","11.75","False",{"$nulls":6},"Valve",null,"3846"]
[null,"4\"","CPVI001000","4.5","4.5","9","0","9","9","0","0","0","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e3ca17ba-e230-da7e-0622-26f9e3a077c0","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 4\" ND, 150 LB, RF, ASME B16.10, 9\" LG",null,null,"114.64","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","d52c7f2f-cebb-57ae-bfe7-42103363efef","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","Manual","HandWheel","27","11.75","False",{"$nulls":6},"Valve",null,"3848"]
[null,"6\"","CPVI001000","6.625","6.625","10.5","0","11","11","0","0","0","1","1","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","63dcff6a-62f9-ded9-c02b-5318baf0bf2b","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 6\" ND, 150 LB, RF, ASME B16.10, 10 1/2\" LG",null,null,"194","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10.5","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","3d2eae84-2e83-53d7-998f-e42f31682472","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7f821266-6705-432f-9d82-62fb1dc61b9b","Manual","HandWheel","33.25","15.75","False",{"$nulls":6},"Valve",null,"3850"]
[null,"8\"","CPVI001000","8.625","8.625","11.5","0","13.5","13.5","0","0","0","1.12","1.12","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b84ffb32-dd51-33f0-b03d-a5039660e622","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 8\" ND, 150 LB, RF, ASME B16.10, 11 1/2\" LG",null,null,"317.46","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.5","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","ba9aa24d-c923-5fa1-8507-bd7f42e6fbc8","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f9150dd-0ada-454c-a5a8-f02b683b4441","Manual","HandWheel","42","19.5","False",{"$nulls":6},"Valve",null,"3852"]
[null,"10\"","CPVI001000","10.75","10.75","13","0","16","16","0","0","0","1.18","1.18","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","0af9eda2-03c1-0df9-0728-6b40db11f662","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 10\" ND, 150 LB, RF, ASME B16.10, 13\" LG",null,null,"434.31","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","8c02e246-2056-5132-b255-97b9ab9f470a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","af90cd55-9525-410b-b2b6-c67760d26276","Manual","HandWheel","49.75","23.5","False",{"$nulls":6},"Valve",null,"3854"]
[null,"12\"","CPVI001000","12.75","12.75","14","0","19","19","0","0","0","1.25","1.25","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","9b51b12f-6f60-011e-620d-b3d351739e1a","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 12\" ND, 150 LB, RF, ASME B16.10, 14\" LG",null,null,"656.97","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","b1fde21e-baa3-53f8-8ac6-21b24c3a706d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","Manual","HandWheel","56.75","23.5","False",{"$nulls":6},"Valve",null,"3856"]
[null,"14\"","CPVI001000","14","14","15","0","21","21","0","0","0","1.37","1.37","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3aa3afbe-21fb-be61-669b-70a6bae8b01e","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 14\" ND, 150 LB, RF, ASME B16.10, 15\" LG",null,null,"895.07","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","c4952511-c89f-5d19-b79c-2db81d13d837","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","95186260-05ab-4f34-9f3b-a9e4661430dd","Manual","HandWheel","66.5","31.5","False",{"$nulls":6},"Valve",null,"3858"]
[null,"16\"","CPVI001000","16","16","16","0","23.5","23.5","0","0","0","1.44","1.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","6572d619-0f55-2979-ca90-2ca99bd98d81","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 16\" ND, 150 LB, RF, ASME B16.10, 16\" LG",null,null,"1155.22","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"16","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","aa31ec4d-9878-55ba-8a78-499e82dcd829","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","e7b757cd-087d-47b7-9775-a17b2e752794","Manual","HandWheel","73.25","31.5","False",{"$nulls":6},"Valve",null,"3860"]
[null,"18\"","CPVI001000","18","18","17","0","25","25","0","0","0","1.56","1.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","05b80e39-f68b-151f-fb79-a76a1d52e794","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 18\" ND, 150 LB, RF, ASME B16.10, 17\" LG",null,null,"1587.32","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"17","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","6a2647d2-4cba-5a93-bede-36a3269fe945","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","ea29d9dc-eac3-422f-8b07-2a851d4650c6","Manual","HandWheel","82","43.25","False",{"$nulls":6},"Valve",null,"3862"]
[null,"20\"","CPVI001000","20","20","18","0","27.5","27.5","0","0","0","1.68","1.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d13d0a47-7f6c-6321-3bdc-ea90fb5a275b","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 20\" ND, 150 LB, RF, ASME B16.10, 18\" LG",null,null,"2462.56","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","7696894c-62ef-5264-965d-dca3c6980998","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","60165ae9-ac00-4b7f-bd73-40e4094b7ace","Manual","HandWheel","92","43.25","False",{"$nulls":6},"Valve",null,"3864"]
[null,"24\"","CPVI001000","24","24","20","0","32","32","0","0","0","1.87","1.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e059c5cb-1e93-62e9-1dac-9a989d2d3a19","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 24\" ND, 150 LB, RF, ASME B16.10, 20\" LG",null,null,"3231.97","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"20","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","a37c97c9-efd0-5ea9-808a-c0eccbf327ed","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","879658da-2bb0-4344-a874-3edf9988d3e0","Manual","HandWheel","107.5","78.5","False",{"$nulls":6},"Valve",null,"3866"]
[null,"26\"","CPVI001000","26","26","22","0","34.25","34.25","0","0","0","2.69","2.69","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b944f290-f21b-1f63-3caf-2238a35db0eb","ALL","26","in","26","FL",null,null,"RF","2.69","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 26\" ND, 150 LB, RF, ASME B16.10, 22\" LG",null,null,"3745.64","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","cfa98c8c-1059-56d7-867f-e8bf95335a1f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1df90dcc-8aed-4df7-9625-1161fe156ec4","Manual","HandWheel","115.5","78.5","False",{"$nulls":6},"Valve",null,"3868"]
[null,"28\"","CPVI001000","28","28","24","0","36.5","36.5","0","0","0","2.81","2.81","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b7bd34dd-f497-ecb9-4852-07b3f64887f0","ALL","28","in","28","FL",null,null,"RF","2.81","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 28\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,"4257.12","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","56994710-4f6e-5bd0-bcdf-cafbb025298d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f967a14-50de-418a-9806-0f90316e6e17","Manual","HandWheel","133.5","78.5","False",{"$nulls":6},"Valve",null,"3870"]
[null,"30\"","CPVI001000","30","30","24","0","38.75","38.75","0","0","0","2.94","2.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","a66b7119-8967-ac55-3ef1-db807b3ca57e","ALL","30","in","30","FL",null,null,"RF","2.94","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 30\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,"5246.99","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","78f2bbe5-672c-5185-844a-ea3cf6e5f28b","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","3aca9ba6-cada-4b93-998b-9ae0d21028fd","Manual","HandWheel","131","78.5","False",{"$nulls":6},"Valve",null,"3872"]
[null,"36\"","CPVI001000","36","36","28","0","46","46","0","0","0","3.56","3.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","4dbfb265-2169-7bcd-4109-9fbf2848925b","ALL","36","in","36","FL",null,null,"RF","3.56","150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 36\" ND, 150 LB, RF, ASME B16.10, 28\" LG",null,null,"7936.63","LB","VTFL","VALVE","0a479281-ea33-4d70-8446-5b6a67b62156","e9704340-2de7-48b2-834d-6000638c01cd",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"28","Inline","Continuous","Gate","False","False","e9704340-2de7-48b2-834d-6000638c01cd","f110dc0b-a2a4-531b-a86e-50f5f8cee367","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","50447195-3edf-4ced-9e1b-299b3b6464e1","Manual","HandWheel","166","78.5","False",{"$nulls":6},"Valve",null,"3874"]

{"sheet":"GATE VALVE_4","index":7,"n_rows":20,"n_cols":81,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI001000","0.84","0.84","4.25","0","0.84","0.84","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","da15db74-e91a-d644-763f-b770189c7d6d","ALL","0.5","in","0.84","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1/2\" ND, 150 LB, BW, ASME B16.10, 4 1/4\" LG",null,null,null,"LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","f4b5cfdf-dbf9-5c73-9b44-f6f68bffdb0a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3957"]
[null,"3/4\"","CPVI001000","1.05","1.05","4.62","0","1.05","1.05","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","89a9496b-7872-05db-803a-6473c97ccd3e","ALL","0.75","in","1.05","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 3/4\" ND, 150 LB, BW, ASME B16.10, 4 31/50\" LG",null,null,null,"LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.62","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","440a1142-4039-5e91-a15e-6db7fb399b47","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3995"]
[null,"1\"","CPVI001000","1.315","1.315","5","0","1.315","1.315","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","dd49999d-9640-5ad2-ed28-5128d7339687","ALL","1","in","1.315","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1\" ND, 150 LB, BW, ASME B16.10, 5\" LG",null,null,null,"LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","2c9a0cec-0c5c-5aa3-ba28-004f10869860","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3997"]
[null,"1 1/4\"","CPVI001000","1.66","1.66","5.5","0","1.66","1.66","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","0dfced1c-2e5e-a069-580b-73271a4ec4eb","ALL","1.25","in","1.66","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/4\" ND, 150 LB, BW, ASME B16.10, 5 1/2\" LG",null,null,null,"LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","8163ab80-45a7-5b41-92ac-e39089d2328b","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3999"]
[null,"1 1/2\"","CPVI001000","1.91","1.91","6.5","0","1.91","1.91","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","278c8272-6c53-935c-d06a-e6ae808a158f","ALL","1.5","in","1.91","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/2\" ND, 150 LB, BW, ASME B16.10, 6 1/2\" LG",null,null,null,"LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","39bc5fd2-6441-5bc4-a782-c19e7ac0d9e9","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4002"]
[null,"2\"","CPVI001000","2.375","2.375","8.5","0","2.375","2.375","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","cc65ecd6-890a-9597-85dc-ef7b09b725aa","ALL","2","in","2.375","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 2\" ND, 150 LB, BW, ASME B16.10, 8 1/2\" LG",null,null,"30","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","7c25b6dc-9e4e-5e89-9e51-277f51f1690d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4004"]
[null,"2 1/2\"","CPVI001000","2.875","2.875","9.5","0","2.875","2.875","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","a3600e66-a646-2509-9bcd-03253602876c","ALL","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 2 1/2\" ND, 150 LB, BW, ASME B16.10, 9 1/2\" LG",null,null,"40","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9.5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","396432dd-0190-505f-9546-79e5fae1e548","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4006"]
[null,"3\"","CPVI001000","3.5","3.5","11.12","0","3.5","3.5","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","35627e0d-fa9e-83f8-751b-1b29f458f871","ALL","3","in","3.5","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 3\" ND, 150 LB, BW, ASME B16.10, 11 3/25\" LG",null,null,"70","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.12","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","d6d420c6-137f-5f5e-a777-03c93f1c79e3","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","Manual","HandWheel","21.75","11.75","False",{"$nulls":6},"Valve",null,"4008"]
[null,"4\"","CPVI001000","4.5","4.5","12","0","4.5","4.5","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b646696e-cd9a-9dc2-23c4-d1b9b477afb2","ALL","4","in","4.5","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 4\" ND, 150 LB, BW, ASME B16.10, 12\" LG",null,null,"100","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"12","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","5b898293-d299-54c2-8ad1-b223d142e51e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","Manual","HandWheel","27","11.75","False",{"$nulls":6},"Valve",null,"4010"]
[null,"6\"","CPVI001000","6.625","6.625","15.88","0","6.625","6.625","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","f105fad9-56ee-6d5a-c5da-b9383b61c288","ALL","6","in","6.625","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 6\" ND, 150 LB, BW, ASME B16.10, 15 22/25\" LG",null,null,"180","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15.88","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","678d9e47-2477-528f-ac2d-0025d29b4955","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7f821266-6705-432f-9d82-62fb1dc61b9b","Manual","HandWheel","33.25","15.75","False",{"$nulls":6},"Valve",null,"4012"]
[null,"8\"","CPVI001000","8.625","8.625","16.5","0","8.625","8.625","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","a7d81b16-7a7c-243f-3379-1213ecee3351","ALL","8","in","8.625","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 8\" ND, 150 LB, BW, ASME B16.10, 16 1/2\" LG",null,null,"270","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"16.5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","08da2d9f-a610-5006-af25-e1d34b44b997","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f9150dd-0ada-454c-a5a8-f02b683b4441","Manual","HandWheel","42","19.5","False",{"$nulls":6},"Valve",null,"4014"]
[null,"10\"","CPVI001000","10.75","10.75","18","0","10.75","10.75","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e5bd39b9-7d6d-f98c-324b-3d49f1dec979","ALL","10","in","10.75","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 10\" ND, 150 LB, BW, ASME B16.10, 18\" LG",null,null,"450","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","93ee39f9-bfdc-5a6d-983c-d92656225c44","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","af90cd55-9525-410b-b2b6-c67760d26276","Manual","HandWheel","49.75","23.5","False",{"$nulls":6},"Valve",null,"4016"]
[null,"12\"","CPVI001000","12.75","12.75","19.75","0","12.75","12.75","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","41d4fef0-25a1-d1b6-db4d-8371119f2cdd","ALL","12","in","12.75","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 12\" ND, 150 LB, BW, ASME B16.10, 19 3/4\" LG",null,null,"640","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"19.75","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","6092e1fe-47c9-5b06-aa53-8244e44d6208","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","Manual","HandWheel","56.75","23.5","False",{"$nulls":6},"Valve",null,"4018"]
[null,"14\"","CPVI001000","14","14","22.5","0","14","14","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","0afd705b-2943-5063-6543-5be38590e0c3","ALL","14","in","14","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 14\" ND, 150 LB, BW, ASME B16.10, 22 1/2\" LG",null,null,"1015","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22.5","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","6f2b46ef-5411-5392-b779-fc8cc9038c55","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","95186260-05ab-4f34-9f3b-a9e4661430dd","Manual","HandWheel","66.5","31.5","False",{"$nulls":6},"Valve",null,"4020"]
[null,"16\"","CPVI001000","16","16","24","0","16","16","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","93a448d8-7a78-920e-0031-db27c0343bbd","ALL","16","in","16","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 16\" ND, 150 LB, BW, ASME B16.10, 24\" LG",null,null,"1500","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","15ff1568-8012-5929-8ea8-49a402ce239a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","e7b757cd-087d-47b7-9775-a17b2e752794","Manual","HandWheel","73.25","31.5","False",{"$nulls":6},"Valve",null,"4022"]
[null,"18\"","CPVI001000","18","18","26","0","18","18","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","4371fd7a-ea24-d192-a238-edaa7e49fa82","ALL","18","in","18","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 18\" ND, 150 LB, BW, ASME B16.10, 26\" LG",null,null,"2060","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"26","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","2858a323-0c04-5966-a929-6b54abd2771a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","ea29d9dc-eac3-422f-8b07-2a851d4650c6","Manual","HandWheel","82","43.25","False",{"$nulls":6},"Valve",null,"4024"]
[null,"20\"","CPVI001000","20","20","28","0","20","20","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5e64f784-3b8a-2186-5ff4-f554011f651a","ALL","20","in","20","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 20\" ND, 150 LB, BW, ASME B16.10, 28\" LG",null,null,"2360","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"28","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","1243c34b-9e94-5dae-923a-4b7536590bcb","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","60165ae9-ac00-4b7f-bd73-40e4094b7ace","Manual","HandWheel","92","43.25","False",{"$nulls":6},"Valve",null,"4026"]
[null,"24\"","CPVI001000","24","24","32","0","24","24","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","8ce4b18c-b266-eced-c857-d81424d72649","ALL","24","in","24","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 24\" ND, 150 LB, BW, ASME B16.10, 32\" LG",null,null,"3480","LB","VTBW","VALVE","c7e02b76-4dd8-4690-b94f-4d24d2826c0d","799bbb13-28c0-4237-b4e6-f108cbf07daa",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"32","Inline","Continuous","Gate","False","False","799bbb13-28c0-4237-b4e6-f108cbf07daa","58321d80-db2c-5f03-8e43-f5f3e1c24a0e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","879658da-2bb0-4344-a874-3edf9988d3e0","Manual","HandWheel","107.5","78.5","False",{"$nulls":6},"Valve",null,"4028"]

{"sheet":"PLUG VALVE_4","index":8,"n_rows":13,"n_cols":81,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"4\"","CPVI010000","4.5","4.5","12","0","9","9","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","ac2714de-8f32-9b2e-feb9-52692c3790f9","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 4\" ND, 150 LB, RF, ASME B16.10, 12\" LG",null,null,"79","LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"12","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","8f4fccca-892f-5e2f-85df-0262b85bfdbd","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","2a1e71a8-cea2-469a-af13-672596bc151a","Manual","HandLever","13.875","44","False",{"$nulls":6},"Valve",null,"4332"]
[null,"5\"","CPVI010000","5.56","5.56","15","0","10","10","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d7fc6b9c-b4c9-da5c-18ca-d2df750d8487","ALL","5","in","5.563","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 5\" ND, 150 LB, RF, ASME B16.10, 15\" LG",null,null,null,"LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","57a9cb3f-f294-5a8e-8284-e0973c0f9452","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","3b428250-2347-4a52-9bb5-8497ecb0f6dd","Manual","HandLever","8.75","30","False",{"$nulls":6},"Valve",null,"4348"]
[null,"6\"","CPVI010000","6.63","6.63","15.5","0","11","11","0","0","-1","1","1","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b8230ce1-98a0-acbb-e425-280bb9c6e91f","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 6\" ND, 150 LB, RF, ASME B16.10, 15 1/2\" LG",null,null,"122","LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15.5","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","acc4bbd3-9ea8-5f65-ae97-1651714ba67f","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b985b3ec-3421-4a14-b498-3d5f49b52589","Manual","HandLever","11.5","30","False",{"$nulls":6},"Valve",null,"4350"]
[null,"8\"","CPVI010000","8.63","8.63","18","0","13.5","13.5","0","0","-1","1.12","1.12","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b72b7d80-3881-aca1-aed6-4843e4b66995","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 8\" ND, 150 LB, RF, ASME B16.10, 18\" LG",null,null,"220","LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","164c49a9-807c-5680-9201-3776a831c303","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5c04ba24-a4ed-4794-a425-069eb5c978ed","Manual","HandLever","13.5","30","False",{"$nulls":6},"Valve",null,"4352"]
[null,"10\"","CPVI010000","10.75","10.75","21","0","16","16","0","0","-1","1.18","1.18","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b38148b8-9ba6-f154-170d-8b736fb2e1b0","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 10\" ND, 150 LB, RF, ASME B16.10, 21\" LG",null,null,"330","LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"21","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","db44fb86-71d9-535c-aca8-3e41ab76b340","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","4011aff6-fa15-409c-a0d0-5cc7734c9887","Manual","HandLever","15.25","30","False",{"$nulls":6},"Valve",null,"4354"]
[null,"12\"","CPVI010000","12.75","12.75","24","0","19","19","0","0","-1","1.25","1.25","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","4f84a662-fdd2-2c6d-c770-2e48b8a13314","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 12\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,"437","LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","e6083f13-8437-573a-a7ed-b99af3988fd2","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","Manual","HandLever","16.25","30","False",{"$nulls":6},"Valve",null,"4356"]
[null,"14\"","CPVI010000","14","14","27","0","21","21","0","0","-1","1.37","1.37","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","73110e1e-f976-ded6-2038-aa27ae163bf6","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 14\" ND, 150 LB, RF, ASME B16.10, 27\" LG",null,null,"650","LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"27","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","e5234984-fd13-507e-a3ad-e0366ddcb4c2","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4358"]
[null,"16\"","CPVI010000","16","16","30","0","23.5","23.5","0","0","-1","1.44","1.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","cb5661e3-baab-ed5d-f0e3-68783e9423ae","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 16\" ND, 150 LB, RF, ASME B16.10, 30\" LG",null,null,null,"LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"30","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","474e2255-088d-5e09-ae28-1dd5a5223a0f","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4360"]
[null,"18\"","CPVI010000","18","18","34","0","25","25","0","0","-1","1.56","1.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","ae1372ce-3e98-e7f6-f17c-46a348e69d75","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 18\" ND, 150 LB, RF, ASME B16.10, 34\" LG",null,null,null,"LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"34","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","723730ee-b1c9-5cb5-9045-cb108ad094e1","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4362"]
[null,"20\"","CPVI010000","20","20","36","0","27.5","27.5","0","0","-1","1.68","1.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","942e43ec-01ce-9cc3-3bc9-51aa8605f2c9","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 20\" ND, 150 LB, RF, ASME B16.10, 36\" LG",null,null,null,"LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","a07314db-10d8-53f9-8e44-03a17ee8b8af","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4364"]
[null,"24\"","CPVI010000","24","24","42","0","32","32","0","0","-1","1.87","1.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","c4069e20-92d8-ad97-64cf-d1e65a492072","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 24\" ND, 150 LB, RF, ASME B16.10, 42\" LG",null,null,null,"LB","VPFL","VALVE","72347e66-ec50-448c-97bf-0f05770992d7","d6c762c5-c43d-4d28-967a-cd99aa115805",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"42","Inline","Continuous","Plug","False","False","d6c762c5-c43d-4d28-967a-cd99aa115805","54e33dd9-2638-5214-9ea6-ce7ba36c7c26","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4366"]

{"sheet":"PLUG VALVE_3","index":9,"n_rows":13,"n_cols":81,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1\"","CPVI010000","1.32","1.32","5.5","0","4.25","4.25","0","0","-1","0.56","0.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","83273c19-9617-a0e9-c7b2-9f0216d41aec","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 1\" ND, 150 LB, RF, ASME B16.10, 5 1/2\" LG",null,null,null,"LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","945060e0-b180-592e-ad3b-e8beda80d3ba","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","37894da0-c8af-467e-ad0c-c1b2f6e65219","Manual","HandLever","2.88","8.75","False",{"$nulls":6},"Valve",null,"4178"]
[null,"1 1/2\"","CPVI010000","1.91","1.91","6.5","0","5","5","0","0","-1","0.68","0.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","ea2886a6-c293-0921-42e2-794f0c83b405","ALL","1.5","in","1.91","FL",null,null,"RF","0.68","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 6 1/2\" LG",null,null,"33.07","LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","87a4f227-d0f1-534a-9dd8-948c6efa70ee","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","95f070a6-4fd5-4323-a634-1ba9ed7e13fb","Manual","HandLever","3.6","12.5","False",{"$nulls":6},"Valve",null,"4201"]
[null,"2\"","CPVI010000","2.38","2.38","7","0","6","6","0","0","-1","0.75","0.75","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","442a128d-8212-fc7f-e839-3706c665ea21","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 2\" ND, 150 LB, RF, ASME B16.10, 7\" LG",null,null,"44.09","LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","b4b5ed11-3fc7-501e-bd43-48807458ac00","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba14331c-3cfe-463c-abca-3a629699735a","Manual","HandLever","4","18","False",{"$nulls":6},"Valve",null,"4203"]
[null,"2 1/2\"","CPVI010000","2.88","2.88","7.5","0","7","7","0","0","-1","0.87","0.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","8334f1e0-5b1c-f5da-1cd0-9f56efc47a8c","ALL","2.5","in","2.875","FL",null,null,"RF","0.87","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 7 1/2\" LG",null,null,"66.14","LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7.5","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","d6e0c74e-3589-5ea5-8524-2dd452379148","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","bae61cb2-cd55-422f-b094-cbcf4aec2474","Manual","HandLever","5.7","24","False",{"$nulls":6},"Valve",null,"4205"]
[null,"3\"","CPVI010000","3.5","3.5","8","0","7.5","7.5","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","c142db86-1b0f-f7f9-f3fc-f63cc6bcd0ae","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 3\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,"88.19","LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","3cb3efe8-9542-567d-8047-3ff4366b34ec","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","bae61cb2-cd55-422f-b094-cbcf4aec2474","Manual","HandLever","5.7","24","False",{"$nulls":6},"Valve",null,"4207"]
[null,"4\"","CPVI010000","4.5","4.5","9","0","9","9","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","22c2e8d5-b873-e5ef-f460-78b1f594a4dc","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 4\" ND, 150 LB, RF, ASME B16.10, 9\" LG",null,null,"132.28","LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","249c8132-433b-5c08-aa65-ce275022fcd4","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81badf1-6af2-4061-a972-33a3924e8242","Manual","HandLever","8.7402","26.5354","False",{"$nulls":6},"Valve",null,"4209"]
[null,"5\"","CPVI010000","5.56","5.56","10","0","10","10","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","f3f62cdb-89f8-aef3-2e11-36781877da3b","ALL","5","in","5.563","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 5\" ND, 150 LB, RF, ASME B16.10, 10\" LG",null,null,null,"LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","57db7fd5-62b5-55b6-8407-9ffc98930848","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","3b428250-2347-4a52-9bb5-8497ecb0f6dd","Manual","HandLever","8.75","30","False",{"$nulls":6},"Valve",null,"4211"]
[null,"6\"","CPVI010000","6.63","6.63","10.5","0","11","11","0","0","-1","1","1","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","57fbdc4e-4825-39b2-b8b2-b3134f4c6f89","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 6\" ND, 150 LB, RF, ASME B16.10, 10 1/2\" LG",null,null,"242.51","LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10.5","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","0196192e-ac0e-5ce2-8068-01c15e33c9be","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b985b3ec-3421-4a14-b498-3d5f49b52589","Manual","HandLever","11.5","30","False",{"$nulls":6},"Valve",null,"4213"]
[null,"8\"","CPVI010000","8.63","8.63","11.5","0","13.5","13.5","0","0","-1","1.12","1.12","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","f72abc4a-ac96-a1ad-59d9-81cc6338fc1e","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 8\" ND, 150 LB, RF, ASME B16.10, 11 1/2\" LG",null,null,null,"LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.5","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","5e8fa65f-f2f3-5379-817c-1ea8fe522158","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5c04ba24-a4ed-4794-a425-069eb5c978ed","Manual","HandLever","13.5","30","False",{"$nulls":6},"Valve",null,"4215"]
[null,"10\"","CPVI010000","10.75","10.75","13","0","16","16","0","0","-1","1.18","1.18","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","c66c9785-5af3-149d-165d-dc5004c853a0","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 10\" ND, 150 LB, RF, ASME B16.10, 13\" LG",null,null,null,"LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","6e5871dd-bc1a-5153-9dc6-5cbfe7c33c20","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","4011aff6-fa15-409c-a0d0-5cc7734c9887","Manual","HandLever","15.25","30","False",{"$nulls":6},"Valve",null,"4217"]
[null,"12\"","CPVI010000","12.75","12.75","14","0","19","19","0","0","-1","1.25","1.25","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3beb081d-397d-9e78-0bea-6602cc2fe3e4","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,"0","in","Plug Valve","ASME B16.10","Short Pattern","Plug Valve, Short Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, SHORT PATTERN, 12\" ND, 150 LB, RF, ASME B16.10, 14\" LG",null,null,null,"LB","VPFL","VALVE","3a581e60-b24f-4444-ab6c-2d03fc81879d","ac2ef88f-0428-4492-af8c-f71ff73a41e7",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Plug","False","False","ac2ef88f-0428-4492-af8c-f71ff73a41e7","5e32e8a3-5c73-5f60-a666-adfdb57a7da7","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","Manual","HandLever","16.25","30","False",{"$nulls":6},"Valve",null,"4219"]

{"sheet":"BUTTERFLY VALVE_1","index":10,"n_rows":13,"n_cols":83,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H11","H12","H21","H22","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H11","H12","H21","H22","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPVI256000","3.5","3.5","1.88","0","7.5","7.5","6.75","6.75","0","0","-1","0.94","0.94","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","1a29f3ee-c7da-8f84-7b91-7ebaa365611b","ALL","3","in","3.5","LUG",null,null,"RF","0.94","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 3\" ND, 150 LB, LUG, RF, ASME B16.10, 1 22/25\" LG",null,null,"11.02","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"1.88","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","d8f4f0fa-c966-58a5-9201-10b5dbcfba83","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","14a38483-5252-44c9-b313-4af077f430a4","Manual","HandLever","7","6.5","False",{"$nulls":6},"Valve",null,"3569"]
[null,"4\"","CPVI256000","4.5","4.5","2.12","0","9","9","8.1","8.1","0","0","-1","0.94","0.94","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","7da162be-80c2-7698-03ed-409c3272c10a","ALL","4","in","4.5","LUG",null,null,"RF","0.94","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 4\" ND, 150 LB, LUG, RF, ASME B16.10, 2 3/25\" LG",null,null,"16.98","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.12","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","96afb3b8-e00e-5a80-9d19-88838c434d28","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","3eafb794-44d6-4307-81eb-bfb9b676421e","Manual","HandLever","7.75","10.5","False",{"$nulls":6},"Valve",null,"3595"]
[null,"6\"","CPVI256000","6.63","6.63","2.25","0","11","11","9.9","9.9","0","0","-1","1","1","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","208a070b-2ebd-a65f-96c2-7644db4e3988","ALL","6","in","6.63","LUG",null,null,"RF","1","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 6\" ND, 150 LB, LUG, RF, ASME B16.10, 2 1/4\" LG",null,null,"29.98","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.25","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","ed86f000-455c-58b0-910b-9d7fa78941be","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5559017f-64c8-4534-a5ec-c0c8fa2b960b","Manual","HandLever","8.75","10.5","False",{"$nulls":6},"Valve",null,"3597"]
[null,"8\"","CPVI256000","8.63","8.63","2.5","0","13.5","13.5","12.15","12.15","0","0","-1","1.12","1.12","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","0c9b4f9c-81a6-7475-ebca-3eea2cac8528","ALL","8","in","8.63","LUG",null,null,"RF","1.12","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 8\" ND, 150 LB, LUG, RF, ASME B16.10, 2 1/2\" LG",null,null,"44.09","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.5","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","48895582-6ecd-5967-92ec-c803d8745226","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5a101043-71bb-43ee-b8b1-f88ffc9fd7b0","Manual","HandLever","10.25","14","False",{"$nulls":6},"Valve",null,"3599"]
[null,"10\"","CPVI256000","10.75","10.75","2.81","0","16","16","14.4","14.4","0","0","-1","1.19","1.19","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","bf7f94da-c797-6cbf-9d6f-452ebfcb5721","ALL","10","in","10.75","LUG",null,null,"RF","1.19","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 10\" ND, 150 LB, LUG, RF, ASME B16.10, 2 81/100\" LG",null,null,"70.55","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.81","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","a71fa2bf-7027-52f4-aee6-55fa9f9dfa00","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ddcb694e-a0f1-411a-b499-42359fc626dc","Manual","HandLever","11.5","14","False",{"$nulls":6},"Valve",null,"3602"]
[null,"12\"","CPVI256000","12.75","12.75","3.19","0","19","19","17.1","17.1","0","0","-1","1.25","1.25","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","dae18843-24b6-e9a0-b9c4-5a12c1a1f206","ALL","12","in","12.75","LUG",null,null,"RF","1.25","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 12\" ND, 150 LB, LUG, RF, ASME B16.10, 3 5/25\" LG",null,null,"66.14","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"3.19","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","a93e22e2-0440-59b3-b32d-0a5c8a5aec2f","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","cea247f5-355c-40af-84eb-eddcd1f98df3","Manual","HandLever","13.25","14","False",{"$nulls":6},"Valve",null,"3604"]
[null,"14\"","CPVI256000","14","14","3.62","0","21","21","18.9","18.9","0","0","-1","1.38","1.38","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","16a4f7b5-571d-b2fc-daad-b9bbfa7bd5c2","ALL","14","in","14","LUG",null,null,"RF","1.38","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 14\" ND, 150 LB, LUG, RF, ASME B16.10, 3 31/50\" LG",null,null,"134.48","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"3.62","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","76c67d36-e389-5721-a544-c858cd8f3b8d","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","e681b696-660d-46c3-a52d-02765ba90bec","Manual","HandLever","14.5","14","False",{"$nulls":6},"Valve",null,"3606"]
[null,"16\"","CPVI256000","16","16","4","0","23.5","23.5","21.15","21.15","0","0","-1","1.44","1.44","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","57809666-2260-7f62-e174-9f7dee5b106f","ALL","16","in","16","LUG",null,null,"RF","1.44","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 16\" ND, 150 LB, LUG, RF, ASME B16.10, 4\" LG",null,null,"182.98","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","815fc625-75ed-56cb-bbc8-400ac217cd33","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","45730dd4-988d-48e3-978e-5de04277f5dc","Manual","HandLever","15.75","14","False",{"$nulls":6},"Valve",null,"3608"]
[null,"18\"","CPVI256000","18","18","4.5","0","25","25","22.5","22.5","0","0","-1","1.56","1.56","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","e676b1a6-cf6e-1015-1970-16d069c8aa06","ALL","18","in","18","LUG",null,null,"RF","1.56","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 18\" ND, 150 LB, LUG, RF, ASME B16.10, 4 1/2\" LG",null,null,"233.69","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.5","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","ce412070-4049-5bfa-a465-a32296be576b","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","e3817f3d-3795-461a-9d63-f89ce6a43eba","Manual","HandLever","16.5","14","False",{"$nulls":6},"Valve",null,"3610"]
[null,"20\"","CPVI256000","20","20","5","0","27.5","27.5","24.75","24.75","0","0","-1","1.69","1.69","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","aaa22ecb-6c37-3816-7b10-06d469005c6c","ALL","20","in","20","LUG",null,null,"RF","1.69","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 20\" ND, 150 LB, LUG, RF, ASME B16.10, 5\" LG",null,null,"319.67","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","c656c7cb-0591-545d-a818-0d20dba18946","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","27092ef5-afd7-4ded-987f-99fce4e691cc","Manual","HandLever","18.75","14","False",{"$nulls":6},"Valve",null,"3612"]
[null,"24\"","CPVI256000","24","24","6.06","0","32","32","28.8","28.8","0","0","-1","1.88","1.88","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","31342c04-d3e5-bb2d-6c59-739d699d4c51","ALL","24","in","24","LUG",null,null,"RF","1.88","150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, LUG, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 24\" ND, 150 LB, LUG, RF, ASME B16.10, 6 3/50\" LG",null,null,"504.86","LB","VYFL","VALVE","98b9e84f-5a47-45ec-9f1c-e34699f78e38","66b61acb-8db3-48b2-a865-7f5420b9258b",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.06","Inline","Continuous","Butterfly","False","False","66b61acb-8db3-48b2-a865-7f5420b9258b","a55cda94-96d4-5c29-bce3-6f5b83f0e8ed","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b72129de-f087-4db9-9c9b-3793a4ce05bf","Manual","HandLever","21","14","False",{"$nulls":6},"Valve",null,"3614"]

{"sheet":"PLUG VALVE_2","index":11,"n_rows":14,"n_cols":81,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"2\"","CPVI010000","2.38","2.38","7","0","6","6","0","0","-1","0.75","0.75","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","2da6535c-4e0b-7a9b-d516-17f7d04286bf","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 2\" ND, 150 LB, RF, ASME B16.10, 7\" LG",null,null,null,"LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","15297e2a-51cf-5715-97fd-b0270fca963a","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba14331c-3cfe-463c-abca-3a629699735a","Manual","HandLever","4","18","False",{"$nulls":6},"Valve",null,"4255"]
[null,"3\"","CPVI010000","3.5","3.5","8","0","7.5","7.5","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","2b19c5a6-6ab0-c2f6-ab54-3ae24981bfe7","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 3\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,null,"LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","69312f9b-3489-5071-8f0c-39d89c336f56","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","bae61cb2-cd55-422f-b094-cbcf4aec2474","Manual","HandLever","5.7","24","False",{"$nulls":6},"Valve",null,"4275"]
[null,"4\"","CPVI010000","4.5","4.5","9","0","9","9","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","49106c9a-3e50-6484-b70f-ba293872258e","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 4\" ND, 150 LB, RF, ASME B16.10, 9\" LG",null,null,null,"LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","ec3342fd-9e07-5a99-a5b1-f94248f1a2a2","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81badf1-6af2-4061-a972-33a3924e8242","Manual","HandLever","8.7402","26.5354","False",{"$nulls":6},"Valve",null,"4277"]
[null,"6\"","CPVI010000","6.63","6.63","15.5","0","11","11","0","0","-1","1","1","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","61ed40ad-8230-7064-39d1-ae84985a41e1","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 6\" ND, 150 LB, RF, ASME B16.10, 15 1/2\" LG",null,null,"297.62","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15.5","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","9c19e8ca-921e-5d77-8f94-f9b1db949a00","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b985b3ec-3421-4a14-b498-3d5f49b52589","Manual","HandLever","11.5","30","False",{"$nulls":6},"Valve",null,"4279"]
[null,"8\"","CPVI010000","8.63","8.63","18","0","13.5","13.5","0","0","-1","1.12","1.12","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","9a6aba31-91f9-6a72-452b-b19b2106b73b","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 8\" ND, 150 LB, RF, ASME B16.10, 18\" LG",null,null,"374.79","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","171bf538-cb2f-587e-b375-97be01336cfa","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5c04ba24-a4ed-4794-a425-069eb5c978ed","Manual","HandLever","13.5","30","False",{"$nulls":6},"Valve",null,"4281"]
[null,"10\"","CPVI010000","10.75","10.75","21","0","16","16","0","0","-1","1.18","1.18","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","8025ec35-c70c-f9fb-7d9e-6c52e7017f6c","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 10\" ND, 150 LB, RF, ASME B16.10, 21\" LG",null,null,"507.06","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"21","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","f4c4d530-b909-5205-b310-77c6296ddba2","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","4011aff6-fa15-409c-a0d0-5cc7734c9887","Manual","HandLever","15.25","30","False",{"$nulls":6},"Valve",null,"4283"]
[null,"12\"","CPVI010000","12.75","12.75","24","0","19","19","0","0","-1","1.25","1.25","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","306498f7-1f42-ef34-bfac-c03940055c60","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 12\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,"771.62","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","7cbfe5d5-4fca-5105-8496-9154e0f56c92","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","8a849e1f-7bf0-48a0-93c4-06c9a65d012b","Manual","HandLever","16.25","30","False",{"$nulls":6},"Valve",null,"4285"]
[null,"14\"","CPVI010000","14","14","27","0","21","21","0","0","-1","1.37","1.37","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","6b383657-ea40-7624-e7e5-727ca83ea3ae","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 14\" ND, 150 LB, RF, ASME B16.10, 27\" LG",null,null,"1014.13","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"27","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","a156936c-9102-5299-8086-862abd351100","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4287"]
[null,"16\"","CPVI010000","16","16","30","0","23.5","23.5","0","0","-1","1.44","1.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d0b835e1-71b0-fa63-3c33-f4b110dbd932","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 16\" ND, 150 LB, RF, ASME B16.10, 30\" LG",null,null,"1543.23","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"30","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","e252dcbd-8013-522c-a6f0-227e23668bd5","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4289"]
[null,"18\"","CPVI010000","18","18","34","0","25","25","0","0","-1","1.56","1.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e9324f58-8e73-d64a-08b5-da813a4831ac","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 18\" ND, 150 LB, RF, ASME B16.10, 34\" LG",null,null,"1940.07","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"34","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","0bb92706-ca22-5121-9d71-c5c50e1aca59","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4291"]
[null,"20\"","CPVI010000","20","20","36","0","27.5","27.5","0","0","-1","1.68","1.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","9245741e-c593-c743-393f-8a871f531fd8","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 20\" ND, 150 LB, RF, ASME B16.10, 36\" LG",null,null,"2314.85","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","792e9656-36c7-5aff-bd0b-e232b321ed30","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4293"]
[null,"24\"","CPVI010000","24","24","42","0","32","32","0","0","-1","1.87","1.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","936fa054-87ea-e493-1583-e68d81d0c08f","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,"0","in","Plug Valve","ASME B16.10","Venturi","Plug Valve, Venturi, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, VENTURI, 24\" ND, 150 LB, RF, ASME B16.10, 42\" LG",null,null,"4475.38","LB","VPFL","VALVE","ae47a14b-f45a-4ac7-a70d-421915312b3d","b5b85be9-06d5-4880-bbe2-e1621fd46937",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"42","Inline","Continuous","Plug","False","False","b5b85be9-06d5-4880-bbe2-e1621fd46937","28d41f70-666c-5662-99ce-19419e94b1df","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba801f79-2792-4e8d-9e8a-831bcc3c30f0","Manual","HandLever","21.5","30","False",{"$nulls":6},"Valve",null,"4295"]

{"sheet":"PLUG VALVE_1","index":12,"n_rows":8,"n_cols":81,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1\"","CPVI010000","1.32","1.32","7","0","4.25","4.25","0","0","-1","0.56","0.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d6aaeb96-9a1b-ad36-fab3-b9c6d001e002","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,"0","in","Plug Valve","ASME B16.10","Full Bore","Plug Valve, Full Bore, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, FULL BORE, 1\" ND, 150 LB, RF, ASME B16.10, 7\" LG",null,null,"8","LB","VPFL","VALVE","61b58248-0ad4-4043-ad1b-bc6f422043ca","7c795669-47e5-45fe-82ad-98e5dca118ad",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7","Inline","Continuous","Plug","False","False","7c795669-47e5-45fe-82ad-98e5dca118ad","80e35f57-5334-56dc-ab9b-ddbe832093ae","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","37894da0-c8af-467e-ad0c-c1b2f6e65219","Manual","HandLever","2.88","8.75","False",{"$nulls":6},"Valve",null,"4146"]
[null,"1 1/2\"","CPVI010000","1.91","1.91","8.75","0","5","5","0","0","-1","0.68","0.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e9554197-9632-8949-3e0e-48f378ac4932","ALL","1.5","in","1.91","FL",null,null,"RF","0.68","150",null,null,"0","in","Plug Valve","ASME B16.10","Full Bore","Plug Valve, Full Bore, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, FULL BORE, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 8 3/4\" LG",null,null,"14","LB","VPFL","VALVE","61b58248-0ad4-4043-ad1b-bc6f422043ca","7c795669-47e5-45fe-82ad-98e5dca118ad",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.75","Inline","Continuous","Plug","False","False","7c795669-47e5-45fe-82ad-98e5dca118ad","1abf0ee0-173a-54df-9e2a-1e0d740534ed","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","95f070a6-4fd5-4323-a634-1ba9ed7e13fb","Manual","HandLever","3.6","12.5","False",{"$nulls":6},"Valve",null,"4168"]
[null,"2\"","CPVI010000","2.38","2.38","10.5","0","6","6","0","0","-1","0.75","0.75","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","88b6c628-f755-e4f8-6fe4-1517f6580571","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,"0","in","Plug Valve","ASME B16.10","Full Bore","Plug Valve, Full Bore, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, FULL BORE, 2\" ND, 150 LB, RF, ASME B16.10, 10 1/2\" LG",null,null,"23","LB","VPFL","VALVE","61b58248-0ad4-4043-ad1b-bc6f422043ca","7c795669-47e5-45fe-82ad-98e5dca118ad",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10.5","Inline","Continuous","Plug","False","False","7c795669-47e5-45fe-82ad-98e5dca118ad","d84f6e47-034d-584d-a2d4-1016769d5bb0","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ba14331c-3cfe-463c-abca-3a629699735a","Manual","HandLever","4","18","False",{"$nulls":6},"Valve",null,"4170"]
[null,"2 1/2\"","CPVI010000","2.88","2.88","11.75","0","7","7","0","0","-1","0.87","0.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3a6e92f9-2e49-4e75-45d8-cd9aa20d5fda","ALL","2.5","in","2.875","FL",null,null,"RF","0.87","150",null,null,"0","in","Plug Valve","ASME B16.10","Full Bore","Plug Valve, Full Bore, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, FULL BORE, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 11 3/4\" LG",null,null,"36","LB","VPFL","VALVE","61b58248-0ad4-4043-ad1b-bc6f422043ca","7c795669-47e5-45fe-82ad-98e5dca118ad",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.75","Inline","Continuous","Plug","False","False","7c795669-47e5-45fe-82ad-98e5dca118ad","ea598309-8baa-5462-8d9e-fcf6fc722c8e","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","bae61cb2-cd55-422f-b094-cbcf4aec2474","Manual","HandLever","5.7","24","False",{"$nulls":6},"Valve",null,"4172"]
[null,"3\"","CPVI010000","3.5","3.5","13.5","0","7.5","7.5","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3205bed0-b38a-af5a-f98b-8404f3055e21","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Full Bore","Plug Valve, Full Bore, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, FULL BORE, 3\" ND, 150 LB, RF, ASME B16.10, 13 1/2\" LG",null,null,"36","LB","VPFL","VALVE","61b58248-0ad4-4043-ad1b-bc6f422043ca","7c795669-47e5-45fe-82ad-98e5dca118ad",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13.5","Inline","Continuous","Plug","False","False","7c795669-47e5-45fe-82ad-98e5dca118ad","570b1c72-6134-5097-94d1-75a21922f986","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","bae61cb2-cd55-422f-b094-cbcf4aec2474","Manual","HandLever","5.7","24","False",{"$nulls":6},"Valve",null,"4174"]
[null,"4\"","CPVI010000","4.5","4.5","17","0","9","9","0","0","-1","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","84e9fa05-9810-eb4b-5388-ffa4575a7696","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Plug Valve","ASME B16.10","Full Bore","Plug Valve, Full Bore, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, FULL BORE, 4\" ND, 150 LB, RF, ASME B16.10, 17\" LG",null,null,"79","LB","VPFL","VALVE","61b58248-0ad4-4043-ad1b-bc6f422043ca","7c795669-47e5-45fe-82ad-98e5dca118ad",{"$nulls":4},"2",null,"Valves","SKEY=VPFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"17","Inline","Continuous","Plug","False","False","7c795669-47e5-45fe-82ad-98e5dca118ad","928e5e5d-db4a-51d2-b2b5-a646a2c1986d","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81badf1-6af2-4061-a972-33a3924e8242","Manual","HandLever","8.7402","26.5354","False",{"$nulls":6},"Valve",null,"4176"]

{"sheet":"BALL VALVE_1","index":13,"n_rows":22,"n_cols":97,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1 1/2\"","CPVI008000","1.91","1.91","7.5","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","21db5b22-8b95-29f4-811d-dccd0aab2572","S1","1.5","in","1.91","BV",{"$nulls":4},"150",null,null,"0","in","c191322c-981a-418c-9b77-f7fe97bf29e6","S2","1.5","in","1.91","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 1 1/2\" ND, 150 LB, BW, ASME B16.10, 7 1/2\" LG",null,null,"35.27","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7.5","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","86bbf81b-b64c-5e23-9de7-da2294e82178","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81efdd5-2420-4cfc-9293-bd52bdc68339","Manual","HandLever","4.5","6.5","False",{"$nulls":6},"Valve",null,"3384"]
[null,"2\"","CPVI008000","2.375","2.375","8.5","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","6b389a9b-7fb2-3d68-0fdf-7b5ed42f1817","S1","2","in","2.375","BV",{"$nulls":4},"150",null,null,"0","in","d20e5454-522b-41bb-9ceb-13be4cdf6283","S2","2","in","2.375","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 2\" ND, 150 LB, BW, ASME B16.10, 8 1/2\" LG",null,null,"41.88","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","f36ff695-0acb-5a28-888c-83a64206825f","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81efdd5-2420-4cfc-9293-bd52bdc68339","Manual","HandLever","4.5","6.5","False",{"$nulls":6},"Valve",null,"3425"]
[null,"2 1/2\"","CPVI008000","2.875","2.875","9.5","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","5ea1e08e-1e24-462a-f1ce-6ca90766f862","S1","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,"0","in","b018afb4-e05a-4074-a35f-8d5f06b29c6a","S2","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 2 1/2\" ND, 150 LB, BW, ASME B16.10, 9 1/2\" LG",null,null,"57.32","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9.5","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","efc943ed-3209-5a94-8cfa-9ec48619c13a","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b1f8b162-a8db-43b9-bf35-537ed298e07a","Manual","HandLever","4.75","6.5","False",{"$nulls":6},"Valve",null,"3427"]
[null,"3\"","CPVI008000","3.5","3.5","11.12","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","d0148878-1e41-40fc-d0e3-e806b75eef08","S1","3","in","3.5","BV",{"$nulls":4},"150",null,null,"0","in","ed3c2e93-6cef-4585-835f-52718e61fd3b","S2","3","in","3.5","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 3\" ND, 150 LB, BW, ASME B16.10, 11 3/25\" LG",null,null,"79.36","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.12","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","ac394656-a127-5c97-8377-807824862147","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","de0125b4-373e-464d-b3fb-1c3d13be8ba9","Manual","HandLever","5","10.5","False",{"$nulls":6},"Valve",null,"3429"]
[null,"4\"","CPVI008000","4.5","4.5","12","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","2aed151a-e878-5392-69b8-2ee75177282e","S1","4","in","4.5","BV",{"$nulls":4},"150",null,null,"0","in","1d930b70-e1c7-44d4-adb0-6bc6fb22a275","S2","4","in","4.5","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 4\" ND, 150 LB, BW, ASME B16.10, 12\" LG",null,null,"112.43","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"12","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","4e8a06cc-b166-565d-a094-f82dfd72b13e","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","81d8de36-487e-43e8-a118-bee64679be4f","Manual","HandLever","5.5","10.5","False",{"$nulls":6},"Valve",null,"3431"]
[null,"6\"","CPVI008000","6.625","6.625","18","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","fc3690ba-2c55-b07f-24e8-26d7f45d8211","S1","6","in","6.625","BV",{"$nulls":4},"150",null,null,"0","in","2c19d758-b3c9-4576-ab69-05d797419a86","S2","6","in","6.625","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 6\" ND, 150 LB, BW, ASME B16.10, 18\" LG",null,null,"189.59","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","e98277ca-36d8-5cc8-932b-6401627a8627","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","0b48c097-258b-4e07-99a2-75ab6e1de5a2","Manual","HandLever","7","10.5","False",{"$nulls":6},"Valve",null,"3433"]
[null,"8\"","CPVI008000","8.625","8.625","20.5","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","89598e17-f374-6994-9152-627a51344ed2","S1","8","in","8.625","BV",{"$nulls":4},"150",null,null,"0","in","1b779fc7-06ca-4748-94c1-42b36e7bf249","S2","8","in","8.625","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 8\" ND, 150 LB, BW, ASME B16.10, 20 1/2\" LG",null,null,"302.03","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"20.5","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","2c62ea1a-b6b5-55d3-88ea-b10f8f0cf3f7","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","0bb4b333-0cca-4114-a794-8ef777a0aec9","Manual","HandLever","8","14","False",{"$nulls":6},"Valve",null,"3435"]
[null,"10\"","CPVI008000","10.75","10.75","22","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","50fb189a-a0e2-dccc-789f-9cec77ee5603","S1","10","in","10.75","BV",{"$nulls":4},"150",null,null,"0","in","dbde76ca-f131-47f9-8c3a-951be0d6b2d0","S2","10","in","10.75","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 10\" ND, 150 LB, BW, ASME B16.10, 22\" LG",null,null,"577.61","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","16b0fe6a-4367-58f1-a8d6-191a39918494","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","dcb67e85-ba74-4252-8d70-c13a0eb17c1c","Manual","HandLever","9","14","False",{"$nulls":6},"Valve",null,"3437"]
[null,"12\"","CPVI008000","12.75","12.75","25","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","e9e5eed1-77ac-0d8a-6f42-f62ad826ea11","S1","12","in","12.75","BV",{"$nulls":4},"150",null,null,"0","in","791806cf-bc77-4a50-b1cf-fc9985a8991f","S2","12","in","12.75","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 12\" ND, 150 LB, BW, ASME B16.10, 25\" LG",null,null,"769.41","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"25","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","8202f6f9-2bb0-5619-8d82-80f093694af6","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","c9366c8b-c436-460a-97c5-ae5419e5aa2d","Manual","HandLever","10","14","False",{"$nulls":6},"Valve",null,"3439"]
[null,"14\"","CPVI008000","14","14","30","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","9d064bd4-d239-a219-533d-e299e5fbcb18","S1","14","in","14","BV",{"$nulls":4},"150",null,null,"0","in","18f7a0af-d303-43a6-b651-42c3f4dc5680","S2","14","in","14","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 14\" ND, 150 LB, BW, ASME B16.10, 30\" LG",null,null,"1144.19","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"30","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","b350b145-4049-55c1-85c5-16a9aab58f2a","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","df388247-531c-47ef-bbe7-b63d17abdead","Manual","HandLever","11","14","False",{"$nulls":6},"Valve",null,"3441"]
[null,"16\"","CPVI008000","16","16","33","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","58a34dbe-dcec-52dc-6053-2105dafe16a9","S1","16","in","16","BV",{"$nulls":4},"150",null,null,"0","in","9eb4a7b2-2b22-4e43-86c1-5e00e97b3dcb","S2","16","in","16","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 16\" ND, 150 LB, BW, ASME B16.10, 33\" LG",null,null,"1649.05","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"33","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","005c342d-5594-55ea-93a2-3dcf563eb389","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","0d9b5135-4fc3-40db-b8cc-9955f70d82f5","Manual","HandLever","12","14","False",{"$nulls":6},"Valve",null,"3443"]
[null,"18\"","CPVI008000","18","18","36","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","d89a1652-a487-d238-9d6d-b681bcfe9e5f","S1","18","in","18","BV",{"$nulls":4},"150",null,null,"0","in","3240fd3b-cfce-4b25-9da7-e5a82907c5c4","S2","18","in","18","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 18\" ND, 150 LB, BW, ASME B16.10, 36\" LG",null,null,"2156.11","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","c8f186b7-e12a-534e-9e17-f2adda41de20","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","7d07ce87-7155-4217-a375-e784f9501de6","Manual","HandLever","13.5","14","False",{"$nulls":6},"Valve",null,"3445"]
[null,"20\"","CPVI008000","20","20","39","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","ba566fc9-b598-5de8-b440-a4d0b6106798","S1","20","in","20","BV",{"$nulls":4},"150",null,null,"0","in","aa7caea3-dc4d-451e-86c7-2bcfdd68bb8d","S2","20","in","20","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 20\" ND, 150 LB, BW, ASME B16.10, 39\" LG",null,null,"3093.08","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"39","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","21191a7f-63a8-5240-8e76-e7890adf34e4","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","98899958-b00c-419a-b9a9-1be7902cd941","Manual","HandLever","14","14","False",{"$nulls":6},"Valve",null,"3447"]
[null,"24\"","CPVI008000","24","24","45","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","253a4dde-67de-edb4-841f-a4da9ba4b658","S1","24","in","24","BV",{"$nulls":4},"150",null,null,"0","in","a7fd92bd-7a3e-4646-be72-69b59aef5614","S2","24","in","24","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 24\" ND, 150 LB, BW, ASME B16.10, 45\" LG",null,null,"4122.63","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"45","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","d19a1344-10a6-5a43-bd85-29e7775216a9","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","c6cb6dce-1151-4467-bc57-ebe08050091c","Manual","HandLever","16","14","False",{"$nulls":6},"Valve",null,"3449"]
[null,"26\"","CPVI008000","26","26","49","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","947ba356-9d46-3868-8aa9-0ed82fa66786","S1","26","in","26","BV",{"$nulls":4},"150",null,null,"0","in","505450c1-d6bf-4d01-91cc-dd7b8030dac8","S2","26","in","26","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 26\" ND, 150 LB, BW, ASME B16.10, 49\" LG",null,null,"4497.42","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"49","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","46dccfd3-a305-53a2-b3df-0030aaa1ec3b","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","140daba8-eca6-4b10-8453-23e47ffa713d","Manual","HandLever","17","16","False",{"$nulls":6},"Valve",null,"3451"]
[null,"28\"","CPVI008000","28","28","53","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","6e717887-0377-e1f4-224c-743bee07aa7d","S1","28","in","28","BV",{"$nulls":4},"150",null,null,"0","in","7e053c0d-fba1-41a7-8f62-9797bb40c4a9","S2","28","in","28","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 28\" ND, 150 LB, BW, ASME B16.10, 53\" LG",null,null,"5246.99","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"53","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","d04137e3-4e0e-57c9-bd6c-51beaf64b416","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","a4005ed0-298d-4584-ba75-a08e057a73bf","Manual","HandLever","18","16","False",{"$nulls":6},"Valve",null,"3453"]
[null,"30\"","CPVI008000","30","30","55","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","8fc480f4-8d9f-10b9-dce0-b070eb005ea0","S1","30","in","30","BV",{"$nulls":4},"150",null,null,"0","in","dc49217b-1ca8-4737-95fb-99f831212b2b","S2","30","in","30","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 30\" ND, 150 LB, BW, ASME B16.10, 55\" LG",null,null,"5809.17","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"55","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","99621a02-a607-5fe9-a548-f629083b1a35","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","a811db4b-e49b-4978-a35f-cb9c19558fd1","Manual","HandLever","19","16","False",{"$nulls":6},"Valve",null,"3455"]
[null,"32\"","CPVI008000","32","32","60","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","8a3e7c36-0b77-3a99-fb6b-fa0c7cb2badd","S1","32","in","32","BV",{"$nulls":4},"150",null,null,"0","in","d1462e6f-9cdd-4f06-8409-f2d270db7119","S2","32","in","32","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 32\" ND, 150 LB, BW, ASME B16.10, 60\" LG",null,null,"6371.35","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"60","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","0de9c3ba-e612-509f-bec2-c21ea5ccd660","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","9bc59a01-dfdc-495b-bbdf-b5e876c2e233","Manual","HandLever","20","16","False",{"$nulls":6},"Valve",null,"3457"]
[null,"34\"","CPVI008000","34","34","64","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","b670043c-ca7c-b97b-4619-aea71b5265a8","S1","34","in","34","BV",{"$nulls":4},"150",null,null,"0","in","a584a35d-00df-4f27-b5d6-098ab33410af","S2","34","in","34","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 34\" ND, 150 LB, BW, ASME B16.10, 64\" LG",null,null,null,"LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"64","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","20a3eb99-1e3d-5bc7-821c-77bd341b8550","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","801bc4ee-daeb-4b63-8e9a-0072064e67e2","Manual","HandLever","21","16","False",{"$nulls":6},"Valve",null,"3459"]
[null,"36\"","CPVI008000","36","36","68","0","-2","-2","0","0","0","0","-2","-2","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","57ee21fd-4c8e-cb02-7ace-97563e87ac98","S1","36","in","36","BV",{"$nulls":4},"150",null,null,"0","in","5b10fea2-7900-4831-94eb-6a021cfa4244","S2","36","in","36","BV",{"$nulls":4},"150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 36\" ND, 150 LB, BW, ASME B16.10, 68\" LG",null,null,"7683.1","LB","VBBW","VALVE","96fecf45-4c80-4bec-b5dd-ee2f41fb31ff","e107bd23-43ae-47bc-bdd9-b41b094b19cf",{"$nulls":4},"2",null,"Valves","SKEY=VBBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"68","Inline","Continuous","Ball","False","False","e107bd23-43ae-47bc-bdd9-b41b094b19cf","3a1b1fb7-eb35-5a86-b036-06139e38cdf7","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","7320d51e-92e3-4406-946b-c2677e6bf68b","Manual","HandLever","22","16","False",{"$nulls":6},"Valve",null,"3461"]

{"sheet":"PLUG VALVE","index":14,"n_rows":11,"n_cols":81,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"2\"","CPVI010000","0.01","0.01","10.5","0","2.375","2.375","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","51c6e574-2ae6-bc1c-15ab-81444269288b","ALL","2","in","2.375","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 2\" ND, 150 LB, BW, ASME B16.10, 10 1/2\" LG",null,null,"44.09","LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10.5","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","f94afb70-930e-5738-9f74-de95a5574ce7","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","6ac4b970-aa35-435b-84b4-bf5e7d2ac2b5","Manual","HandLever","6.4961","16.1417","False",{"$nulls":6},"Valve",null,"4297"]
[null,"2 1/2\"","CPVI010000","0.01","0.01","12","0","2.875","2.875","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","9fd50f1f-0411-bd75-eff8-c2a394d964b0","ALL","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 2 1/2\" ND, 150 LB, BW, ASME B16.10, 12\" LG",null,null,"66.14","LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"12","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","f6fda9e7-9153-56d0-b929-b44c742b418d","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","92178400-e304-4a42-a01e-83ad89385bb8","Manual","HandLever","7.0472","16.1417","False",{"$nulls":6},"Valve",null,"4316"]
[null,"3\"","CPVI010000","0.01","0.01","13","0","3.5","3.5","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","221ab6a1-004b-2f03-8ec4-f57a36147f7b","ALL","3","in","3.5","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 3\" ND, 150 LB, BW, ASME B16.10, 13\" LG",null,null,"88.19","LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","1816b40b-d792-5b8e-98d0-f521e7fcc0d1","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","92178400-e304-4a42-a01e-83ad89385bb8","Manual","HandLever","7.0472","16.1417","False",{"$nulls":6},"Valve",null,"4318"]
[null,"4\"","CPVI010000","0.01","0.01","14","0","4.5","4.5","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","db1e3b3d-6f6e-bb67-e096-0019c612839e","ALL","4","in","4.5","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 4\" ND, 150 LB, BW, ASME B16.10, 14\" LG",null,null,"132.28","LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","d5b429f6-2eba-5960-84d9-01082409ccbd","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","3512211a-086e-4c9d-8ec4-24b7a97db83a","Manual","HandLever","5","30","False",{"$nulls":6},"Valve",null,"4320"]
[null,"5\"","CPVI010000","0.01","0.01","15","0","5.563","5.563","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","20a65cdc-ccad-60f8-9f12-1c646798b446","ALL","5","in","5.563","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 5\" ND, 150 LB, BW, ASME B16.10, 15\" LG",null,null,null,"LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","eb8ad6e7-0c3d-568d-80e9-ddffdf65cdb4","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","40405c3d-0651-468e-a192-4946a91c87e7","Manual","HandLever","5.5","30","False",{"$nulls":6},"Valve",null,"4322"]
[null,"6\"","CPVI010000","0.01","0.01","18","0","6.625","6.625","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","45bed296-81cd-3ac8-4557-f6d9cfccfb4c","ALL","6","in","6.625","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 6\" ND, 150 LB, BW, ASME B16.10, 18\" LG",null,null,"242.51","LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","19a04aa4-528d-5f60-8308-985967f8a8b6","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b3e5a1b5-7e06-4790-a12d-60836ca245a7","Manual","HandLever","6","30","False",{"$nulls":6},"Valve",null,"4324"]
[null,"8\"","CPVI010000","0.01","0.01","20.5","0","8.625","8.625","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","301ec46e-d680-0aa1-c5bb-1bafbe16eb2f","ALL","8","in","8.625","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 8\" ND, 150 LB, BW, ASME B16.10, 20 1/2\" LG",null,null,null,"LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"20.5","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","3ef8d842-8567-5578-9858-0f4023d6259e","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","d81badf1-6af2-4061-a972-33a3924e8242","Manual","HandLever","8.7402","26.5354","False",{"$nulls":6},"Valve",null,"4326"]
[null,"10\"","CPVI010000","0.01","0.01","22","0","10.75","10.75","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","da69b6ed-304b-29dd-a8c8-0bccb99b6b7c","ALL","10","in","10.75","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 10\" ND, 150 LB, BW, ASME B16.10, 22\" LG",null,null,null,"LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","38adf83f-a5a1-57aa-9b79-dc529aa53079","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","2990e987-6c60-4251-b2a0-4e27c78dc135","Manual","HandLever","13.875","44","False",{"$nulls":6},"Valve",null,"4328"]
[null,"12\"","CPVI010000","0.01","0.01","25","0","12.75","12.75","0","0","-1","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5415c402-51ba-4bd8-f8c3-fe0e22e910d7","ALL","12","in","12.75","BV",{"$nulls":4},"150",null,null,"0","in","Plug Valve","ASME B16.10",null,"Plug Valve, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","PLUG VALVE, 12\" ND, 150 LB, BW, ASME B16.10, 25\" LG",null,null,null,"LB","VPBW","VALVE","61928f34-ba47-4031-91a1-4def97d4755f","29a0786e-9d1f-40c0-8cd7-12074e046cb4",{"$nulls":4},"2",null,"Valves","SKEY=VPBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"25","Inline","Continuous","Plug","False","False","29a0786e-9d1f-40c0-8cd7-12074e046cb4","4bdeaeae-c201-5cd1-bcf9-a03cf98d6404","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","328f39de-736a-4dd4-b79c-2f84deb1ec9c","Manual","HandLever","13.875","44","False",{"$nulls":6},"Valve",null,"4330"]

{"sheet":"BALL VALVE","index":15,"n_rows":20,"n_cols":82,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI008000","0.84","0.84","4.25","0","3.5","3.5","0","0","0","0","0.44","0.44","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","a270a1b6-1303-4a36-2858-709ef9b30579","ALL","0.5","in","0.84","FL",null,null,"RF","0.44","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 1/2\" ND, 150 LB, RF, ASME B16.10, 4 1/4\" LG",null,null,"11.02","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","5982e227-2f99-500d-924c-a3333b6c7c3a","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","351cdd93-c271-4bac-b995-050a67fdf152","Manual","HandLever","3.63","6.5","False",{"$nulls":6},"Valve",null,"3463"]
[null,"3/4\"","CPVI008000","1.05","1.05","4.62","0","3.88","3.88","0","0","0","0","0.5","0.5","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","dedec040-57e4-b446-8dfc-00990cd0c9e0","ALL","0.75","in","1.05","FL",null,null,"RF","0.5","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 3/4\" ND, 150 LB, RF, ASME B16.10, 4 31/50\" LG",null,null,"15.43","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.62","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","1a01d36e-cc2b-5c99-a4f3-50f73c1ec1f1","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","351cdd93-c271-4bac-b995-050a67fdf152","Manual","HandLever","3.63","6.5","False",{"$nulls":6},"Valve",null,"3488"]
[null,"1\"","CPVI008000","1.315","1.315","5","0","4.25","4.25","0","0","0","0","0.56","0.56","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","272cad73-654e-ab66-2643-5819fdf5eaa8","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 1\" ND, 150 LB, RF, ASME B16.10, 5\" LG",null,null,"22.04","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","6ffd1fcc-756a-55d5-b996-2337cdefb689","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","351cdd93-c271-4bac-b995-050a67fdf152","Manual","HandLever","3.63","6.5","False",{"$nulls":6},"Valve",null,"3490"]
[null,"1 1/4\"","CPVI008000","1.66","1.66","5.5","0","4.62","4.62","0","0","0","0","0.62","0.62","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","d9e12c1a-44e2-dd75-188b-071e30c71f5d","ALL","1.25","in","1.66","FL",null,null,"RF","0.62","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 1 1/4\" ND, 150 LB, RF, ASME B16.10, 5 1/2\" LG",null,null,"33.06","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","02ffd84a-c02b-5525-b19c-4993ae78a027","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","351cdd93-c271-4bac-b995-050a67fdf152","Manual","HandLever","3.63","6.5","False",{"$nulls":6},"Valve",null,"3492"]
[null,"1 1/2\"","CPVI008000","1.91","1.91","6.5","0","5","5","0","0","0","0","0.68","0.68","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","07e24526-ddce-fcb6-3525-b22b8a94c1ed","ALL","1.5","in","1.91","FL",null,null,"RF","0.68","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 6 1/2\" LG",null,null,"39.68","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","21c944fd-c72a-53c9-bc6c-1ab2d09e019d","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","351cdd93-c271-4bac-b995-050a67fdf152","Manual","HandLever","3.63","6.5","False",{"$nulls":6},"Valve",null,"3494"]
[null,"2\"","CPVI008000","2.375","2.375","7","0","6","6","0","0","0","0","0.75","0.75","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","7d9d303c-1a70-5e35-bb70-9bd376368145","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 2\" ND, 150 LB, RF, ASME B16.10, 7\" LG",null,null,"48.5","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","77404743-654b-57c6-9ff8-d9df2f5169b6","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","351cdd93-c271-4bac-b995-050a67fdf152","Manual","HandLever","3.63","6.5","False",{"$nulls":6},"Valve",null,"3496"]
[null,"2 1/2\"","CPVI008000","2.875","2.875","7.5","0","7","7","0","0","0","0","0.87","0.87","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","a0075bd4-b4d9-fd05-8167-7b3fd15e2036","ALL","2.5","in","2.875","FL",null,null,"RF","0.87","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 7 1/2\" LG",null,null,"66.13","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7.5","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","4b6e02b0-6a4b-5d53-bc8c-3cc6a90a3887","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","02c4c27f-4ae3-4bd2-9e91-ae3be54d166a","Manual","HandLever","4","6.5","False",{"$nulls":6},"Valve",null,"3498"]
[null,"3\"","CPVI008000","3.5","3.5","8","0","7.5","7.5","0","0","0","0","0.94","0.94","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","0720bc9a-3e92-d399-b222-65bdd9c348c4","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 3\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,"92.59","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","ee328d98-50c9-5561-9a54-f8361b0be0e4","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","f40acc41-aa31-4dd1-9428-c99dda8d6c23","Manual","HandLever","5.69","10.5","False",{"$nulls":6},"Valve",null,"3501"]
[null,"4\"","CPVI008000","4.5","4.5","9","0","9","9","0","0","0","0","0.94","0.94","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","c11adc3c-0058-5067-c432-1446161e16f6","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 4\" ND, 150 LB, RF, ASME B16.10, 9\" LG",null,null,"132.27","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","371bf8f5-6cb5-5d7d-877b-9b157c8165be","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","f40acc41-aa31-4dd1-9428-c99dda8d6c23","Manual","HandLever","5.69","10.5","False",{"$nulls":6},"Valve",null,"3503"]
[null,"6\"","CPVI008000","6.625","6.625","15.5","0","11","11","0","0","0","0","1","1","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","a7f386cf-925f-0ce4-252c-a61a683b41a2","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 6\" ND, 150 LB, RF, ASME B16.10, 15 1/2\" LG",null,null,"222.66","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15.5","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","da296a43-fc49-535e-a483-fcad731b3bb4","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","0b48c097-258b-4e07-99a2-75ab6e1de5a2","Manual","HandLever","7","10.5","False",{"$nulls":6},"Valve",null,"3505"]
[null,"8\"","CPVI008000","8.625","8.625","18","0","13.5","13.5","0","0","0","0","1.12","1.12","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","bac98ef1-5d93-35ea-eeb6-5cbb34209c23","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 8\" ND, 150 LB, RF, ASME B16.10, 18\" LG",null,null,"354.94","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","8061c779-0f44-5ea6-acff-96932fffddfc","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","c27da085-ef36-4e79-86d1-0af7d4ad54a7","Manual","HandLever","8.75","14","False",{"$nulls":6},"Valve",null,"3507"]
[null,"10\"","CPVI008000","10.75","10.75","21","0","16","16","0","0","0","0","1.18","1.18","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","9c5ebfdb-403c-a0b3-68ca-a7e6755100b2","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 10\" ND, 150 LB, RF, ASME B16.10, 21\" LG",null,null,"679.02","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"21","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","3bcd1617-8893-5611-883e-65faf36167f1","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ddcb694e-a0f1-411a-b499-42359fc626dc","Manual","HandLever","11.5","14","False",{"$nulls":6},"Valve",null,"3509"]
[null,"12\"","CPVI008000","12.75","12.75","24","0","19","19","0","0","0","0","1.25","1.25","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","4eb9c396-4bcb-47f8-e565-0a67c35f0bde","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 12\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,"903.89","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","62720d97-86e0-51c0-8df3-114a16799172","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","7ad52f56-e93d-4c01-9400-093773391624","Manual","HandLever","13.5","14","False",{"$nulls":6},"Valve",null,"3511"]
[null,"14\"","CPVI008000","14","14","27","0","21","21","0","0","0","0","1.37","1.37","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","7bcfe2a9-4b9f-2982-5dd1-98fd9d7bb9ea","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 14\" ND, 150 LB, RF, ASME B16.10, 27\" LG",null,null,"1344.81","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"27","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","10e445b2-ef92-5767-9801-9a9973f92464","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","9a0dc275-cb55-4643-b2f3-af5e55bae7f6","Manual","HandLever","15.25","14","False",{"$nulls":6},"Valve",null,"3513"]
[null,"16\"","CPVI008000","16","16","30","0","23.5","23.5","0","0","0","0","1.44","1.44","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","7ce5d216-51a9-ed31-b05c-593587ed1020","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 16\" ND, 150 LB, RF, ASME B16.10, 30\" LG",null,null,"1940.06","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"30","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","b165d669-b0b3-5fea-8e4c-c0da4e670188","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","4fc00a7c-91b6-4d8c-9542-a57ce77d839d","Manual","HandLever","16.25","14","False",{"$nulls":6},"Valve",null,"3515"]
[null,"18\"","CPVI008000","18","18","34","0","25","25","0","0","0","0","1.56","1.56","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","022eb110-fab2-2bcd-fafa-0109a5b764f6","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 18\" ND, 150 LB, RF, ASME B16.10, 34\" LG",null,null,"2535.31","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"34","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","4b26441b-b2a6-5340-a054-62c14caec96e","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","9b9df8f6-06f0-44a4-8291-961395f9ca60","Manual","HandLever","21.5","14","False",{"$nulls":6},"Valve",null,"3517"]
[null,"20\"","CPVI008000","20","20","36","0","27.5","27.5","0","0","0","0","1.68","1.68","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","c415bf82-7c7f-781f-9f2f-7235922af158","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 20\" ND, 150 LB, RF, ASME B16.10, 36\" LG",null,null,"3637.62","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","0cc8fad0-9ace-5ef7-9291-9a0ac5e8be53","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","9b9df8f6-06f0-44a4-8291-961395f9ca60","Manual","HandLever","21.5","14","False",{"$nulls":6},"Valve",null,"3519"]
[null,"24\"","CPVI008000","24","24","42","0","32","32","0","0","0","0","1.87","1.87","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,B1,B2,","7619be09-6353-6a2f-ee2d-5513aee50b49","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,null,"in","Ball Valve","ASME B16.10","Long Pattern","Ball Valve, Long Pattern, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BALL VALVE, LONG PATTERN, 24\" ND, 150 LB, RF, ASME B16.10, 42\" LG",null,null,"4850.16","LB","VBFL","VALVE","70a86934-9d2b-4c5e-add1-7aa8a35c6689","e5dbc98a-b669-4f2a-924e-ee4b9d272617",{"$nulls":4},"2",null,"Valves","SKEY=VBFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"42","Inline","Continuous","Ball","False","False","e5dbc98a-b669-4f2a-924e-ee4b9d272617","eb735d0a-243d-59c7-bf5e-c0ba5db59c95","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","9b9df8f6-06f0-44a4-8291-961395f9ca60","Manual","HandLever","21.5","14","False",{"$nulls":6},"Valve",null,"3521"]

{"sheet":"BUTTERFLY VALVE","index":16,"n_rows":13,"n_cols":83,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H11","H12","H21","H22","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H11","H12","H21","H22","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPVI256000","3.5","3.5","1.88","0","7.5","7.5","6.75","6.75","0","0","-1","0.94","0.94","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","e85c1f58-eec7-434b-4cc4-79cedc857ae4","ALL","3","in","3.5","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 3\" ND, 150 LB, WFR, RF, ASME B16.10, 1 22/25\" LG",null,null,"11.02","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"1.88","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","e68bb1b7-972a-5b1e-b7e3-196a1e72c758","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","14a38483-5252-44c9-b313-4af077f430a4","Manual","HandLever","7","6.5","False",{"$nulls":6},"Valve",null,"3523"]
[null,"4\"","CPVI256000","4.5","4.5","2.12","0","9","9","8.1","8.1","0","0","-1","0.94","0.94","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","50d0d4e4-c800-1b7d-a8e9-025b107dbbf8","ALL","4","in","4.5","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 4\" ND, 150 LB, WFR, RF, ASME B16.10, 2 3/25\" LG",null,null,"16.98","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.12","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","8074a538-9468-5738-a5b1-4a604e479466","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","3eafb794-44d6-4307-81eb-bfb9b676421e","Manual","HandLever","7.75","10.5","False",{"$nulls":6},"Valve",null,"3549"]
[null,"6\"","CPVI256000","6.63","6.63","2.25","0","11","11","9.9","9.9","0","0","-1","1","1","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","9e8fe78e-7738-d81b-2ee4-29875675db02","ALL","6","in","6.63","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 6\" ND, 150 LB, WFR, RF, ASME B16.10, 2 1/4\" LG",null,null,"29.98","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.25","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","fa5ab5a1-2f03-5316-83cb-48f47b002568","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5559017f-64c8-4534-a5ec-c0c8fa2b960b","Manual","HandLever","8.75","10.5","False",{"$nulls":6},"Valve",null,"3551"]
[null,"8\"","CPVI256000","8.63","8.63","2.5","0","13.5","13.5","12.15","12.15","0","0","-1","1.12","1.12","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","53759bb7-ba12-cce3-f325-b566f28fb587","ALL","8","in","8.63","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 8\" ND, 150 LB, WFR, RF, ASME B16.10, 2 1/2\" LG",null,null,"44.09","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.5","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","22905c23-5d4d-5c9e-b299-74d9bb712828","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","5a101043-71bb-43ee-b8b1-f88ffc9fd7b0","Manual","HandLever","10.25","14","False",{"$nulls":6},"Valve",null,"3553"]
[null,"10\"","CPVI256000","10.75","10.75","2.81","0","16","16","14.4","14.4","0","0","-1","1.19","1.19","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","71546a6e-8553-5bc3-cc9e-952546a83954","ALL","10","in","10.75","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 10\" ND, 150 LB, WFR, RF, ASME B16.10, 2 81/100\" LG",null,null,"70.55","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"2.81","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","e7f43be1-6d93-508e-84a6-9783c81086ff","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","ddcb694e-a0f1-411a-b499-42359fc626dc","Manual","HandLever","11.5","14","False",{"$nulls":6},"Valve",null,"3555"]
[null,"12\"","CPVI256000","12.75","12.75","3.19","0","19","19","17.1","17.1","0","0","-1","1.25","1.25","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","3607fe68-5c75-863e-34ea-3b41a3ff3433","ALL","12","in","12.75","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 12\" ND, 150 LB, WFR, RF, ASME B16.10, 3 5/25\" LG",null,null,"66.14","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"3.19","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","a021491a-2b8e-5ee7-a48e-5b810d375ddc","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","cea247f5-355c-40af-84eb-eddcd1f98df3","Manual","HandLever","13.25","14","False",{"$nulls":6},"Valve",null,"3557"]
[null,"14\"","CPVI256000","14","14","3.62","0","21","21","18.9","18.9","0","0","-1","1.38","1.38","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","c592fc47-c178-2cf4-0cbf-1c743e33e400","ALL","14","in","14","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 14\" ND, 150 LB, WFR, RF, ASME B16.10, 3 31/50\" LG",null,null,"134.48","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"3.62","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","8709fac5-64d8-5c76-822f-6570ea93daba","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","e681b696-660d-46c3-a52d-02765ba90bec","Manual","HandLever","14.5","14","False",{"$nulls":6},"Valve",null,"3559"]
[null,"16\"","CPVI256000","16","16","4","0","23.5","23.5","21.15","21.15","0","0","-1","1.44","1.44","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","261c8d2b-c479-786a-6c17-40bee985a03d","ALL","16","in","16","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 16\" ND, 150 LB, WFR, RF, ASME B16.10, 4\" LG",null,null,"182.98","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","05b49bdd-31c8-5da1-a3a6-5df9fc3d30b6","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","45730dd4-988d-48e3-978e-5de04277f5dc","Manual","HandLever","15.75","14","False",{"$nulls":6},"Valve",null,"3561"]
[null,"18\"","CPVI256000","18","18","4.5","0","25","25","22.5","22.5","0","0","-1","1.56","1.56","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","cb82cb54-4c27-8cdd-efd4-707f86d1dace","ALL","18","in","18","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 18\" ND, 150 LB, WFR, RF, ASME B16.10, 4 1/2\" LG",null,null,"233.69","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.5","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","0834b3d7-7238-59e4-8142-a05ae83634b1","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","e3817f3d-3795-461a-9d63-f89ce6a43eba","Manual","HandLever","16.5","14","False",{"$nulls":6},"Valve",null,"3563"]
[null,"20\"","CPVI256000","20","20","5","0","27.5","27.5","24.75","24.75","0","0","-1","1.69","1.69","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","28f0cfa8-5e65-183e-691e-a1a7056ffb30","ALL","20","in","20","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 20\" ND, 150 LB, WFR, RF, ASME B16.10, 5\" LG",null,null,"319.67","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","3186395f-b3b3-5b42-b8a0-387eb779227a","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","27092ef5-afd7-4ded-987f-99fce4e691cc","Manual","HandLever","18.75","14","False",{"$nulls":6},"Valve",null,"3565"]
[null,"24\"","CPVI256000","24","24","6.06","0","32","32","28.8","28.8","0","0","-1","1.88","1.88","D1,D2,L,LS,H11,H12,H21,H22,W1,W2,OF,B1,B2,","7c83aa46-889c-ab5b-0961-efedb9fc721c","ALL","24","in","24","WF",null,null,"RF",null,"150",null,null,"0","in","Butterfly Valve","ASME B16.10","Offset","Butterfly Valve, Offset, 150 LB, WFR, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Lever","BUTTERFLY VALVE, OFFSET, 24\" ND, 150 LB, WFR, RF, ASME B16.10, 6 3/50\" LG",null,null,"504.86","LB","VYFL","VALVE","faf89c2d-2bc0-45e3-a714-97b02666b9b9","2a5e2aeb-8f23-4cbf-bf90-602d468e0344",{"$nulls":4},"2",null,"Valves","SKEY=VYFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.06","Inline","Continuous","Butterfly","False","False","2a5e2aeb-8f23-4cbf-bf90-602d468e0344","592220b2-6e73-5ceb-a17a-cdf200218609","Hand Lever","dfba20f9-ae50-4ccc-aaef-796bf7a5767e","b72129de-f087-4db9-9c9b-3793a4ce05bf","Manual","HandLever","21","14","False",{"$nulls":6},"Valve",null,"3567"]

{"sheet":"CHECK VALVE","index":17,"n_rows":26,"n_cols":81,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI011000","0.84","0.84","4.25","0","0.924","0.924","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","61b6765b-3a90-44d1-9e0e-aca41588c0ac","ALL","0.5","in","0.84","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1/2\" ND, 150 LB, BW, ASME B16.10, 4 1/4\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","965c5526-e476-5373-b374-8b96b0798253",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3616"]
[null,"3/4\"","CPVI011000","1.05","1.05","4.62","0","1.155","1.155","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","116a9006-4b98-4e82-86e5-2ba3ac364ba8","ALL","0.75","in","1.05","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 3/4\" ND, 150 LB, BW, ASME B16.10, 4 31/50\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.62","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","c1651a76-e0de-59a2-8eac-12de76335fe2",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3618"]
[null,"1\"","CPVI011000","1.315","1.315","5","0","1.4465","1.4465","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e9b7a392-8c14-4c96-b17b-dfa501291e4c","ALL","1","in","1.315","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1\" ND, 150 LB, BW, ASME B16.10, 5\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","195ff15a-edb0-5904-b405-995162f2a4a3",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3620"]
[null,"1 1/4\"","CPVI011000","1.66","1.66","5.5","0","1.826","1.826","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3941acfd-a7b3-44c8-9aac-bd2d004f5d9b","ALL","1.25","in","1.66","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1 1/4\" ND, 150 LB, BW, ASME B16.10, 5 1/2\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","184f9757-8984-5ca8-b810-085194b1b285",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3622"]
[null,"1 1/2\"","CPVI011000","1.91","1.91","6.5","0","2.101","2.101","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","af0b1ebb-2e28-411f-a149-5f80b8f7d457","ALL","1.5","in","1.91","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 1 1/2\" ND, 150 LB, BW, ASME B16.10, 6 1/2\" LG",null,null,"18.74","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","d24f5ba2-4d14-53c3-8dd0-cf2b7a0cb6a6",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3624"]
[null,"2\"","CPVI011000","2.375","2.375","8","0","2.6125","2.6125","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","eb5f6674-9eba-4ae0-9513-eae09909d9e4","ALL","2","in","2.375","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 2\" ND, 150 LB, BW, ASME B16.10, 8\" LG",null,null,"26.46","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","c8eecaeb-7665-5d61-a433-cb7f894036b2",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3626"]
[null,"2 1/2\"","CPVI011000","2.875","2.875","8.5","0","3.1625","3.1625","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5b9f7b96-2614-446c-952c-335206499a5d","ALL","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 2 1/2\" ND, 150 LB, BW, ASME B16.10, 8 1/2\" LG",null,null,"37.48","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","e1b77862-577a-5c90-8dd4-e7055b4cb35d",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3628"]
[null,"3\"","CPVI011000","3.5","3.5","9.5","0","3.85","3.85","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","c78e7f5f-d848-45b1-9adc-7606b615fc1e","ALL","3","in","3.5","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 3\" ND, 150 LB, BW, ASME B16.10, 9 1/2\" LG",null,null,"39.68","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","647c05d8-7eac-58b8-bb2d-a151823a7ab2",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3630"]
[null,"4\"","CPVI011000","4.5","4.5","11.5","0","4.95","4.95","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","7a4b0aed-b3c1-4a15-8b6c-0c6aea50aabb","ALL","4","in","4.5","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 4\" ND, 150 LB, BW, ASME B16.10, 11 1/2\" LG",null,null,"70.55","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","c69b7419-a72c-59fd-9e50-2eb16c5eac3c",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3632"]
[null,"5\"","CPVI011000","5.563","5.563","13","0","6.1193","6.1193","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e831de28-011c-4e03-b6a7-d5c8189f6fd1","ALL","5","in","5.563","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 5\" ND, 150 LB, BW, ASME B16.10, 13\" LG",null,null,"125.66","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","62361518-18c7-5681-9bc5-1ca6ff1767a8",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3634"]
[null,"6\"","CPVI011000","6.625","6.625","14","0","7.2875","7.2875","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","0c143304-206e-4ed0-b9dd-3e0f4b30eaf5","ALL","6","in","6.625","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 6\" ND, 150 LB, BW, ASME B16.10, 14\" LG",null,null,"132.28","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","56e8f98c-6546-5676-a220-775c3010a6f4",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3636"]
[null,"8\"","CPVI011000","8.625","8.625","19.5","0","9.4875","9.4875","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3aa97275-4eff-4b11-8ed6-6d97f138506e","ALL","8","in","8.625","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 8\" ND, 150 LB, BW, ASME B16.10, 19 1/2\" LG",null,null,"233.69","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"19.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","2b8a7584-dda8-501e-86ef-7dc1b3b34e62",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3638"]
[null,"10\"","CPVI011000","10.75","10.75","24.5","0","11.825","11.825","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","f55300a6-bf3f-4f8b-949b-d3e4a0628906","ALL","10","in","10.75","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 10\" ND, 150 LB, BW, ASME B16.10, 24 1/2\" LG",null,null,"383.61","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","d2531486-4eeb-598f-b8f2-b798e493a153",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3640"]
[null,"12\"","CPVI011000","12.75","12.75","27.5","0","14.025","14.025","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","7b6a488d-d5b4-4c2a-ac4a-0cecc5a7367d","ALL","12","in","12.75","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 12\" ND, 150 LB, BW, ASME B16.10, 27 1/2\" LG",null,null,"568.79","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"27.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","8d046b45-8160-5404-875a-3e8093bc7961",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3642"]
[null,"14\"","CPVI011000","14","14","21","0","15.4","15.4","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","23c1b8bd-8838-4f33-a039-f93a43b2ada7","ALL","14","in","14","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 14\" ND, 150 LB, BW, ASME B16.10, 21\" LG",null,null,"811.3","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"21","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","ddca389b-3ff9-54c0-a31f-754adb70f469",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3644"]
[null,"16\"","CPVI011000","16","16","36","0","17.6","17.6","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","ce93344e-be94-41bc-a399-6d4069b2d0f9","ALL","16","in","16","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 16\" ND, 150 LB, BW, ASME B16.10, 36\" LG",null,null,"1064.83","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","ff7ea3df-3d7e-5eb9-b4a1-1c9fc96dac27",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3646"]
[null,"18\"","CPVI011000","18","18","38.5","0","19.8","19.8","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","dda11374-ca00-4e8f-9cc4-99369ad4f990","ALL","18","in","18","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 18\" ND, 150 LB, BW, ASME B16.10, 38 1/2\" LG",null,null,"1510.17","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"38.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","3c9e088c-e1f3-5421-b873-51d0a8bda649",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3648"]
[null,"20\"","CPVI011000","20","20","38.5","0","22","22","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e9300fe7-6f67-4984-b1ac-45409e4330e1","ALL","20","in","20","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 20\" ND, 150 LB, BW, ASME B16.10, 38 1/2\" LG",null,null,"1587.33","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"38.5","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","c4866e06-4346-545a-96a0-64a144e35571",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3650"]
[null,"22\"","CPVI011000","22","22","42","0","24.2","24.2","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","51afbe15-c0c1-47fc-bad6-1eec5f8c4dc2","ALL","22","in","22","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 22\" ND, 150 LB, BW, ASME B16.10, 42\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"42","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","8d6b286d-67ec-5b18-89f9-3fed42b41d81",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3652"]
[null,"24\"","CPVI011000","24","24","51","0","26.4","26.4","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","6f83604b-9a84-44a8-ad51-95961c61a496","ALL","24","in","24","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 24\" ND, 150 LB, BW, ASME B16.10, 51\" LG",null,null,"2535.31","LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"51","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","82e5bbf9-c074-5bb6-9a91-29098425dc98",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3654"]
[null,"26\"","CPVI011000","26","26","51","0","28.6","28.6","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","1e1c22cd-dc52-494b-9fca-515e997e2887","ALL","26","in","26","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 26\" ND, 150 LB, BW, ASME B16.10, 51\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"51","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","1bb807c7-cd87-5439-932e-1c0384c71d3a",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3656"]
[null,"28\"","CPVI011000","28","28","57","0","30.8","30.8","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","68bd4df4-fc6d-4436-acd4-249c72d3b931","ALL","28","in","28","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 28\" ND, 150 LB, BW, ASME B16.10, 57\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"57","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","550f7d0a-7a14-5ad7-94b6-456c7684ed1b",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3658"]
[null,"30\"","CPVI011000","30","30","60","0","33","33","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d2811cce-5d26-4c05-aff3-096034b681eb","ALL","30","in","30","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 30\" ND, 150 LB, BW, ASME B16.10, 60\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"60","Inline","Continuous","Check","True","False","06b4e43f-ad2b-4236-b86e-e562945be75d","2830fb8e-981c-5441-ac98-db275bad8c2b",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3660"]
[null,"36\"","CPVI011000","36","36","77","0","39.6","39.6","0","0","-1","0.01","0.01","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3acdff50-5ab2-44b2-92ef-f6e2405efef0","ALL","36","in","36","BV",{"$nulls":4},"150",null,null,"0","in","Check Valve","ASME B16.10","Swing","Check Valve, Swing, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB","CHECK VALVE, SWING, 36\" ND, 150 LB, BW, ASME B16.10, 77\" LG",null,null,null,"LB","VCBW","VALVE","d2910329-36da-45a7-a843-4ab586123f71","06b4e43f-ad2b-4236-b86e-e562945be75d",{"$nulls":4},"2",null,"Valves","SKEY=VCBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"77","Inline","Continuous","Check","False","False","06b4e43f-ad2b-4236-b86e-e562945be75d","40623c36-9cf4-5200-9092-87dc213dc417",{"$nulls":7},"False",{"$nulls":6},"Valve",null,"3662"]

{"sheet":"GLOBE VALVE","index":18,"n_rows":8,"n_cols":86,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","D3","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI004000_OFOF","0.84","0.84","4.25","0","-2","-2","1.4",null,null,"0","0.594","0.594","0.54","0.54","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","217c1079-ef10-95c0-cdcf-c088f9d37f2f","ALL","0.5","in","0.84","SW",{"$nulls":4},"150",null,null,"0.54","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1/2\" ND, 150 LB, SW, ASME B16.10, 4 1/4\" LG",{"$nulls":4},"VGSW","VALVE","faa59825-7322-464f-9251-819b96f19d1b","ae416669-2277-41ed-9ed0-c9d1fbb9a824",{"$nulls":4},"2",null,"Valves","SKEY=VGSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Globe","False","False","ae416669-2277-41ed-9ed0-c9d1fbb9a824","57ace688-9f50-5e47-9ee9-b5e1df6024ce","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4132"]
[null,"3/4\"","CPVI004000_OFOF","1.05","1.05","4.625","0","-2","-2","1.552",null,null,"0","0.605","0.605","0.55","0.55","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","641b02de-9699-e457-90ca-f272772f526c","ALL","0.75","in","1.05","SW",{"$nulls":4},"150",null,null,"0.55","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 3/4\" ND, 150 LB, SW, ASME B16.10, 4 5/8\" LG",{"$nulls":4},"VGSW","VALVE","faa59825-7322-464f-9251-819b96f19d1b","ae416669-2277-41ed-9ed0-c9d1fbb9a824",{"$nulls":4},"2",null,"Valves","SKEY=VGSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.625","Inline","Continuous","Globe","False","False","ae416669-2277-41ed-9ed0-c9d1fbb9a824","edf72178-4110-5e77-a902-f21b8394dc83","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4136"]
[null,"1\"","CPVI004000_OFOF","1.315","1.315","5","0","-2","-2","1.7",null,null,"0","0.759","0.759","0.69","0.69","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","37d02e6c-1baf-b01d-2abf-40bd18569478","ALL","1","in","1.315","SW",{"$nulls":4},"150",null,null,"0.69","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1\" ND, 150 LB, SW, ASME B16.10, 5\" LG",{"$nulls":4},"VGSW","VALVE","faa59825-7322-464f-9251-819b96f19d1b","ae416669-2277-41ed-9ed0-c9d1fbb9a824",{"$nulls":4},"2",null,"Valves","SKEY=VGSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Globe","False","False","ae416669-2277-41ed-9ed0-c9d1fbb9a824","df287683-49d1-5b0a-8bd8-827dbcacf5c6","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4138"]
[null,"1 1/4\"","CPVI004000_OFOF","1.66","1.66","5.5","0","-2","-2","1.848",null,null,"0","0.781","0.781","0.71","0.71","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","8bf92ff2-11c1-06c1-014f-4e1bac4e9c2d","ALL","1.25","in","1.66","SW",{"$nulls":4},"150",null,null,"0.71","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1 1/4\" ND, 150 LB, SW, ASME B16.10, 5 1/2\" LG",{"$nulls":4},"VGSW","VALVE","faa59825-7322-464f-9251-819b96f19d1b","ae416669-2277-41ed-9ed0-c9d1fbb9a824",{"$nulls":4},"2",null,"Valves","SKEY=VGSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Globe","False","False","ae416669-2277-41ed-9ed0-c9d1fbb9a824","7ab43098-99cb-5a2f-be61-be4f688aca63","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4140"]
[null,"1 1/2\"","CPVI004000_OFOF","1.91","1.91","6.5","0","-2","-2","2",null,null,"0","0.803","0.803","0.73","0.73","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","050f961c-784c-e387-6c5f-ea8b666e5f6c","ALL","1.5","in","1.91","SW",{"$nulls":4},"150",null,null,"0.73","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 1 1/2\" ND, 150 LB, SW, ASME B16.10, 6 1/2\" LG",{"$nulls":4},"VGSW","VALVE","faa59825-7322-464f-9251-819b96f19d1b","ae416669-2277-41ed-9ed0-c9d1fbb9a824",{"$nulls":4},"2",null,"Valves","SKEY=VGSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Globe","False","False","ae416669-2277-41ed-9ed0-c9d1fbb9a824","ed5b94ca-c4af-59a8-a6cf-b3e0dbc7732f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4142"]
[null,"2\"","CPVI004000_OFOF","2.375","2.375","8","0","-2","-2","2.4",null,null,"0","0.836","0.836","0.76","0.76","0","0","D1,D2,L,LS,H1,H2,D3,W1,W2,OF,L1,L2,I1,I2,B1,B2,","060d26e4-3c1f-f343-1e88-d9eec76441f7","ALL","2","in","2.375","SW",{"$nulls":4},"150",null,null,"0.76","in","Globe Valve","ASME B16.10",null,"Globe Valve, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GLOBE VALVE, 2\" ND, 150 LB, SW, ASME B16.10, 8\" LG",{"$nulls":4},"VGSW","VALVE","faa59825-7322-464f-9251-819b96f19d1b","ae416669-2277-41ed-9ed0-c9d1fbb9a824",{"$nulls":4},"2",null,"Valves","SKEY=VGSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Globe","False","False","ae416669-2277-41ed-9ed0-c9d1fbb9a824","244069a3-c771-5851-9473-7452d1ad9e94","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7779af35-d169-432a-a897-31b7b304b299","Manual","HandWheel","16.25","11.75","False",{"$nulls":6},"Valve",null,"4144"]

{"sheet":"GATE VALVE_3","index":19,"n_rows":26,"n_cols":81,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI001000","0.84","0.84","4.25","0","0.84","0.84","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","14589163-b184-f1f5-6f1d-6cb81342edbe","ALL","0.5","in","0.84","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1/2\" ND, 150 LB, BW, ASME B16.10, 4 1/4\" LG",null,null,"8.81","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","47f2a6b2-bd13-557f-86e1-03bc7e7b086b","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3711"]
[null,"3/4\"","CPVI001000","1.05","1.05","4.625","0","1.05","1.05","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","edd3113c-15c7-627a-2570-6279aee656a9","ALL","0.75","in","1.05","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 3/4\" ND, 150 LB, BW, ASME B16.10, 4 5/8\" LG",null,null,"11.02","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.625","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","96e52b93-ae8b-57a9-af26-c61c5352358f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3749"]
[null,"1\"","CPVI001000","1.315","1.315","5","0","1.315","1.315","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b9757a57-472a-abec-aac6-fa4279f375b6","ALL","1","in","1.315","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1\" ND, 150 LB, BW, ASME B16.10, 5\" LG",null,null,"17.63","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","d1921699-d8b8-55e7-8d99-2903f165ec96","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3751"]
[null,"1 1/4\"","CPVI001000","1.66","1.66","5.5","0","1.66","1.66","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","883ab7ac-7864-e865-871c-f1508034793e","ALL","1.25","in","1.66","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1 1/4\" ND, 150 LB, BW, ASME B16.10, 5 1/2\" LG",null,null,"26.45","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","380dc069-027f-5d8f-8d5c-6e1d81fceb06","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3753"]
[null,"1 1/2\"","CPVI001000","1.91","1.91","6.5","0","1.91","1.91","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","449bc88c-7522-b145-43d0-acb599e410c1","ALL","1.5","in","1.91","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 1 1/2\" ND, 150 LB, BW, ASME B16.10, 6 1/2\" LG",null,null,"33.06","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","f6c1bd59-8a02-51e4-8cee-9b7457b50bde","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3755"]
[null,"2\"","CPVI001000","2.375","2.375","8.5","0","2.375","2.375","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","9e6b1900-e069-aba7-0185-55807b581798","ALL","2","in","2.375","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 2\" ND, 150 LB, BW, ASME B16.10, 8 1/2\" LG",null,null,"33.06","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","18bb23b0-cd86-52c5-b8d2-5a274b15e56a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3757"]
[null,"2 1/2\"","CPVI001000","2.875","2.875","9.5","0","2.875","2.875","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","a12ed0b9-e385-5efe-ed54-c22d37bcad25","ALL","2.5","in","2.875","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 2 1/2\" ND, 150 LB, BW, ASME B16.10, 9 1/2\" LG",null,null,"50.7","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9.5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","622da1a6-6ac4-5b1b-ab1c-1e319c3c9462","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3759"]
[null,"3\"","CPVI001000","3.5","3.5","11.12","0","3.5","3.5","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","2eb910a6-7dca-88d6-13fb-87b86e89697d","ALL","3","in","3.5","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 3\" ND, 150 LB, BW, ASME B16.10, 11 3/25\" LG",null,null,"61.72","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.12","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","759f224f-293a-5de5-b60b-662887a2b52d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","Manual","HandWheel","21.75","11.75","False",{"$nulls":6},"Valve",null,"3761"]
[null,"4\"","CPVI001000","4.5","4.5","12","0","4.5","4.5","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","9bda4250-7227-4144-a5db-3615cf5b839a","ALL","4","in","4.5","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 4\" ND, 150 LB, BW, ASME B16.10, 12\" LG",null,null,"97","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"12","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","d69f6f39-1bf4-5ecf-9f2b-72d74fde93da","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","Manual","HandWheel","27","11.75","False",{"$nulls":6},"Valve",null,"3763"]
[null,"6\"","CPVI001000","6.625","6.625","15.88","0","6.625","6.625","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","cc637314-79f7-6256-0ac4-89b0e1bdeb1a","ALL","6","in","6.625","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 6\" ND, 150 LB, BW, ASME B16.10, 15 22/25\" LG",null,null,"163.14","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15.88","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","19155f22-9f3a-542d-aa9f-21cbe1cb6a70","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7f821266-6705-432f-9d82-62fb1dc61b9b","Manual","HandWheel","33.25","15.75","False",{"$nulls":6},"Valve",null,"3765"]
[null,"8\"","CPVI001000","8.625","8.625","16.5","0","8.625","8.625","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","8fb5e375-dfea-1dd7-2d6a-293f3a5c6f26","ALL","8","in","8.625","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 8\" ND, 150 LB, BW, ASME B16.10, 16 1/2\" LG",null,null,"268.96","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"16.5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","1358f7fc-56b6-564d-8d90-8c99120b9f26","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f9150dd-0ada-454c-a5a8-f02b683b4441","Manual","HandWheel","42","19.5","False",{"$nulls":6},"Valve",null,"3767"]
[null,"10\"","CPVI001000","10.75","10.75","18","0","10.75","10.75","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","2ec1a380-f21f-612e-9bcc-4526806777d1","ALL","10","in","10.75","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 10\" ND, 150 LB, BW, ASME B16.10, 18\" LG",null,null,"368.17","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","0fb78ff0-0829-50d8-9665-b3301894368e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","af90cd55-9525-410b-b2b6-c67760d26276","Manual","HandWheel","49.75","23.5","False",{"$nulls":6},"Valve",null,"3769"]
[null,"12\"","CPVI001000","12.75","12.75","19.75","0","12.75","12.75","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3e3278b5-e3c1-32f4-2a6d-5eb996ba501e","ALL","12","in","12.75","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 12\" ND, 150 LB, BW, ASME B16.10, 19 3/4\" LG",null,null,"557.76","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"19.75","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","d1ac8ff9-b236-5245-ab7a-ba44033bd4b4","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","Manual","HandWheel","56.75","23.5","False",{"$nulls":6},"Valve",null,"3771"]
[null,"14\"","CPVI001000","14","14","22.5","0","14","14","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","deb922b8-73e2-035e-128d-a8c4a72089b7","ALL","14","in","14","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 14\" ND, 150 LB, BW, ASME B16.10, 22 1/2\" LG",null,null,"760.59","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22.5","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","c636fa8b-02bb-5be9-95e3-fa875aa8207b","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","95186260-05ab-4f34-9f3b-a9e4661430dd","Manual","HandWheel","66.5","31.5","False",{"$nulls":6},"Valve",null,"3773"]
[null,"16\"","CPVI001000","16","16","24","0","16","16","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","1c3aefd7-1fcf-f61d-9a75-f01efe43f284","ALL","16","in","16","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 16\" ND, 150 LB, BW, ASME B16.10, 24\" LG",null,null,"981.05","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","44ff9f65-88da-5280-94e9-6eaf47942069","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","e7b757cd-087d-47b7-9775-a17b2e752794","Manual","HandWheel","73.25","31.5","False",{"$nulls":6},"Valve",null,"3775"]
[null,"18\"","CPVI001000","18","18","26","0","18","18","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","09cc1cf7-65dc-4b8e-14c9-d60ba73f5254","ALL","18","in","18","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 18\" ND, 150 LB, BW, ASME B16.10, 26\" LG",null,null,"1349.22","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"26","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","ae5b543a-a5a4-5652-8e5b-872a2a1ff6be","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","ea29d9dc-eac3-422f-8b07-2a851d4650c6","Manual","HandWheel","82","43.25","False",{"$nulls":6},"Valve",null,"3777"]
[null,"20\"","CPVI001000","20","20","28","0","20","20","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","6969f92d-4c43-76fd-c4a9-27396e7caea2","ALL","20","in","20","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 20\" ND, 150 LB, BW, ASME B16.10, 28\" LG",null,null,"2092.18","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"28","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","0810f934-1608-5b6c-ac56-b5530e0f2ded","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","60165ae9-ac00-4b7f-bd73-40e4094b7ace","Manual","HandWheel","92","43.25","False",{"$nulls":6},"Valve",null,"3779"]
[null,"24\"","CPVI001000","24","24","32","0","24","24","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","34f7f569-33a3-2264-44d0-6815208c3138","ALL","24","in","24","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 24\" ND, 150 LB, BW, ASME B16.10, 32\" LG",null,null,"2746.95","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"32","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","79fd4a7d-07cd-5eee-b07a-5c5312f4c642","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","879658da-2bb0-4344-a874-3edf9988d3e0","Manual","HandWheel","107.5","78.5","False",{"$nulls":6},"Valve",null,"3781"]
[null,"26\"","CPVI001000","26","26","34","0","26","26","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","6785589e-5a6c-0641-1625-dd3066e739ab","ALL","26","in","26","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 26\" ND, 150 LB, BW, ASME B16.10, 34\" LG",null,null,"3183.47","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"34","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","df955bf1-698c-5db5-8d76-ac4400bddfb9","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1df90dcc-8aed-4df7-9625-1161fe156ec4","Manual","HandWheel","115.5","78.5","False",{"$nulls":6},"Valve",null,"3783"]
[null,"28\"","CPVI001000","28","28","36","0","28","28","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","32dd8256-e040-6ebf-5ff1-f966f63e88df","ALL","28","in","28","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 28\" ND, 150 LB, BW, ASME B16.10, 36\" LG",null,null,"3617.78","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","646ccac0-23cc-5808-bc6e-c379d2319fde","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f967a14-50de-418a-9806-0f90316e6e17","Manual","HandWheel","133.5","78.5","False",{"$nulls":6},"Valve",null,"3785"]
[null,"30\"","CPVI001000","30","30","36","0","30","30","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","37653f8c-1007-7430-94ed-c9a3831594fc","ALL","30","in","30","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 30\" ND, 150 LB, BW, ASME B16.10, 36\" LG",null,null,"4459.94","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"36","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","a9f73c0b-a7f2-58cd-9b95-93fb7fdb41b7","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","3aca9ba6-cada-4b93-998b-9ae0d21028fd","Manual","HandWheel","131","78.5","False",{"$nulls":6},"Valve",null,"3787"]
[null,"32\"","CPVI001000","32","32","38","0","32","32","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e5fa37aa-561d-3ffe-1073-a5867b556753","ALL","32","in","32","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 32\" ND, 150 LB, BW, ASME B16.10, 38\" LG",null,null,null,"LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"38","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","c0c662e5-ebd1-5755-ac14-9c6d6e36f157","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","aab3b7da-7cee-42c1-b7cc-ede34fcd62c3","Manual","HandWheel","148","78.5","False",{"$nulls":6},"Valve",null,"3789"]
[null,"34\"","CPVI001000","34","34","40","0","34","34","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","8deddd2f-1f80-79f7-4658-50894c345900","ALL","34","in","34","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 34\" ND, 150 LB, BW, ASME B16.10, 40\" LG",null,null,null,"LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"40","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","dc1a18ee-1876-5063-80f4-53da3f7ed989","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","23d3e45c-5718-406d-9b1d-96f1951e80a5","Manual","HandWheel","140","36","False",{"$nulls":6},"Valve",null,"3791"]
[null,"36\"","CPVI001000","36","36","40","0","36","36","0","0","0","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","f346e66b-f6e9-4af3-5290-54ce5d7ed9cd","ALL","36","in","36","BV",{"$nulls":4},"150",null,null,"0","in","Gate Valve","ASME B16.10","Double Disc","Gate Valve, Double Disc, 150 LB, BW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, DOUBLE DISC, 36\" ND, 150 LB, BW, ASME B16.10, 40\" LG",null,null,"6746.13","LB","VTBW","VALVE","3633db1e-e076-4d51-8ed5-dbc6fbec4970","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f",{"$nulls":4},"2",null,"Valves","SKEY=VTBW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"40","Inline","Continuous","Gate","False","False","dd0fdc17-1bbc-4955-9bbb-45439e7ad83f","20c71bb6-4d77-5ad0-8b7b-760af585f92f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","50447195-3edf-4ced-9e1b-299b3b6464e1","Manual","HandWheel","166","78.5","False",{"$nulls":6},"Valve",null,"3793"]

{"sheet":"GATE VALVE_2","index":20,"n_rows":24,"n_cols":81,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI001000","0.84","0.84","4.25","0","3.5","3.5","0","0","0","0.44","0.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","377b1ced-fcf3-2eab-6b06-99c46067a026","ALL","0.5","in","0.84","FL",null,null,"RF","0.44","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1/2\" ND, 150 LB, RF, ASME B16.10, 4 1/4\" LG",null,null,null,"LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","e8695c1f-536e-55f8-9931-a5c41ea23cd1","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3876"]
[null,"3/4\"","CPVI001000","1.05","1.05","4.62","0","3.88","3.88","0","0","0","0.5","0.5","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e54864fd-91e7-5a9f-87b5-8554483e6daa","ALL","0.75","in","1.05","FL",null,null,"RF","0.5","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 3/4\" ND, 150 LB, RF, ASME B16.10, 4 31/50\" LG",null,null,null,"LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.62","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","9e2ca64d-b574-51b8-ab6c-2ac31b8f1bc0","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3915"]
[null,"1\"","CPVI001000","1.315","1.315","5","0","4.25","4.25","0","0","0","0.56","0.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","3a98a813-8a21-81c0-ada0-f7b6de6d12e7","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1\" ND, 150 LB, RF, ASME B16.10, 5\" LG",null,null,"14","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","4484075e-af24-5884-a1a5-5db87673a4a8","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3917"]
[null,"1 1/4\"","CPVI001000","1.66","1.66","5.5","0","4.62","4.62","0","0","0","0.62","0.62","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","93fc1cc5-7026-7db1-74eb-4edec679d8e9","ALL","1.25","in","1.66","FL",null,null,"RF","0.62","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/4\" ND, 150 LB, RF, ASME B16.10, 5 1/2\" LG",null,null,null,"LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","c12dbef6-dbbd-5cd4-83ab-a36c748c6f41","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3919"]
[null,"1 1/2\"","CPVI001000","1.91","1.91","6.5","0","5","5","0","0","0","0.68","0.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","d831a2dd-ddcf-e316-658b-84f0bf3d54f2","ALL","1.5","in","1.91","FL",null,null,"RF","0.68","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/2\" ND, 150 LB, RF, ASME B16.10, 6 1/2\" LG",null,null,"25","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","c9e50fa0-5e7c-50f2-b05d-92a06433a2ae","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3921"]
[null,"2\"","CPVI001000","2.375","2.375","7","0","6","6","0","0","0","0.75","0.75","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","27f0879e-a66c-3114-d69b-1d0c798a0eac","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 2\" ND, 150 LB, RF, ASME B16.10, 7\" LG",null,null,"35","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","63eaf1a7-29e9-5739-af6d-e23fc1a9cb53","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3923"]
[null,"2 1/2\"","CPVI001000","2.875","2.875","7.5","0","7","7","0","0","0","0.87","0.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","91adb775-5a42-8bd2-5bcb-6f2f16df6b5b","ALL","2.5","in","2.875","FL",null,null,"RF","0.87","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 2 1/2\" ND, 150 LB, RF, ASME B16.10, 7 1/2\" LG",null,null,"50","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"7.5","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","9c3291cf-3313-590e-891d-183fc746f66a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"3925"]
[null,"3\"","CPVI001000","3.5","3.5","8","0","7.5","7.5","0","0","0","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","fe14804b-f90b-7f9d-0aeb-67a2a2b2675d","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 3\" ND, 150 LB, RF, ASME B16.10, 8\" LG",null,null,"80","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","d27965aa-4005-5df9-98c9-3da3abce26db","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","706b48a3-a23b-4b4c-89a3-95e5f4f31fed","Manual","HandWheel","21.75","11.75","False",{"$nulls":6},"Valve",null,"3927"]
[null,"4\"","CPVI001000","4.5","4.5","9","0","9","9","0","0","0","0.94","0.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","807d511e-7a9c-0d36-ba13-5f41a9ab029d","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 4\" ND, 150 LB, RF, ASME B16.10, 9\" LG",null,null,"110","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"9","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","b2b61bdf-b459-5539-93e0-4ca3ac313f81","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","a8e6aee1-8df3-4ff1-86b8-74c1eea1daab","Manual","HandWheel","27","11.75","False",{"$nulls":6},"Valve",null,"3929"]
[null,"6\"","CPVI001000","6.625","6.625","10.5","0","11","11","0","0","0","1","1","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5f5de6f2-c6c6-8809-83cc-ecaa48e136da","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 6\" ND, 150 LB, RF, ASME B16.10, 10 1/2\" LG",null,null,"190","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"10.5","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","0850b788-8d9e-5cf3-96ff-61e44c43810e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","7f821266-6705-432f-9d82-62fb1dc61b9b","Manual","HandWheel","33.25","15.75","False",{"$nulls":6},"Valve",null,"3931"]
[null,"8\"","CPVI001000","8.625","8.625","11.5","0","13.5","13.5","0","0","0","1.12","1.12","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","0d3842e3-78ac-3737-a7b2-813d60bd1606","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 8\" ND, 150 LB, RF, ASME B16.10, 11 1/2\" LG",null,null,"310","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"11.5","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","0698f67e-d03b-5cf8-8d38-c61090f85af3","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f9150dd-0ada-454c-a5a8-f02b683b4441","Manual","HandWheel","42","19.5","False",{"$nulls":6},"Valve",null,"3933"]
[null,"10\"","CPVI001000","10.75","10.75","13","0","16","16","0","0","0","1.18","1.18","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","bb040c32-6b5d-d3ac-7c97-6aca89bed33b","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 10\" ND, 150 LB, RF, ASME B16.10, 13\" LG",null,null,"490","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"13","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","2a7095b1-9310-598e-a8bb-1b2a5d56dd45","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","af90cd55-9525-410b-b2b6-c67760d26276","Manual","HandWheel","49.75","23.5","False",{"$nulls":6},"Valve",null,"3935"]
[null,"12\"","CPVI001000","12.75","12.75","14","0","19","19","0","0","0","1.25","1.25","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5b59245b-6063-ea32-888f-b980d8b1e832","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 12\" ND, 150 LB, RF, ASME B16.10, 14\" LG",null,null,"700","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"14","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","3c908752-f8b8-5081-9839-eb357132c65f","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","81f07c98-bf1a-4705-9e04-8c8d2b5b0766","Manual","HandWheel","56.75","23.5","False",{"$nulls":6},"Valve",null,"3937"]
[null,"14\"","CPVI001000","14","14","15","0","21","21","0","0","0","1.37","1.37","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","eb6587e8-6947-a364-3089-2a3bd119e34f","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 14\" ND, 150 LB, RF, ASME B16.10, 15\" LG",null,null,"990","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"15","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","28a7d6e1-4cd1-5109-a5f7-1e6b65def4f3","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","95186260-05ab-4f34-9f3b-a9e4661430dd","Manual","HandWheel","66.5","31.5","False",{"$nulls":6},"Valve",null,"3939"]
[null,"16\"","CPVI001000","16","16","16","0","23.5","23.5","0","0","0","1.44","1.44","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b7b5971b-1a06-29b9-c490-94ed40a9b5d1","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 16\" ND, 150 LB, RF, ASME B16.10, 16\" LG",null,null,"1385","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"16","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","d312b3cb-5d55-5c4b-9fdc-7ad482c97bc8","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","e7b757cd-087d-47b7-9775-a17b2e752794","Manual","HandWheel","73.25","31.5","False",{"$nulls":6},"Valve",null,"3941"]
[null,"18\"","CPVI001000","18","18","17","0","25","25","0","0","0","1.56","1.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","5a6c93e5-b9ce-3719-8ccf-eb1a7b911925","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 18\" ND, 150 LB, RF, ASME B16.10, 17\" LG",null,null,"1810","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"17","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","a8792353-1225-53aa-84c9-19bedaea032a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","ea29d9dc-eac3-422f-8b07-2a851d4650c6","Manual","HandWheel","82","43.25","False",{"$nulls":6},"Valve",null,"3943"]
[null,"20\"","CPVI001000","20","20","18","0","27.5","27.5","0","0","0","1.68","1.68","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","2e3b1037-76a4-c0c4-4541-b0cf55d5e348","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 20\" ND, 150 LB, RF, ASME B16.10, 18\" LG",null,null,"2150","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"18","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","19ea0cde-975e-5d6c-ba37-843e4ede9419","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","60165ae9-ac00-4b7f-bd73-40e4094b7ace","Manual","HandWheel","92","43.25","False",{"$nulls":6},"Valve",null,"3945"]
[null,"24\"","CPVI001000","24","24","20","0","32","32","0","0","0","1.87","1.87","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","4950a80b-75d0-5eb0-a685-be14e3cc95ad","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 24\" ND, 150 LB, RF, ASME B16.10, 20\" LG",null,null,"3260","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"20","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","1d6da1f3-f0a7-5135-bd7f-e215de6d4459","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","879658da-2bb0-4344-a874-3edf9988d3e0","Manual","HandWheel","107.5","78.5","False",{"$nulls":6},"Valve",null,"3947"]
[null,"26\"","CPVI001000","26","26","22","0","34.25","34.25","0","0","0","2.69","2.69","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","62eb5b96-0316-54b0-d411-d4da6c0d26f4","ALL","26","in","26","FL",null,null,"RF","2.69","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 26\" ND, 150 LB, RF, ASME B16.10, 22\" LG",null,null,null,"LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"22","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","5f6ecb09-4a7e-5373-bfbf-ecacd23275e4","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1df90dcc-8aed-4df7-9625-1161fe156ec4","Manual","HandWheel","115.5","78.5","False",{"$nulls":6},"Valve",null,"3949"]
[null,"28\"","CPVI001000","28","28","24","0","36.5","36.5","0","0","0","2.81","2.81","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","b9d705b2-eb93-ebb8-445b-a880709c9434","ALL","28","in","28","FL",null,null,"RF","2.81","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 28\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,null,"LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","2f19afaa-5c94-5d47-8e15-f19e950db379","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","1f967a14-50de-418a-9806-0f90316e6e17","Manual","HandWheel","133.5","78.5","False",{"$nulls":6},"Valve",null,"3951"]
[null,"30\"","CPVI001000","30","30","24","0","38.75","38.75","0","0","0","2.94","2.94","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","bb2181fd-881a-6198-9194-a0cc29dbe1be","ALL","30","in","30","FL",null,null,"RF","2.94","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 30\" ND, 150 LB, RF, ASME B16.10, 24\" LG",null,null,"5310","LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"24","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","f842f6d1-87ca-5c97-82ab-3b8df756dc0c","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","3aca9ba6-cada-4b93-998b-9ae0d21028fd","Manual","HandWheel","131","78.5","False",{"$nulls":6},"Valve",null,"3953"]
[null,"36\"","CPVI001000","36","36","28","0","46","46","0","0","0","3.56","3.56","D1,D2,L,LS,H1,H2,W1,W2,OF,B1,B2,","e0774b7e-efef-6048-e60b-d06b91988b75","ALL","36","in","36","FL",null,null,"RF","3.56","150",null,null,"0","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, RF, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 36\" ND, 150 LB, RF, ASME B16.10, 28\" LG",null,null,null,"LB","VTFL","VALVE","9ecf511c-e45d-416f-9b4c-06ca21cd1a91","38fd3054-b9d1-4dfa-a960-a7ab236625ef",{"$nulls":4},"2",null,"Valves","SKEY=VTFL,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"28","Inline","Continuous","Gate","False","False","38fd3054-b9d1-4dfa-a960-a7ab236625ef","da3dd140-8846-5d25-b035-721bfb927a64","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","50447195-3edf-4ced-9e1b-299b3b6464e1","Manual","HandWheel","166","78.5","False",{"$nulls":6},"Valve",null,"3955"]

{"sheet":"GATE VALVE_1","index":21,"n_rows":8,"n_cols":85,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI001000_OFOF","0.84","0.84","4.25","0","-2","-2",null,null,"0","0.594","0.594","0.54","0.54","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","fa2681bd-853b-63f3-9aab-7d0df9de4542","ALL","0.5","in","0.84","THDF",{"$nulls":4},"150",null,null,"0.54","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1/2\" ND, 150 LB, FPT, ASME B16.10, 4 1/4\" LG",{"$nulls":4},"VTSC","VALVE","f5c19a0e-ea24-477b-b687-fbf3172c4178","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942",{"$nulls":4},"2",null,"Valves","SKEY=VTSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Gate","False","False","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942","4efd1fcf-b53d-5656-a42f-b990756b1bed","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4030"]
[null,"3/4\"","CPVI001000_OFOF","1.05","1.05","4.625","0","-2","-2",null,null,"0","0.605","0.605","0.55","0.55","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","88404621-6f9c-e7d4-5907-db1ea290ea53","ALL","0.75","in","1.05","THDF",{"$nulls":4},"150",null,null,"0.55","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 3/4\" ND, 150 LB, FPT, ASME B16.10, 4 5/8\" LG",{"$nulls":4},"VTSC","VALVE","f5c19a0e-ea24-477b-b687-fbf3172c4178","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942",{"$nulls":4},"2",null,"Valves","SKEY=VTSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.625","Inline","Continuous","Gate","False","False","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942","3cc9ec07-37e4-5b55-b28c-3177f151de8a","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4034"]
[null,"1\"","CPVI001000_OFOF","1.315","1.315","5","0","-2","-2",null,null,"0","0.759","0.759","0.69","0.69","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","565dda20-821a-dd65-b026-e9df2cc3c9b7","ALL","1","in","1.315","THDF",{"$nulls":4},"150",null,null,"0.69","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1\" ND, 150 LB, FPT, ASME B16.10, 5\" LG",{"$nulls":4},"VTSC","VALVE","f5c19a0e-ea24-477b-b687-fbf3172c4178","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942",{"$nulls":4},"2",null,"Valves","SKEY=VTSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Gate","False","False","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942","f5a3c0f6-968f-5c58-abef-1dcf2dc2845e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4036"]
[null,"1 1/4\"","CPVI001000_OFOF","1.66","1.66","5.5","0","-2","-2",null,null,"0","0.781","0.781","0.71","0.71","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","2f55d919-f3a5-601b-f5cd-36f060bcf8f9","ALL","1.25","in","1.66","THDF",{"$nulls":4},"150",null,null,"0.71","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/4\" ND, 150 LB, FPT, ASME B16.10, 5 1/2\" LG",{"$nulls":4},"VTSC","VALVE","f5c19a0e-ea24-477b-b687-fbf3172c4178","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942",{"$nulls":4},"2",null,"Valves","SKEY=VTSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Gate","False","False","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942","73533ab0-1696-51c1-ba12-be64eb7b261d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4038"]
[null,"1 1/2\"","CPVI001000_OFOF","1.91","1.91","6.5","0","-2","-2",null,null,"0","0.803","0.803","0.73","0.73","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","93e188df-5bbe-c7e7-3359-bf35a752c588","ALL","1.5","in","1.91","THDF",{"$nulls":4},"150",null,null,"0.73","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/2\" ND, 150 LB, FPT, ASME B16.10, 6 1/2\" LG",{"$nulls":4},"VTSC","VALVE","f5c19a0e-ea24-477b-b687-fbf3172c4178","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942",{"$nulls":4},"2",null,"Valves","SKEY=VTSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Gate","False","False","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942","f2edc5b3-d180-5ef0-b800-eb5f8256eee0","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4040"]
[null,"2\"","CPVI001000_OFOF","2.375","2.375","8.5","0","-2","-2",null,null,"0","0.836","0.836","0.76","0.76","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","a8e4bcfa-a9ea-bc98-c121-18448a53ec0e","ALL","2","in","2.375","THDF",{"$nulls":4},"150",null,null,"0.76","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, FPT, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 2\" ND, 150 LB, FPT, ASME B16.10, 8 1/2\" LG",{"$nulls":4},"VTSC","VALVE","f5c19a0e-ea24-477b-b687-fbf3172c4178","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942",{"$nulls":4},"2",null,"Valves","SKEY=VTSC,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Gate","False","False","a1ef5f66-a9e3-4f19-a6d5-cfa4f4d13942","68befc83-c175-5df8-868c-4ce1bb0aea7d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4042"]

{"sheet":"GATE VALVE","index":22,"n_rows":8,"n_cols":85,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","LS","H1","H2","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","ValveAlignment","ValveDetail","ValveBodyType","FlowDependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","ActuatorFamilyName","ActuatorFamilyId","ActuatorPartSizeId","OperatorType","ActuatorType","ActuatorHeight","ActuatorWidth","ControlValve","ValveCode","Normally","Failure","EndConnections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","LS","H1","H2","W1","W2","OF","L1","L2","I1","I2","B1","B2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Valve Alignment","Valve Detail","Valve Body Type","Flow Dependent","Offset","ValveBodyFamilyId","ValveBodyPartSizeId","Actuator Family Name","ActuatorFamilyId","ActuatorPartSizeId","Operator Type","Actuator Type","Actuator Height","Actuator Width","Control Valve","Valve Code","Normally","Failure","End Connections","Number","Code","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPVI001000_OFOF","0.84","0.84","4.25","0","-2","-2",null,null,"0","0.418","0.418","0.38","0.38","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","9519a364-8e34-62a0-c77f-a30f9e630e50","ALL","0.5","in","0.84","SW",{"$nulls":4},"150",null,null,"0.38","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1/2\" ND, 150 LB, SW, ASME B16.10, 4 1/4\" LG",{"$nulls":4},"VTSW","VALVE","2e464802-2988-4035-8255-cfe7af79c515","d8f35aa1-db85-4309-9f9f-bf2532156c18",{"$nulls":4},"2",null,"Valves","SKEY=VTSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.25","Inline","Continuous","Gate","False","False","d8f35aa1-db85-4309-9f9f-bf2532156c18","2687e542-7795-5a49-8ff5-29ffbbf613d3","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4044"]
[null,"3/4\"","CPVI001000_OFOF","1.05","1.05","4.625","0","-2","-2",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","c46ad7dd-c18e-22a1-c4c7-aca834555c27","ALL","0.75","in","1.05","SW",{"$nulls":4},"150",null,null,"0.5","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 3/4\" ND, 150 LB, SW, ASME B16.10, 4 5/8\" LG",{"$nulls":4},"VTSW","VALVE","2e464802-2988-4035-8255-cfe7af79c515","d8f35aa1-db85-4309-9f9f-bf2532156c18",{"$nulls":4},"2",null,"Valves","SKEY=VTSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"4.625","Inline","Continuous","Gate","False","False","d8f35aa1-db85-4309-9f9f-bf2532156c18","1ee1ef8d-7f9e-564c-9fa7-6ce27c988ab1","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4048"]
[null,"1\"","CPVI001000_OFOF","1.315","1.315","5","0","-2","-2",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","09f78934-3599-32df-9345-3cbef435c67d","ALL","1","in","1.315","SW",{"$nulls":4},"150",null,null,"0.5","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1\" ND, 150 LB, SW, ASME B16.10, 5\" LG",{"$nulls":4},"VTSW","VALVE","2e464802-2988-4035-8255-cfe7af79c515","d8f35aa1-db85-4309-9f9f-bf2532156c18",{"$nulls":4},"2",null,"Valves","SKEY=VTSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5","Inline","Continuous","Gate","False","False","d8f35aa1-db85-4309-9f9f-bf2532156c18","bf86ab8b-c788-5101-a50c-be4569854b6e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4050"]
[null,"1 1/4\"","CPVI001000_OFOF","1.66","1.66","5.5","0","-2","-2",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","c68c883c-5af7-2c07-8c36-162401d00add","ALL","1.25","in","1.66","SW",{"$nulls":4},"150",null,null,"0.5","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/4\" ND, 150 LB, SW, ASME B16.10, 5 1/2\" LG",{"$nulls":4},"VTSW","VALVE","2e464802-2988-4035-8255-cfe7af79c515","d8f35aa1-db85-4309-9f9f-bf2532156c18",{"$nulls":4},"2",null,"Valves","SKEY=VTSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"5.5","Inline","Continuous","Gate","False","False","d8f35aa1-db85-4309-9f9f-bf2532156c18","6632d81d-2d87-578f-b618-f90dc7eb243e","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4052"]
[null,"1 1/2\"","CPVI001000_OFOF","1.91","1.91","6.5","0","-2","-2",null,null,"0","0.55","0.55","0.5","0.5","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","3385063c-469c-4a5b-21be-60be47c44b05","ALL","1.5","in","1.91","SW",{"$nulls":4},"150",null,null,"0.5","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 1 1/2\" ND, 150 LB, SW, ASME B16.10, 6 1/2\" LG",{"$nulls":4},"VTSW","VALVE","2e464802-2988-4035-8255-cfe7af79c515","d8f35aa1-db85-4309-9f9f-bf2532156c18",{"$nulls":4},"2",null,"Valves","SKEY=VTSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"6.5","Inline","Continuous","Gate","False","False","d8f35aa1-db85-4309-9f9f-bf2532156c18","1d5b04b5-32a6-575f-b613-b48b390e58f5","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4054"]
[null,"2\"","CPVI001000_OFOF","2.375","2.375","8.5","0","-2","-2",null,null,"0","0.682","0.682","0.62","0.62","0","0","D1,D2,L,LS,H1,H2,W1,W2,OF,L1,L2,I1,I2,B1,B2,","a736842b-1d5e-492b-2aa1-b847f61907a5","ALL","2","in","2.375","SW",{"$nulls":4},"150",null,null,"0.62","in","Gate Valve","ASME B16.10","Solid Wedge","Gate Valve, Solid Wedge, 150 LB, SW, ASME B16.10, ASTM A216 Gr WPB, Hand Wheel","GATE VALVE, SOLID WEDGE, 2\" ND, 150 LB, SW, ASME B16.10, 8 1/2\" LG",{"$nulls":4},"VTSW","VALVE","2e464802-2988-4035-8255-cfe7af79c515","d8f35aa1-db85-4309-9f9f-bf2532156c18",{"$nulls":4},"2",null,"Valves","SKEY=VTSW,TYPE=VALVE",null,"ASME Valves Catalog","4_0",null,null,"8.5","Inline","Continuous","Gate","False","False","d8f35aa1-db85-4309-9f9f-bf2532156c18","ebd6c7d6-1412-5956-a2ca-7a77e5405d8d","Hand Wheel","1bc8e695-b9f3-47bd-beff-382ef635b7f6","09af6d70-66a4-4d3c-a8e1-15c344690baf","Manual","HandWheel","15","8","False",{"$nulls":6},"Valve",null,"4056"]

{"sheet":"TEE (RED)","index":23,"n_rows":36,"n_cols":90,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","D3","L1","L2","L3","A","OF","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","SizeRecordId_S3","PortName_S3","NominalDiameter_S3","NominalUnit_S3","MatchingPipeOd_S3","EndType_S3","FlangeStd_S3","GasketStd_S3","Facing_S3","FlangeThickness_S3","PressureClass_S3","Schedule_S3","WallThickness_S3","EngagementLength_S3","LengthUnit_S3","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","BranchAngle1","BranchAngle2","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","D3","L1","L2","L3","A","OF","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Size Record Id_S3","Port Name_S3","Nominal Diameter_S3","Nominal Unit_S3","Matching Pipe OD_S3","End Type_S3","Flange Std_S3","Gasket Std_S3","Facing_S3","Flange Thickness_S3","Pressure Class_S3","Schedule_S3","Wall Thickness_S3","Engagement Length_S3","Port Unit_S3","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Branch Angle1","Branch Angle2","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"4\"x3\"","CPTS","4.5","4.5","3.5","4.12","4.12","3.88","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","085a25b0-332a-554b-aa52-299d60488024","S1","4","in","4.5","BV",{"$nulls":7},"0","in","43471cf4-f4f6-4455-a8a7-2e80a50b8439","S2","4","in","4.5","BV",{"$nulls":7},"0","in","086f7511-cb97-4cee-8592-2f2dea1a0e7f","S3","3","in","3.5","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 4\"X3\" ND, BW, ASME B16.9",null,null,"11.41","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5786"]
[null,"6\"x4\"","CPTS","6.625","6.625","4.5","5.62","5.62","5.12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","3fa22be5-c37d-5fab-a938-ca515cb7532b","S1","6","in","6.625","BV",{"$nulls":7},"0","in","b58fed1c-f938-4e87-aca5-36fbeb5acd69","S2","6","in","6.625","BV",{"$nulls":7},"0","in","e2a08450-d756-4833-a59d-ed2b995aafbd","S3","4","in","4.5","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 6\"X4\" ND, BW, ASME B16.9",null,null,"35.27","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5817"]
[null,"6\"x3\"","CPTS","6.625","6.625","3.5","5.62","5.62","4.88","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","8f14963c-6be1-5504-9867-5c8f8e095f41","S1","6","in","6.625","BV",{"$nulls":7},"0","in","d80c4733-49c6-47a3-976a-4f6a000be6aa","S2","6","in","6.625","BV",{"$nulls":7},"0","in","8eba1e51-7201-4e3e-9b57-a0296510d100","S3","3","in","3.5","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 6\"X3\" ND, BW, ASME B16.9",null,null,"35.27","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5823"]
[null,"8\"x6\"","CPTS","8.625","8.625","6.625","7","7","6.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","a0a54123-dd51-5a07-91e0-df54aaa00c19","S1","8","in","8.625","BV",{"$nulls":7},"0","in","ec8e9103-d690-4905-8eba-230e71e02599","S2","8","in","8.625","BV",{"$nulls":7},"0","in","cb4a0bef-3e5d-461b-896e-20516c30ab55","S3","6","in","6.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 8\"X6\" ND, BW, ASME B16.9",null,null,"61.72","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5829"]
[null,"8\"x4\"","CPTS","8.625","8.625","4.5","7","7","6.12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","177e358f-598f-5859-9d76-5c4a9c84adcf","S1","8","in","8.625","BV",{"$nulls":7},"0","in","a83205c6-d49e-4688-800c-d6873c199300","S2","8","in","8.625","BV",{"$nulls":7},"0","in","d8729004-ef6a-4ffa-8bcb-24fe8ed8726e","S3","4","in","4.5","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 8\"X4\" ND, BW, ASME B16.9",null,null,"61.72","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5835"]
[null,"8\"x3\"","CPTS","8.625","8.625","3.5","7","7","6","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","51828eec-1b9b-5d73-b371-7e7017058b48","S1","8","in","8.625","BV",{"$nulls":7},"0","in","ee09880e-d78e-42aa-a1a8-8c17aa33e511","S2","8","in","8.625","BV",{"$nulls":7},"0","in","d7925f33-c388-45a0-b587-174ca9cfa155","S3","3","in","3.5","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 8\"X3\" ND, BW, ASME B16.9",null,null,null,"LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5841"]
[null,"10\"x8\"","CPTS","10.75","10.75","8.625","8.5","8.5","8","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","9615ca78-a70f-5097-906c-680564e2e91b","S1","10","in","10.75","BV",{"$nulls":7},"0","in","bfad40e2-618f-4b3c-9086-11a013621bcf","S2","10","in","10.75","BV",{"$nulls":7},"0","in","adcac2b9-d3ae-4d79-9d09-9ecbcfbfd7dc","S3","8","in","8.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 10\"X8\" ND, BW, ASME B16.9",null,null,"90.38","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5844"]
[null,"10\"x6\"","CPTS","10.75","10.75","6.625","8.5","8.5","7.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","7d4da781-cefa-5f6e-b1ac-cbec3a424682","S1","10","in","10.75","BV",{"$nulls":7},"0","in","2a248295-aa4c-48f7-98c0-cc33154e3569","S2","10","in","10.75","BV",{"$nulls":7},"0","in","33992c6c-b223-4643-8614-d72cbaaa666e","S3","6","in","6.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 10\"X6\" ND, BW, ASME B16.9",null,null,"90.38","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5847"]
[null,"10\"x4\"","CPTS","10.75","10.75","4.5","8.5","8.5","7.25","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","5bb7d80b-2836-544c-a207-5bb029df9d8d","S1","10","in","10.75","BV",{"$nulls":7},"0","in","38703602-2ead-43f4-a61b-bb0c773c2076","S2","10","in","10.75","BV",{"$nulls":7},"0","in","94811917-9dd4-4333-9e0f-67ab8e493b1f","S3","4","in","4.5","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 10\"X4\" ND, BW, ASME B16.9",null,null,"90.38","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5853"]
[null,"12\"x10\"","CPTS","12.75","12.75","10.75","10","10","9.5","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","4e2b9940-d26b-568c-a089-571a31478d63","S1","12","in","12.75","BV",{"$nulls":7},"0","in","ee18e647-a2e4-44f9-a7a1-ae06ed1bff33","S2","12","in","12.75","BV",{"$nulls":7},"0","in","4417df5f-23dc-4422-84e1-f24fcfa5f1a7","S3","10","in","10.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 12\"X10\" ND, BW, ASME B16.9",null,null,"138.89","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5856"]
[null,"12\"x8\"","CPTS","12.75","12.75","8.625","10","10","9","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","c77b60fe-b21b-59fb-acc2-a3b46fe87362","S1","12","in","12.75","BV",{"$nulls":7},"0","in","0922ab2e-73db-44f1-9623-06201b5eaa1f","S2","12","in","12.75","BV",{"$nulls":7},"0","in","0e38c005-af5d-4821-8243-e1fe25aee596","S3","8","in","8.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 12\"X8\" ND, BW, ASME B16.9",null,null,"138.89","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5859"]
[null,"12\"x6\"","CPTS","12.75","12.75","6.625","10","10","8.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","2d34d153-ba86-55bf-a287-b2f3dfd94265","S1","12","in","12.75","BV",{"$nulls":7},"0","in","387722c6-124c-4b86-a405-f855b8280054","S2","12","in","12.75","BV",{"$nulls":7},"0","in","8971292e-3dfd-4610-b196-f835b406510e","S3","6","in","6.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 12\"X6\" ND, BW, ASME B16.9",null,null,"138.89","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5862"]
[null,"14\"x12\"","CPTS","14","14","12.75","11","11","10.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","5da4e628-d94c-57a2-8693-1822b231e6d1","S1","14","in","14","BV",{"$nulls":7},"0","in","adf2afc5-fd4a-4cf6-b64e-2912bd2a8b5c","S2","14","in","14","BV",{"$nulls":7},"0","in","d91b2733-9ad7-4ce3-9240-ca65db533c9d","S3","12","in","12.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 14\"X12\" ND, BW, ASME B16.9",null,null,"244.71","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5868"]
[null,"14\"x10\"","CPTS","14","14","10.75","11","11","10.12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","4cf3b5b5-c068-50a8-9d4f-ff42ed5bd17e","S1","14","in","14","BV",{"$nulls":7},"0","in","04438abb-d883-4bf0-a585-d08643ba807d","S2","14","in","14","BV",{"$nulls":7},"0","in","0d296246-ea0b-4845-b365-5da740e71f7a","S3","10","in","10.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 14\"X10\" ND, BW, ASME B16.9",null,null,"235.89","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5871"]
[null,"14\"x8\"","CPTS","14","14","8.625","11","11","9.75","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","54a75179-4530-5610-a036-cef2b9c86e72","S1","14","in","14","BV",{"$nulls":7},"0","in","626a2c54-8beb-4541-a45a-49daf9cc353a","S2","14","in","14","BV",{"$nulls":7},"0","in","cf081646-e434-4eb4-8b9a-d5f1aefc60b3","S3","8","in","8.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 14\"X8\" ND, BW, ASME B16.9",null,null,"235.89","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5874"]
[null,"14\"x6\"","CPTS","14","14","6.625","11","11","9.38","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","28fb180c-d42f-5668-b043-7808fecb4e50","S1","14","in","14","BV",{"$nulls":7},"0","in","443d2b3a-d7f7-4290-b596-a3b988f59e39","S2","14","in","14","BV",{"$nulls":7},"0","in","622294a0-0663-4473-8342-c747d761c94c","S3","6","in","6.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 14\"X6\" ND, BW, ASME B16.9",null,null,"235.89","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5877"]
[null,"16\"x14\"","CPTS","16","16","14","12","12","12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","6fd9f4c0-c10c-5419-97a6-4d8c9164346b","S1","16","in","16","BV",{"$nulls":7},"0","in","3cb05220-3714-47af-b6d4-a326bf1bcc69","S2","16","in","16","BV",{"$nulls":7},"0","in","b8b7e2f0-cced-49f0-94b9-fd405f810dda","S3","14","in","14","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 16\"X14\" ND, BW, ASME B16.9",null,null,"262.34","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5880"]
[null,"16\"x12\"","CPTS","16","16","12.75","12","12","11.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","e3b3ef96-8d4f-56b0-866f-e8d3bfd44528","S1","16","in","16","BV",{"$nulls":7},"0","in","24cb0732-873b-46a8-9357-b976192be73e","S2","16","in","16","BV",{"$nulls":7},"0","in","ff73bb9c-6237-43ef-a33b-caae17a5ae9d","S3","12","in","12.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 16\"X12\" ND, BW, ASME B16.9",null,null,"262.34","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5883"]
[null,"16\"x10\"","CPTS","16","16","10.75","12","12","11.12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","3ff4b963-961c-52f3-ad06-3aaf3aa36014","S1","16","in","16","BV",{"$nulls":7},"0","in","cab02536-9758-4de9-9201-d82df040d76b","S2","16","in","16","BV",{"$nulls":7},"0","in","eb2ab464-b91b-45e1-99c2-968a3dee060b","S3","10","in","10.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 16\"X10\" ND, BW, ASME B16.9",null,null,"255.73","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5886"]
[null,"16\"x8\"","CPTS","16","16","8.625","12","12","10.75","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","1b808365-18cb-523d-8e49-8b46186c09b6","S1","16","in","16","BV",{"$nulls":7},"0","in","63ca9dbe-24c1-4d90-a12f-966e8b6dcbad","S2","16","in","16","BV",{"$nulls":7},"0","in","6db103de-f0ad-44f1-ae17-337639fd2bb3","S3","8","in","8.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 16\"X8\" ND, BW, ASME B16.9",null,null,"255.73","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5889"]
[null,"18\"x16\"","CPTS","18","18","16","13.5","13.5","13","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","26b5e725-eba8-5b59-a278-1d3e30d124b9","S1","18","in","18","BV",{"$nulls":7},"0","in","6386083a-5e1c-4d54-a1a9-adeedf37bfea","S2","18","in","18","BV",{"$nulls":7},"0","in","e882fb8c-4d8d-4875-8376-20e2fdfbd36b","S3","16","in","16","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 18\"X16\" ND, BW, ASME B16.9",null,null,"297.62","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5895"]
[null,"18\"x14\"","CPTS","18","18","14","13.5","13.5","13","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","2b9d659e-9fdd-58df-96cc-e4e8fbc4df94","S1","18","in","18","BV",{"$nulls":7},"0","in","4083af74-af5b-44c6-8596-07ea27b18af2","S2","18","in","18","BV",{"$nulls":7},"0","in","cf0eec8c-8c59-450c-b6e6-be75c90729cc","S3","14","in","14","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 18\"X14\" ND, BW, ASME B16.9",null,null,"297.62","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5898"]
[null,"18\"x12\"","CPTS","18","18","12.75","13.5","13.5","12.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","80db8cba-e7e4-542c-99f2-1c5b24a45422","S1","18","in","18","BV",{"$nulls":7},"0","in","e71634bb-ae1d-44f5-81a4-26e3fcc9f0f9","S2","18","in","18","BV",{"$nulls":7},"0","in","1e4070c2-4f37-4322-82d3-a03abfc24d15","S3","12","in","12.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 18\"X12\" ND, BW, ASME B16.9",null,null,"297.62","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5902"]
[null,"18\"x10\"","CPTS","18","18","10.75","13.5","13.5","12.12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","de122082-c8c2-5138-929d-3915a6f2fd18","S1","18","in","18","BV",{"$nulls":7},"0","in","ac79a001-1691-4280-a9e6-03d9675ab98b","S2","18","in","18","BV",{"$nulls":7},"0","in","a0b42156-620f-4981-86f9-5b8cb2e1d022","S3","10","in","10.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 18\"X10\" ND, BW, ASME B16.9",null,null,"284.39","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5905"]
[null,"18\"x8\"","CPTS","18","18","8.625","13.5","13.5","11.75","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","8b89f44d-9356-5799-80fe-1b5b16dbdf31","S1","18","in","18","BV",{"$nulls":7},"0","in","6012d1cc-4e61-4d53-b5d8-21cb1a22a7c4","S2","18","in","18","BV",{"$nulls":7},"0","in","fed13d87-3b88-451c-9911-57b64bf798eb","S3","8","in","8.625","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 18\"X8\" ND, BW, ASME B16.9",null,null,"284.39","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5908"]
[null,"20\"x18\"","CPTS","20","20","18","15","15","14.5","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","4b15da37-86b8-5cc2-a70b-615583401d75","S1","20","in","20","BV",{"$nulls":7},"0","in","60b02fd6-c523-484c-b371-e99e4aa5aae9","S2","20","in","20","BV",{"$nulls":7},"0","in","3840ee58-fc26-4c0f-a40b-4ece8bde528b","S3","18","in","18","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 20\"X18\" ND, BW, ASME B16.9",null,null,"370.37","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5911"]
[null,"20\"x16\"","CPTS","20","20","16","15","15","14","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","e99bef8f-42c1-5a49-bcfc-402282d557f9","S1","20","in","20","BV",{"$nulls":7},"0","in","eb9fbe73-47f6-4d2d-962b-3fd846934717","S2","20","in","20","BV",{"$nulls":7},"0","in","a5f5058c-862d-41ef-bb8b-5c41aaf5c10c","S3","16","in","16","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 20\"X16\" ND, BW, ASME B16.9",null,null,"370.37","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5914"]
[null,"20\"x14\"","CPTS","20","20","14","15","15","14","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","26aa5cf1-71cd-5d56-9749-206e4030659c","S1","20","in","20","BV",{"$nulls":7},"0","in","f1d3560c-480d-4ab6-a041-a32da1a4f8e9","S2","20","in","20","BV",{"$nulls":7},"0","in","0a555cdb-29ba-40eb-8868-1c7cc30fe07e","S3","14","in","14","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 20\"X14\" ND, BW, ASME B16.9",null,null,"359.35","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5917"]
[null,"20\"x12\"","CPTS","20","20","12.75","15","15","13.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","9209c6d4-e8fd-5771-9bfa-3885f483dc30","S1","20","in","20","BV",{"$nulls":7},"0","in","9e4bb4fb-499f-4d84-a90b-54a72d5cac98","S2","20","in","20","BV",{"$nulls":7},"0","in","1033e196-16f5-40dc-8283-34c8f3912ef5","S3","12","in","12.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 20\"X12\" ND, BW, ASME B16.9",null,null,"359.35","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5920"]
[null,"24\"x20\"","CPTS","24","24","20","17","17","17","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","ca67ceb0-51db-56fe-9d66-f02a166cbae1","S1","24","in","24","BV",{"$nulls":7},"0","in","55314955-e7ff-4188-9667-dc9f82ed5b4c","S2","24","in","24","BV",{"$nulls":7},"0","in","e68bf393-dfa9-4fc4-8769-9018e266829c","S3","20","in","20","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 24\"X20\" ND, BW, ASME B16.9",null,null,"500.44","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5950"]
[null,"24\"x18\"","CPTS","24","24","18","17","17","16.5","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","e5cce8f3-c6ec-5e1e-8791-ed84be84ae68","S1","24","in","24","BV",{"$nulls":7},"0","in","e5682277-1fb6-4496-a03d-0529bf50f268","S2","24","in","24","BV",{"$nulls":7},"0","in","7db538f0-0f53-4366-a5da-6b6f1a4f150a","S3","18","in","18","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 24\"X18\" ND, BW, ASME B16.9",null,null,"500.44","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5953"]
[null,"24\"x16\"","CPTS","24","24","16","17","17","16","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","c1af36c7-f9fa-548b-814f-4ccf41e79dc4","S1","24","in","24","BV",{"$nulls":7},"0","in","f494758b-f2c9-43ef-822d-dd8f2c991f30","S2","24","in","24","BV",{"$nulls":7},"0","in","de00bc86-b38e-47b1-9742-55cdd34aa4b7","S3","16","in","16","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 24\"X16\" ND, BW, ASME B16.9",null,null,"489.42","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5956"]
[null,"24\"x14\"","CPTS","24","24","14","17","17","16","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","21134eec-7d48-5e6f-850b-3dda3e8a56ef","S1","24","in","24","BV",{"$nulls":7},"0","in","31f2ea91-53e7-4172-807d-93365e179c18","S2","24","in","24","BV",{"$nulls":7},"0","in","06e95383-e447-4f31-a9cd-8fc786cdc4e1","S3","14","in","14","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 24\"X14\" ND, BW, ASME B16.9",null,null,"489.42","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5959"]
[null,"24\"x12\"","CPTS","24","24","12.75","17","17","15.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","3e4a9c56-a8c2-56d2-b035-683ac2944956","S1","24","in","24","BV",{"$nulls":7},"0","in","03bbcb03-13ac-4579-834a-7477715ff13b","S2","24","in","24","BV",{"$nulls":7},"0","in","846119f6-c845-4201-8962-944dc0b22836","S3","12","in","12.75","BV",{"$nulls":7},"0","in","Tee (red)","ASME B16.9",null,"TEE (RED), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE (RED), 24\"X12\" ND, BW, ASME B16.9",null,null,"480.6","LB","TEBW","TEE","737eedef-e177-44d9-82fc-15f207ce3a81","88b93fc1-47e6-4f1a-8548-bcd7140d19ab",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5962"]

{"sheet":"TEE_1","index":24,"n_rows":7,"n_cols":66,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","D3","L1","L2","L3","L12","L22","L32","I1","I2","I3","A","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","BranchAngle1","BranchAngle2","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","D3","L1","L2","L3","L12","L22","L32","I1","I2","I3","A","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Branch Angle1","Branch Angle2","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPTS_OFOFOF","0.84","0.84","0.84","0.62","0.62","0.62","0.48","0.48","0.48","0.38","0.38","0.38","90","-1","D1,D2,D3,L1,L2,L3,L12,L22,L32,I1,I2,I3,A,OF,","139c7894-ddda-5536-bf3a-90ff7c29b829","ALL","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.38","in","Tee","ASME B16.11",null,"TEE, 3000 LB, SW, ASME B16.11, ASTM A105","TEE, 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.6875","LB","TESW","TEE","8a35227a-1617-4551-b02c-d86b855319f8","978618d4-b3dd-4ccc-a0ab-838016f6439c",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TESW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"3257"]
[null,"3/4\"","CPTS_OFOFOF","1.05","1.05","1.05","0.75","0.75","0.75","0.6","0.6","0.6","0.5","0.5","0.5","90","-1","D1,D2,D3,L1,L2,L3,L12,L22,L32,I1,I2,I3,A,OF,","95f534af-3ad8-53d1-a72a-0eb75fd7ffe6","ALL","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","Tee","ASME B16.11",null,"TEE, 3000 LB, SW, ASME B16.11, ASTM A105","TEE, 3/4\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.875","LB","TESW","TEE","8a35227a-1617-4551-b02c-d86b855319f8","978618d4-b3dd-4ccc-a0ab-838016f6439c",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TESW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"3260"]
[null,"1\"","CPTS_OFOFOF","1.315","1.315","1.315","0.88","0.88","0.88","0.6","0.6","0.6","0.5","0.5","0.5","90","-1","D1,D2,D3,L1,L2,L3,L12,L22,L32,I1,I2,I3,A,OF,","adca63c2-29cf-55ba-a232-c4fe79e981ce","ALL","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","Tee","ASME B16.11",null,"TEE, 3000 LB, SW, ASME B16.11, ASTM A105","TEE, 1\" ND, 3000 LB, SW, ASME B16.11",null,null,"1.4375","LB","TESW","TEE","8a35227a-1617-4551-b02c-d86b855319f8","978618d4-b3dd-4ccc-a0ab-838016f6439c",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TESW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"3263"]
[null,"1 1/2\"","CPTS_OFOFOF","1.9","1.9","1.9","1.25","1.25","1.25","0.6","0.6","0.6","0.5","0.5","0.5","90","-1","D1,D2,D3,L1,L2,L3,L12,L22,L32,I1,I2,I3,A,OF,","424a92ae-410c-5db0-8d86-766566180e58","ALL","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","Tee","ASME B16.11",null,"TEE, 3000 LB, SW, ASME B16.11, ASTM A105","TEE, 1 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"2.4375","LB","TESW","TEE","8a35227a-1617-4551-b02c-d86b855319f8","978618d4-b3dd-4ccc-a0ab-838016f6439c",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TESW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"3269"]
[null,"2\"","CPTS_OFOFOF","2.375","2.375","2.375","1.5","1.5","1.5","0.72","0.72","0.72","0.62","0.62","0.62","90","-1","D1,D2,D3,L1,L2,L3,L12,L22,L32,I1,I2,I3,A,OF,","a5b25a93-adc4-5614-9bab-a6d9c21c3e6b","ALL","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.62","in","Tee","ASME B16.11",null,"TEE, 3000 LB, SW, ASME B16.11, ASTM A105","TEE, 2\" ND, 3000 LB, SW, ASME B16.11",null,null,"4.4375","LB","TESW","TEE","8a35227a-1617-4551-b02c-d86b855319f8","978618d4-b3dd-4ccc-a0ab-838016f6439c",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TESW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"3272"]

{"sheet":"TEE","index":25,"n_rows":13,"n_cols":60,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","D3","L1","L2","L3","A","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","BranchAngle1","BranchAngle2","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","D3","L1","L2","L3","A","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Branch Angle1","Branch Angle2","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPTS","3.5","3.5","3.5","3.38","3.38","3.38","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","b9d8acc9-ad5b-5038-b263-5ce426c1b67b","ALL","3","in","3.5","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 3\" ND, BW, ASME B16.9",null,null,"8.42","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5611"]
[null,"4\"","CPTS","4.5","4.5","4.5","4.12","4.12","4.12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","95306dfa-cc90-5a28-a517-3ccc9a352559","ALL","4","in","4.5","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 4\" ND, BW, ASME B16.9",null,null,"13.22","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5617"]
[null,"6\"","CPTS","6.625","6.625","6.625","5.62","5.62","5.62","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","c9ab02c9-1f6c-5770-8184-b857b9ff09cf","ALL","6","in","6.625","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 6\" ND, BW, ASME B16.9",null,null,"36.33","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5623"]
[null,"8\"","CPTS","8.625","8.625","8.625","7","7","7","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","b24fd3a7-6d97-54cc-b9bf-72de87f15074","ALL","8","in","8.625","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 8\" ND, BW, ASME B16.9",null,null,"72.75","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5626"]
[null,"10\"","CPTS","10.75","10.75","10.75","8.5","8.5","8.5","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","1e361218-83b1-5062-8fd2-08658dc739cd","ALL","10","in","10.75","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 10\" ND, BW, ASME B16.9",null,null,"108.79","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5629"]
[null,"12\"","CPTS","12.75","12.75","12.75","10","10","10","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","73b16332-b4d6-5051-a936-c51d33e9ea1b","ALL","12","in","12.75","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 12\" ND, BW, ASME B16.9",null,null,"143.3","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5632"]
[null,"14\"","CPTS","14","14","14","11","11","11","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","4d8e0e2a-98ae-53b2-9dfc-f513c610f719","ALL","14","in","14","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 14\" ND, BW, ASME B16.9",null,null,"205.02","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5635"]
[null,"16\"","CPTS","16","16","16","12","12","12","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","b9a0d2a3-a469-586c-abc0-2ac6055b254f","ALL","16","in","16","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 16\" ND, BW, ASME B16.9",null,null,"253.53","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5638"]
[null,"18\"","CPTS","18","18","18","13.5","13.5","13.5","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","929a95fe-5891-51b8-adf1-a9100553a134","ALL","18","in","18","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 18\" ND, BW, ASME B16.9",null,null,"297.62","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5641"]
[null,"20\"","CPTS","20","20","20","15","15","15","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","abb35fdd-922a-5dac-8d44-8b43ad7a6f6c","ALL","20","in","20","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 20\" ND, BW, ASME B16.9",null,null,"370.37","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5644"]
[null,"24\"","CPTS","24","24","24","17","17","17","90","-1","D1,D2,D3,L1,L2,L3,A,OF,","27545670-e6a1-5cd9-966f-b42af00f7932","ALL","24","in","24","BV",{"$nulls":7},"0","in","Tee","ASME B16.9",null,"TEE, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","TEE, 24\" ND, BW, ASME B16.9",null,null,"529.1","LB","TEBW","TEE","73fabc32-82af-4795-9d4b-857e4f0c1c91","9369eb32-9e59-459b-b5d4-e235b522d9ad",{"$nulls":4},"3",null,"Fittings","TYPE=TEE,SKEY=TEBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,null,"90",null,"False","Tee",null,"5650"]

{"sheet":"REDUCER (CONC)","index":26,"n_rows":33,"n_cols":69,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","OF","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","OF","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"x2\"","CPJRC","3.5","2.375","3.5","-1","D1,D2,L,OF,","8e590306-3b5f-59b6-b9a2-dc263ec981e6","S1","3","in","3.5","BV",{"$nulls":7},"0","in","1e17be6e-82e7-4884-8a7a-4e890cadfcd4","S2","2","in","2.375","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 3\"X2\" ND, BW, ASME B16.9",null,null,"2.2","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3.5","False","Reducer",null,"5363"]
[null,"4\"x3\"","CPJRC","4.5","3.5","4","-1","D1,D2,L,OF,","7f8b4344-cf9f-543e-8912-ceca87df9e35","S1","4","in","4.5","BV",{"$nulls":7},"0","in","e5b3a9f5-4544-4807-8d9e-01c48707d641","S2","3","in","3.5","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 4\"X3\" ND, BW, ASME B16.9",null,null,"3.52","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"4","False","Reducer",null,"5383"]
[null,"6\"x3\"","CPJRC","6.625","3.5","5.5","-1","D1,D2,L,OF,","904bb0ac-64e3-59b5-84df-2d956659b235","S1","6","in","6.625","BV",{"$nulls":7},"0","in","e2855c92-6d08-4904-8768-f19a48c9cd0f","S2","3","in","3.5","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 6\"X3\" ND, BW, ASME B16.9",null,null,"8.59","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5.5","False","Reducer",null,"5399"]
[null,"6\"x4\"","CPJRC","6.625","4.5","5.5","-1","D1,D2,L,OF,","43875701-a66a-5121-9763-f47850dae468","S1","6","in","6.625","BV",{"$nulls":7},"0","in","b97c6bed-4629-44b4-a8eb-18d32afb77ba","S2","4","in","4.5","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 6\"X4\" ND, BW, ASME B16.9",null,null,"8.59","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5.5","False","Reducer",null,"5404"]
[null,"8\"x4\"","CPJRC","8.625","4.5","6","-1","D1,D2,L,OF,","0c94a94a-1529-5ae3-a561-fb1ce787747d","S1","8","in","8.625","BV",{"$nulls":7},"0","in","b99fbf08-e1d3-470c-979d-e3025043ed98","S2","4","in","4.5","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 8\"X4\" ND, BW, ASME B16.9",null,null,"14.33","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"6","False","Reducer",null,"5410"]
[null,"8\"x6\"","CPJRC","8.625","6.625","6","-1","D1,D2,L,OF,","17fd8102-ea35-5911-93ae-794e89670544","S1","8","in","8.625","BV",{"$nulls":7},"0","in","c4ebbad7-3fe4-4d9b-a371-9a9bb7258e05","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 8\"X6\" ND, BW, ASME B16.9",null,null,"14.33","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"6","False","Reducer",null,"5414"]
[null,"10\"x4\"","CPJRC","10.75","4.5","7","-1","D1,D2,L,OF,","73251383-52cf-5288-a96d-fc7dbfd6f2b1","S1","10","in","10.75","BV",{"$nulls":7},"0","in","2ce2a364-7f78-4946-8180-fd834946f86d","S2","4","in","4.5","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 10\"X4\" ND, BW, ASME B16.9",null,null,"23.58","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7","False","Reducer",null,"5416"]
[null,"10\"x6\"","CPJRC","10.75","6.625","7","-1","D1,D2,L,OF,","59a5a946-8880-5547-91c1-e62cf9f72109","S1","10","in","10.75","BV",{"$nulls":7},"0","in","55acaf18-81af-4c71-8a52-f077571207aa","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 10\"X6\" ND, BW, ASME B16.9",null,null,"23.58","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7","False","Reducer",null,"5420"]
[null,"10\"x8\"","CPJRC","10.75","8.625","7","-1","D1,D2,L,OF,","60d62915-f9bc-5e01-9f6f-63ff0ca9a3d3","S1","10","in","10.75","BV",{"$nulls":7},"0","in","a5df63d8-8c23-4d47-8731-240d8a6fb004","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 10\"X8\" ND, BW, ASME B16.9",null,null,"23.58","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7","False","Reducer",null,"5422"]
[null,"12\"x6\"","CPJRC","12.75","6.625","8","-1","D1,D2,L,OF,","e363e147-a056-595e-a3cb-b9f73b0c8936","S1","12","in","12.75","BV",{"$nulls":7},"0","in","f3ba766d-9cd6-4925-ba5a-4b3396b7dfd1","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 12\"X6\" ND, BW, ASME B16.9",null,null,"33.06","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"8","False","Reducer",null,"5426"]
[null,"12\"x8\"","CPJRC","12.75","8.625","8","-1","D1,D2,L,OF,","fd4d39c5-1a47-5e37-b0cd-a4972320ab04","S1","12","in","12.75","BV",{"$nulls":7},"0","in","10611e3b-0d9a-43ee-9704-7a4a3662f788","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 12\"X8\" ND, BW, ASME B16.9",null,null,"33.06","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"8","False","Reducer",null,"5428"]
[null,"12\"x10\"","CPJRC","12.75","10.75","8","-1","D1,D2,L,OF,","5d64b4be-7e92-5ea6-be7e-1a163c1ea2a1","S1","12","in","12.75","BV",{"$nulls":7},"0","in","ca863853-dec3-4813-92e7-5f966115d192","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 12\"X10\" ND, BW, ASME B16.9",null,null,"33.06","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"8","False","Reducer",null,"5430"]
[null,"14\"x6\"","CPJRC","14","6.625","13","-1","D1,D2,L,OF,","39dca92e-f4f2-5392-adc1-043fc2b405c0","S1","14","in","14","BV",{"$nulls":7},"0","in","298c9a80-f279-4f4f-b9dc-a9ab4e965516","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 14\"X6\" ND, BW, ASME B16.9",null,null,"59.3","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","False","Reducer",null,"5432"]
[null,"14\"x8\"","CPJRC","14","8.625","13","-1","D1,D2,L,OF,","717a0732-f1bf-5337-b65e-fe95679f1b61","S1","14","in","14","BV",{"$nulls":7},"0","in","f553e845-92a4-4b1b-a540-d467f2f661b7","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 14\"X8\" ND, BW, ASME B16.9",null,null,"59.3","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","False","Reducer",null,"5434"]
[null,"14\"x10\"","CPJRC","14","10.75","13","-1","D1,D2,L,OF,","e16733bd-4168-53b0-b168-1c91a16302ad","S1","14","in","14","BV",{"$nulls":7},"0","in","d71ac767-98e6-4580-8779-bd76ac4ce93f","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 14\"X10\" ND, BW, ASME B16.9",null,null,"59.3","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","False","Reducer",null,"5436"]
[null,"14\"x12\"","CPJRC","14","12.75","13","-1","D1,D2,L,OF,","3666a5c6-bd0d-51fa-9a65-5c5265113c86","S1","14","in","14","BV",{"$nulls":7},"0","in","52403d51-a145-48d8-85e6-5968b0aa3120","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 14\"X12\" ND, BW, ASME B16.9",null,null,"59.3","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","False","Reducer",null,"5438"]
[null,"16\"x8\"","CPJRC","16","8.625","14","-1","D1,D2,L,OF,","8b275269-3b2b-5d6f-a751-aa6e1f21b3d1","S1","16","in","16","BV",{"$nulls":7},"0","in","5f779b74-af63-41e2-97b7-e35fc985ec12","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 16\"X8\" ND, BW, ASME B16.9",null,null,"72.75","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","False","Reducer",null,"5440"]
[null,"16\"x10\"","CPJRC","16","10.75","14","-1","D1,D2,L,OF,","354bd6a2-c7a8-55d7-93bc-f46d599d4900","S1","16","in","16","BV",{"$nulls":7},"0","in","c62b0322-59d3-4cf6-b9c3-57d6a867a5d6","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 16\"X10\" ND, BW, ASME B16.9",null,null,"72.75","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","False","Reducer",null,"5442"]
[null,"16\"x12\"","CPJRC","16","12.75","14","-1","D1,D2,L,OF,","f9a45bdb-5b74-52dc-a230-1f8447878ad6","S1","16","in","16","BV",{"$nulls":7},"0","in","6d4771c9-efb9-44c1-b4a7-145d698ea3f6","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 16\"X12\" ND, BW, ASME B16.9",null,null,"72.75","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","False","Reducer",null,"5444"]
[null,"16\"x14\"","CPJRC","16","14","14","-1","D1,D2,L,OF,","28561b5b-e9c5-5551-951f-ede039da6de7","S1","16","in","16","BV",{"$nulls":7},"0","in","95cc94d8-2bee-46e0-a725-437361ea10e9","S2","14","in","14","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 16\"X14\" ND, BW, ASME B16.9",null,null,"72.75","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","False","Reducer",null,"5446"]
[null,"18\"x10\"","CPJRC","18","10.75","15","-1","D1,D2,L,OF,","5750a59b-a14e-5732-b7f8-f0b1f77d97c0","S1","18","in","18","BV",{"$nulls":7},"0","in","e10c6cec-ebd2-46b5-b241-287705fda647","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 18\"X10\" ND, BW, ASME B16.9",null,null,"88.18","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","False","Reducer",null,"5448"]
[null,"18\"x12\"","CPJRC","18","12.75","15","-1","D1,D2,L,OF,","c927e9e1-5d49-5b6b-8ead-26ac57abeb12","S1","18","in","18","BV",{"$nulls":7},"0","in","ce5ffe6f-9217-4ea8-ba10-bc061e3b98b0","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 18\"X12\" ND, BW, ASME B16.9",null,null,"88.18","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","False","Reducer",null,"5450"]
[null,"18\"x14\"","CPJRC","18","14","15","-1","D1,D2,L,OF,","575dbe76-6ad9-5e28-acb2-396c58c322ef","S1","18","in","18","BV",{"$nulls":7},"0","in","88e18692-939b-4a48-83cf-c2ad40472372","S2","14","in","14","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 18\"X14\" ND, BW, ASME B16.9",null,null,"88.18","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","False","Reducer",null,"5452"]
[null,"18\"x16\"","CPJRC","18","16","15","-1","D1,D2,L,OF,","9b66d167-e207-5c42-894f-fb931d10e594","S1","18","in","18","BV",{"$nulls":7},"0","in","b08a2810-bb77-4f04-9802-0b9f2589714e","S2","16","in","16","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 18\"X16\" ND, BW, ASME B16.9",null,null,"88.18","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","False","Reducer",null,"5454"]
[null,"20\"x12\"","CPJRC","20","12.75","20","-1","D1,D2,L,OF,","12447bc7-6d84-5a23-899b-f0c6ec98e6f7","S1","20","in","20","BV",{"$nulls":7},"0","in","9f71dc49-3922-4d15-8ad1-96e26e81f2e8","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 20\"X12\" ND, BW, ASME B16.9",null,null,"130.07","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5456"]
[null,"20\"x14\"","CPJRC","20","14","20","-1","D1,D2,L,OF,","8d518889-fc5a-599a-92e6-d0916d0f2340","S1","20","in","20","BV",{"$nulls":7},"0","in","c3a0565c-3e51-471f-b7f0-a9502e3a2f20","S2","14","in","14","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 20\"X14\" ND, BW, ASME B16.9",null,null,"130.07","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5458"]
[null,"20\"x16\"","CPJRC","20","16","20","-1","D1,D2,L,OF,","076c8fcc-c88d-58b5-b1bf-3b2c6aff23f2","S1","20","in","20","BV",{"$nulls":7},"0","in","32b4a142-177e-42ab-86b1-d9904823e429","S2","16","in","16","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 20\"X16\" ND, BW, ASME B16.9",null,null,"130.07","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5460"]
[null,"20\"x18\"","CPJRC","20","18","20","-1","D1,D2,L,OF,","a38bf629-5c9c-5ffb-b890-6c8f58993c39","S1","20","in","20","BV",{"$nulls":7},"0","in","33ef11fb-4a2d-4f89-8a54-1e2d3d0f996b","S2","18","in","18","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 20\"X18\" ND, BW, ASME B16.9",null,null,"130.07","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5462"]
[null,"24\"x16\"","CPJRC","24","16","20","-1","D1,D2,L,OF,","95700ac2-5281-555e-98b7-0da7648bb173","S1","24","in","24","BV",{"$nulls":7},"0","in","862b5842-c8b3-4599-a40b-a4ba31af3c7a","S2","16","in","16","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 24\"X16\" ND, BW, ASME B16.9",null,null,"158.73","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5472"]
[null,"24\"x18\"","CPJRC","24","18","20","-1","D1,D2,L,OF,","f56489bc-cbc2-510b-be9a-b2cdfcd20702","S1","24","in","24","BV",{"$nulls":7},"0","in","1a6cbe6b-4542-4e22-b6b0-7fcab628e39c","S2","18","in","18","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 24\"X18\" ND, BW, ASME B16.9",null,null,"158.73","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5474"]
[null,"24\"x20\"","CPJRC","24","20","20","-1","D1,D2,L,OF,","d1373018-ea70-56c1-9ab8-dc04c70aa6cd","S1","24","in","24","BV",{"$nulls":7},"0","in","5a5356d4-5ac6-4a60-99d1-8a2691968682","S2","20","in","20","BV",{"$nulls":7},"0","in","REDUCER (CONC)","ASME B16.9",null,"REDUCER (CONC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (CONC), 24\"X20\" ND, BW, ASME B16.9",null,null,"158.73","LB","RCBW","REDUCER","8a6d1697-e5a5-4aa0-9fb2-fde71b00808e","268c99ee-96e7-4272-a8cd-06837d88615d",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-CONCENTRIC,SKEY=RCBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","False","Reducer",null,"5476"]

{"sheet":"REDUCER (ECC)","index":27,"n_rows":34,"n_cols":70,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","E","OF","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","E","OF","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","Eccentricity","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"x2\"","CPJRE","3.5","2.375","3.5","0","-1","D1,D2,L,E,OF,","6a5f0055-6af0-50bc-bdb9-56ac4f0822e2","S1","3","in","3.5","BV",{"$nulls":7},"0","in","434c56b4-bb91-4e45-a1cc-d2190b7dab90","S2","2","in","2.375","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 3\"X2\" ND, BW, ASME B16.9",null,null,"2.2","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3.5","True","Reducer",null,"5094"]
[null,"4\"x2\"","CPJRE","4.5","2.375","4","0","-1","D1,D2,L,E,OF,","7a947db1-1cca-5728-ba8d-3f58afdc7e2a","S1","4","in","4.5","BV",{"$nulls":7},"0","in","196578bd-a88a-4240-83a4-3cf65aa54173","S2","2","in","2.375","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 4\"X2\" ND, BW, ASME B16.9",null,null,"3.52","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"4","True","Reducer",null,"5111"]
[null,"4\"x3\"","CPJRE","4.5","3.5","4","0","-1","D1,D2,L,E,OF,","1673e64a-fb90-5e10-a295-36b5461f67ad","S1","4","in","4.5","BV",{"$nulls":7},"0","in","5903a939-d38b-407e-b1af-18fb30f2571e","S2","3","in","3.5","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 4\"X3\" ND, BW, ASME B16.9",null,null,"3.52","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"4","True","Reducer",null,"5115"]
[null,"6\"x3\"","CPJRE","6.625","3.5","5.5","0","-1","D1,D2,L,E,OF,","3814b68e-9428-5ca6-831a-3575663a3782","S1","6","in","6.625","BV",{"$nulls":7},"0","in","58d7fe31-b082-461b-a776-06198ccc421d","S2","3","in","3.5","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 6\"X3\" ND, BW, ASME B16.9",null,null,"8.59","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5.5","True","Reducer",null,"5131"]
[null,"6\"x4\"","CPJRE","6.625","4.5","5.5","0","-1","D1,D2,L,E,OF,","cc95c2f6-31cf-5bd5-a76f-5b94330bc503","S1","6","in","6.625","BV",{"$nulls":7},"0","in","c201ce9b-39e9-4755-a733-22b93edfc63e","S2","4","in","4.5","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 6\"X4\" ND, BW, ASME B16.9",null,null,"8.59","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5.5","True","Reducer",null,"5135"]
[null,"8\"x4\"","CPJRE","8.625","4.5","6","0","-1","D1,D2,L,E,OF,","9a8cca14-70db-53e9-b694-c6814223860b","S1","8","in","8.625","BV",{"$nulls":7},"0","in","5aa8ae71-ad1e-45a1-a4e3-cc9355203175","S2","4","in","4.5","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 8\"X4\" ND, BW, ASME B16.9",null,null,"14.33","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"6","True","Reducer",null,"5141"]
[null,"8\"x6\"","CPJRE","8.625","6.625","6","0","-1","D1,D2,L,E,OF,","45dbdefe-dcbd-5103-b2fa-89395bbf1930","S1","8","in","8.625","BV",{"$nulls":7},"0","in","65b8b05b-bf94-4e78-844f-9cc376286067","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 8\"X6\" ND, BW, ASME B16.9",null,null,"14.33","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"6","True","Reducer",null,"5145"]
[null,"10\"x4\"","CPJRE","10.75","4.5","7","0","-1","D1,D2,L,E,OF,","0d339a4c-4d97-5dd0-af98-d22d1f8ffc69","S1","10","in","10.75","BV",{"$nulls":7},"0","in","1b70dcac-c992-4f38-a937-7c83d51e98c9","S2","4","in","4.5","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 10\"X4\" ND, BW, ASME B16.9",null,null,"23.58","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7","True","Reducer",null,"5147"]
[null,"10\"x6\"","CPJRE","10.75","6.625","7","0","-1","D1,D2,L,E,OF,","67ebbc72-ae20-5a0a-8470-274b0058977b","S1","10","in","10.75","BV",{"$nulls":7},"0","in","b12e8fa7-a136-4cbb-932b-c97f98b389d5","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 10\"X6\" ND, BW, ASME B16.9",null,null,"23.58","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7","True","Reducer",null,"5151"]
[null,"10\"x8\"","CPJRE","10.75","8.625","7","0","-1","D1,D2,L,E,OF,","6f000235-ffa7-5aaa-8591-f648dbddd1c3","S1","10","in","10.75","BV",{"$nulls":7},"0","in","84285636-581b-4c94-8aa0-cd99e2e9832e","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 10\"X8\" ND, BW, ASME B16.9",null,null,"23.58","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7","True","Reducer",null,"5153"]
[null,"12\"x6\"","CPJRE","12.75","6.625","8","0","-1","D1,D2,L,E,OF,","63777b78-1c30-56ff-bb1b-f83073accb4b","S1","12","in","12.75","BV",{"$nulls":7},"0","in","710cb3aa-806b-4a11-a1af-2b7c8a533f08","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 12\"X6\" ND, BW, ASME B16.9",null,null,"33.06","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"8","True","Reducer",null,"5157"]
[null,"12\"x8\"","CPJRE","12.75","8.625","8","0","-1","D1,D2,L,E,OF,","927c2f6c-e701-52fe-a0e5-18c35b419613","S1","12","in","12.75","BV",{"$nulls":7},"0","in","9092ad03-bf03-44dd-a6cc-24abae887c81","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 12\"X8\" ND, BW, ASME B16.9",null,null,"33.06","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"8","True","Reducer",null,"5159"]
[null,"12\"x10\"","CPJRE","12.75","10.75","8","0","-1","D1,D2,L,E,OF,","08ab8f0a-3bd1-518c-97c5-1f50c1e9e84e","S1","12","in","12.75","BV",{"$nulls":7},"0","in","2b63ece0-8085-43e7-b109-5309f4d5bd53","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 12\"X10\" ND, BW, ASME B16.9",null,null,"33.06","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"8","True","Reducer",null,"5161"]
[null,"14\"x6\"","CPJRE","14","6.625","13","0","-1","D1,D2,L,E,OF,","a8d92c75-4912-5eaf-9ef8-4efd11bb34e5","S1","14","in","14","BV",{"$nulls":7},"0","in","7dfe00ae-32b8-4921-8a00-f54648db52b0","S2","6","in","6.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 14\"X6\" ND, BW, ASME B16.9",null,null,"59.3","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","True","Reducer",null,"5163"]
[null,"14\"x8\"","CPJRE","14","8.625","13","0","-1","D1,D2,L,E,OF,","9aad37ca-b593-566a-b1f2-0fccf1a398c2","S1","14","in","14","BV",{"$nulls":7},"0","in","1c7b1c8b-ca5e-4f05-a265-7e08be841e94","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 14\"X8\" ND, BW, ASME B16.9",null,null,"59.3","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","True","Reducer",null,"5165"]
[null,"14\"x10\"","CPJRE","14","10.75","13","0","-1","D1,D2,L,E,OF,","f50d8b1c-aa36-57cd-a850-9fc8723c370f","S1","14","in","14","BV",{"$nulls":7},"0","in","2628e111-66ac-46b7-a041-49ee084d4ab1","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 14\"X10\" ND, BW, ASME B16.9",null,null,"59.3","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","True","Reducer",null,"5167"]
[null,"14\"x12\"","CPJRE","14","12.75","13","0","-1","D1,D2,L,E,OF,","52a4d656-14d7-580e-89bc-df1d3d536194","S1","14","in","14","BV",{"$nulls":7},"0","in","0fa282c7-5f38-45ba-be76-9ecee8de2b79","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 14\"X12\" ND, BW, ASME B16.9",null,null,"59.3","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"13","True","Reducer",null,"5169"]
[null,"16\"x8\"","CPJRE","16","8.625","14","0","-1","D1,D2,L,E,OF,","f3faae83-3bb5-59e4-a5b2-ddb7658ec124","S1","16","in","16","BV",{"$nulls":7},"0","in","2771979f-b71d-4178-b5bd-4746e238847c","S2","8","in","8.625","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 16\"X8\" ND, BW, ASME B16.9",null,null,"72.75","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","True","Reducer",null,"5171"]
[null,"16\"x10\"","CPJRE","16","10.75","14","0","-1","D1,D2,L,E,OF,","a1fe6d1d-5630-5e08-9ba1-486181492135","S1","16","in","16","BV",{"$nulls":7},"0","in","4c3743a5-df18-4949-86dc-4da4dc09b153","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 16\"X10\" ND, BW, ASME B16.9",null,null,"72.75","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","True","Reducer",null,"5173"]
[null,"16\"x12\"","CPJRE","16","12.75","14","0","-1","D1,D2,L,E,OF,","aea0c07d-02f4-5a05-b6e2-b8005d99e1c5","S1","16","in","16","BV",{"$nulls":7},"0","in","a4ac35ad-b180-48fe-9024-4c8f4345d6da","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 16\"X12\" ND, BW, ASME B16.9",null,null,"72.75","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","True","Reducer",null,"5175"]
[null,"16\"x14\"","CPJRE","16","14","14","0","-1","D1,D2,L,E,OF,","55a2edfa-03d2-5c92-af08-10f34465a329","S1","16","in","16","BV",{"$nulls":7},"0","in","4a4eaae7-2857-4c9c-84c3-d8038c6a6cbc","S2","14","in","14","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 16\"X14\" ND, BW, ASME B16.9",null,null,"72.75","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"14","True","Reducer",null,"5177"]
[null,"18\"x10\"","CPJRE","18","10.75","15","0","-1","D1,D2,L,E,OF,","80c44170-fd08-5c15-b894-ca1fc83f965b","S1","18","in","18","BV",{"$nulls":7},"0","in","a7094a35-fda6-4cac-a752-f5402d8e8fcf","S2","10","in","10.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 18\"X10\" ND, BW, ASME B16.9",null,null,"88.18","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","True","Reducer",null,"5179"]
[null,"18\"x12\"","CPJRE","18","12.75","15","0","-1","D1,D2,L,E,OF,","db4061ff-7619-57db-a805-424631056f29","S1","18","in","18","BV",{"$nulls":7},"0","in","a02f6185-e51f-4561-88d9-90ca2fb910c2","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 18\"X12\" ND, BW, ASME B16.9",null,null,"88.18","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","True","Reducer",null,"5181"]
[null,"18\"x14\"","CPJRE","18","14","15","0","-1","D1,D2,L,E,OF,","79b73ac4-e0dd-5453-ac4e-8815f31ec778","S1","18","in","18","BV",{"$nulls":7},"0","in","26d3332e-99fb-491f-abf5-be5b7e82bff1","S2","14","in","14","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 18\"X14\" ND, BW, ASME B16.9",null,null,"88.18","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","True","Reducer",null,"5183"]
[null,"18\"x16\"","CPJRE","18","16","15","0","-1","D1,D2,L,E,OF,","af5db36b-1dcb-532f-b0ea-d0f11a8b99ef","S1","18","in","18","BV",{"$nulls":7},"0","in","8ff55fb6-c6d1-4cc4-9f02-7df7dc4bdb30","S2","16","in","16","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 18\"X16\" ND, BW, ASME B16.9",null,null,"88.18","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"15","True","Reducer",null,"5185"]
[null,"20\"x12\"","CPJRE","20","12.75","20","0","-1","D1,D2,L,E,OF,","1bb44144-1dad-5aa2-8677-22529cb5389f","S1","20","in","20","BV",{"$nulls":7},"0","in","5bdc9032-001e-4659-a7d0-af960e77e848","S2","12","in","12.75","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 20\"X12\" ND, BW, ASME B16.9",null,null,"130.07","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5187"]
[null,"20\"x14\"","CPJRE","20","14","20","0","-1","D1,D2,L,E,OF,","fc3697bb-bb6e-5c87-b0b0-98d0c3a4939f","S1","20","in","20","BV",{"$nulls":7},"0","in","6cbbe778-af85-4b59-b0d1-4086ab2fdc71","S2","14","in","14","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 20\"X14\" ND, BW, ASME B16.9",null,null,"130.07","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5189"]
[null,"20\"x16\"","CPJRE","20","16","20","0","-1","D1,D2,L,E,OF,","acbce935-1a00-50ad-af91-8de6708fbc25","S1","20","in","20","BV",{"$nulls":7},"0","in","b3a27735-df27-4080-97ec-98e688474f49","S2","16","in","16","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 20\"X16\" ND, BW, ASME B16.9",null,null,"130.07","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5191"]
[null,"20\"x18\"","CPJRE","20","18","20","0","-1","D1,D2,L,E,OF,","0714aba8-29fe-58ef-85ca-3d86f8040e9f","S1","20","in","20","BV",{"$nulls":7},"0","in","4fc14f5b-5c0b-4a00-8be1-a0acbd1d369c","S2","18","in","18","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 20\"X18\" ND, BW, ASME B16.9",null,null,"130.07","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5193"]
[null,"24\"x16\"","CPJRE","24","16","20","0","-1","D1,D2,L,E,OF,","af13f1f2-2188-54dd-af77-c33db8ebb572","S1","24","in","24","BV",{"$nulls":7},"0","in","96b09c3a-1e40-4734-97b1-ce42759e69db","S2","16","in","16","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 24\"X16\" ND, BW, ASME B16.9",null,null,"158.73","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5204"]
[null,"24\"x18\"","CPJRE","24","18","20","0","-1","D1,D2,L,E,OF,","a478713e-5f8f-590a-b76c-e95004e3ce17","S1","24","in","24","BV",{"$nulls":7},"0","in","7f9e1d66-42da-46c1-8819-7636771e0f16","S2","18","in","18","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 24\"X18\" ND, BW, ASME B16.9",null,null,"158.73","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5206"]
[null,"24\"x20\"","CPJRE","24","20","20","0","-1","D1,D2,L,E,OF,","de5816f5-8a46-5b08-8557-02a4eca29245","S1","24","in","24","BV",{"$nulls":7},"0","in","45662a11-ddba-4016-a1ef-201037559624","S2","20","in","20","BV",{"$nulls":7},"0","in","REDUCER (ECC)","ASME B16.9",null,"REDUCER (ECC), BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","REDUCER (ECC), 24\"X20\" ND, BW, ASME B16.9",null,null,"158.73","LB","REBW","REDUCER","e8b2ac13-06fa-4059-bed7-e7b908443ca9","ae5694af-d465-4869-bf45-2abaf201e29a",{"$nulls":4},"2",null,"Fittings","TYPE=REDUCER-ECCENTRIC,SKEY=REBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"20","True","Reducer",null,"5208"]

{"sheet":"PIPE, SEAMLESS","index":28,"n_rows":18,"n_cols":56,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","L","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","UseFixedLength","CutLength","LinearWeight","LinearWeightUnit","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","L","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Fixed Length","Use Fixed Length","Cut Length","Linear Weight","Linear Weight Unit","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPP","0.84","-1","-1","D,L,OF,","b1d9050c-3a3f-5211-b92f-5f07c281e395","ALL","0.5","in","0.84","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 1/2\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"0.85","LB/FT","Pipe",null,"4973"]
[null,"3/4\"","CPP","1.05","-1","-1","D,L,OF,","807e72e2-6db5-5ce7-b21b-b68f8e44b293","ALL","0.75","in","1.05","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 3/4\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"1.13","LB/FT","Pipe",null,"4975"]
[null,"1\"","CPP","1.315","-1","-1","D,L,OF,","8b800c61-bc01-576f-a8d0-2db59b9bf064","ALL","1","in","1.315","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 1\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"1.68","LB/FT","Pipe",null,"4977"]
[null,"1 1/2\"","CPP","1.9","-1","-1","D,L,OF,","2684a27f-9448-53e9-a9c5-d91f7d6a63e1","ALL","1.5","in","1.9","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 1 1/2\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"2.72","LB/FT","Pipe",null,"4981"]
[null,"2\"","CPP","2.375","-1","-1","D,L,OF,","3bc22516-7836-5e20-81e0-97437daf5166","ALL","2","in","2.375","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 2\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"3.66","LB/FT","Pipe",null,"4983"]
[null,"3\"","CPP","3.5","-1","-1","D,L,OF,","958ad30c-4022-50ed-bccb-07e3e3c19f72","ALL","3","in","3.5","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 3\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"7.58","LB/FT","Pipe",null,"4987"]
[null,"4\"","CPP","4.5","-1","-1","D,L,OF,","3f9c9ca5-8e15-5eae-acc5-5c2b34718a39","ALL","4","in","4.5","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 4\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"10.8","LB/FT","Pipe",null,"4991"]
[null,"6\"","CPP","6.625","-1","-1","D,L,OF,","7b9daa32-8d2a-5338-ac91-12253be5ad8f","ALL","6","in","6.625","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 6\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"18.99","LB/FT","Pipe",null,"4995"]
[null,"8\"","CPP","8.625","-1","-1","D,L,OF,","bace49c4-5dc0-5eac-b7ec-7dfa22c29386","ALL","8","in","8.625","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 8\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"28.58","LB/FT","Pipe",null,"4997"]
[null,"10\"","CPP","10.75","-1","-1","D,L,OF,","11a45713-2ef0-5018-bf1b-d02032683c79","ALL","10","in","10.75","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 10\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"40.52","LB/FT","Pipe",null,"4999"]
[null,"12\"","CPP","12.75","-1","-1","D,L,OF,","5c08e063-e407-56eb-b723-863361aab952","ALL","12","in","12.75","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 12\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"49.61","LB/FT","Pipe",null,"5002"]
[null,"14\"","CPP","14","-1","-1","D,L,OF,","0f5128cb-d2b6-58b0-a480-be5ab273ddb2","ALL","14","in","14","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 14\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"54.62","LB/FT","Pipe",null,"5004"]
[null,"16\"","CPP","16","-1","-1","D,L,OF,","45adedd4-949a-5587-a021-47bc15442b92","ALL","16","in","16","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 16\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"62.64","LB/FT","Pipe",null,"5006"]
[null,"18\"","CPP","18","-1","-1","D,L,OF,","453a4906-38a4-5d25-97b7-ac8baa0b9037","ALL","18","in","18","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 18\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"70.65","LB/FT","Pipe",null,"5008"]
[null,"20\"","CPP","20","-1","-1","D,L,OF,","c238bfa9-f11d-55fb-80b9-5c7253a10f9f","ALL","20","in","20","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 20\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"78.67","LB/FT","Pipe",null,"5010"]
[null,"24\"","CPP","24","-1","-1","D,L,OF,","f3ec9aa1-954f-5d76-8fa6-0b3293ad6842","ALL","24","in","24","PL",{"$nulls":7},"0","in","Pipe, Seamless","ASME B36.10",null,"PIPE, SEAMLESS, PE, ASME B36.10, ASTM A106 Gr B SMLS, Sch 40","PIPE, SEAMLESS, 24\" ND, PE, ASME B36.10",null,null,null,"LB",null,"PIPE","3516703d-50ea-454a-b39d-8c70b492f0c3","c12271bf-ca35-4a55-8d2f-95fda9f7b86f",{"$nulls":4},"2",null,"Pipe","TYPE=PIPE",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"0","False",null,"94.71","LB/FT","Pipe",null,"5014"]

{"sheet":"SOCKOLET","index":29,"n_rows":62,"n_cols":74,"rows_kept":62,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","L","D2","W","A","L1","I","OF","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PartSubType","Length","CurveRadius","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","L","D2","W","A","L1","I","OF","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Part Subtype","Length","Curve Radius","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"2\"x1/2\"","CPNS_W_OF","0.84","0.625","2.375","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","ad610fc4-615f-5ea0-b433-8482b4277a06","S1","2","in","2.375","BV",{"$nulls":4},"3000",null,null,"0","in","ca5d8f12-e3ab-4157-b931-e5842d9125d9","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 2\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7477"]
[null,"2\"x3/4\"","CPNS_W_OF","1.05","0.5625","2.375","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","a9344d99-63a1-5e46-974a-aec545b8c7a8","S1","2","in","2.375","BV",{"$nulls":4},"3000",null,null,"0","in","a66785a3-b704-4703-9a7c-c6b26053a6ff","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 2\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7479"]
[null,"2\"x1\"","CPNS_W_OF","1.315","0.8125","2.375","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","b43342ec-6c21-5e2d-9690-d2a01a603f7d","S1","2","in","2.375","BV",{"$nulls":4},"3000",null,null,"0","in","fdd556f9-eb49-4028-82a1-e778f1bc5cef","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 2\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7481"]
[null,"2\"x1 1/2\"","CPNS_W_OF","1.9","0.875","2.375","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","a745a8a2-9c1e-5f90-a8b6-643156a429f7","S1","2","in","2.375","BV",{"$nulls":4},"3000",null,null,"0","in","5c6e0d02-f3fd-4e2c-9ad4-462a236a70ea","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 2\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7485"]
[null,"2\"","CPNS_W_OF","2.375","0.875","2.375","3.5","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","26f80105-7856-5f2b-9ed4-d6c53ce69932","S1","2","in","2.375","BV",{"$nulls":4},"3000",null,null,"0","in","7ee3d0b2-6079-4e1c-ab71-343bc0f53d88","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 2\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7487"]
[null,"3\"x1/2\"","CPNS_W_OF","0.84","0.625","3.5","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","ea4de034-ac8f-5300-b646-efaaf16667a8","S1","3","in","3.5","BV",{"$nulls":4},"3000",null,null,"0","in","93525448-ac2c-46f7-9994-78e78724309a","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 3\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7516"]
[null,"3\"x3/4\"","CPNS_W_OF","1.05","0.5625","3.5","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","0c2e31c1-0925-505c-9bdf-2796aa64cc08","S1","3","in","3.5","BV",{"$nulls":4},"3000",null,null,"0","in","3ff810e1-10da-4136-b2c7-ef7b9bc6cafd","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 3\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7518"]
[null,"3\"x1\"","CPNS_W_OF","1.315","0.8125","3.5","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","74587390-a7e2-5389-8ee2-9cdd359b6d05","S1","3","in","3.5","BV",{"$nulls":4},"3000",null,null,"0","in","36b0ddd4-dfb6-424d-b45b-df6895f53034","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 3\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7520"]
[null,"3\"x1 1/2\"","CPNS_W_OF","1.9","0.875","3.5","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","b1e66096-8e0e-59b7-b99f-e5e240b89203","S1","3","in","3.5","BV",{"$nulls":4},"3000",null,null,"0","in","1f1387b9-bcc7-431d-9b6a-33c239c45ed0","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 3\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7524"]
[null,"3\"x2\"","CPNS_W_OF","2.375","0.875","3.5","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","2d1f26e3-9ab6-54d6-973c-0fb39e3801c8","S1","3","in","3.5","BV",{"$nulls":4},"3000",null,null,"0","in","182fc46c-9114-460c-9254-cb76188d095f","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 3\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7526"]
[null,"4\"x1/2\"","CPNS_W_OF","0.84","0.625","4.5","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","fd28081d-ef7b-5e07-ada4-d1ac760e16b7","S1","4","in","4.5","BV",{"$nulls":4},"3000",null,null,"0","in","a8cae131-66a3-4a0c-91a4-9d4842633b63","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 4\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7560"]
[null,"4\"x3/4\"","CPNS_W_OF","1.05","0.5625","4.5","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","88e14ca5-9738-5791-8dac-e0bb333e4d34","S1","4","in","4.5","BV",{"$nulls":4},"3000",null,null,"0","in","d035d246-b2de-4997-a0cc-f7ec507275a9","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 4\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7562"]
[null,"4\"x1\"","CPNS_W_OF","1.315","0.8125","4.5","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","60c9c5be-d212-50c4-a0af-0f489dd4dfc6","S1","4","in","4.5","BV",{"$nulls":4},"3000",null,null,"0","in","f165f2b8-3037-4638-92d8-df3b0206ebeb","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 4\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7564"]
[null,"4\"x1 1/2\"","CPNS_W_OF","1.9","0.875","4.5","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","c8d22ee1-4b97-51f5-87d1-491ce69748ce","S1","4","in","4.5","BV",{"$nulls":4},"3000",null,null,"0","in","e7a26864-fc1a-446a-9860-c11f4fe0049c","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 4\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7568"]
[null,"4\"x2\"","CPNS_W_OF","2.375","0.875","4.5","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","fee10ede-d56d-5842-b02d-b3ec65f2106c","S1","4","in","4.5","BV",{"$nulls":4},"3000",null,null,"0","in","9651b3a0-bb5f-42ab-8eed-0df94c8fa36f","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 4\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7570"]
[null,"6\"x1/2\"","CPNS_W_OF","0.84","0.625","6.625","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","0721a8f0-710d-5621-b14c-f0f8ef92f2bc","S1","6","in","6.625","BV",{"$nulls":4},"3000",null,null,"0","in","546567e4-053b-4cf9-97c0-074fe2ff412c","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 6\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7609"]
[null,"6\"x3/4\"","CPNS_W_OF","1.05","0.5625","6.625","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","4e0f932c-5cd0-53c5-a141-117e2f84bc7a","S1","6","in","6.625","BV",{"$nulls":4},"3000",null,null,"0","in","5cd72b2a-e2ec-4e53-9de6-6b2ad3a35067","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 6\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7611"]
[null,"6\"x1\"","CPNS_W_OF","1.315","0.8125","6.625","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","67f7bced-24fa-5987-98d3-caa4827dc89c","S1","6","in","6.625","BV",{"$nulls":4},"3000",null,null,"0","in","e4cd54a0-cc26-4000-b4f5-b4af4697453f","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 6\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7613"]
[null,"6\"x1 1/2\"","CPNS_W_OF","1.9","0.875","6.625","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","d738d60a-51ce-55b3-85c9-cc0d0b5f289f","S1","6","in","6.625","BV",{"$nulls":4},"3000",null,null,"0","in","866791cb-86fc-49e8-8fe9-bd8e340fd8c2","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 6\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7617"]
[null,"6\"x2\"","CPNS_W_OF","2.375","0.875","6.625","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","7830110d-6061-5c82-8438-dcba401f7c9b","S1","6","in","6.625","BV",{"$nulls":4},"3000",null,null,"0","in","e2c2b4fa-b829-4444-8fb7-3956e3946b9d","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 6\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7619"]
[null,"8\"x1/2\"","CPNS_W_OF","0.84","0.625","8.625","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","9c525029-cd08-539c-90a6-847f6fe2062c","S1","8","in","8.625","BV",{"$nulls":4},"3000",null,null,"0","in","4e2f0b03-a826-40ea-9f7e-d8702fa9e194","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 8\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7633"]
[null,"8\"x3/4\"","CPNS_W_OF","1.05","0.5625","8.625","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","c85af750-895b-5aaa-ac2d-e8968d1683d7","S1","8","in","8.625","BV",{"$nulls":4},"3000",null,null,"0","in","1c479d7a-54f2-4c40-97dc-ef4dd192acf6","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 8\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7635"]
[null,"8\"x1\"","CPNS_W_OF","1.315","0.8125","8.625","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","0327b5de-d9ef-562b-9e5d-5d734c9e3ca6","S1","8","in","8.625","BV",{"$nulls":4},"3000",null,null,"0","in","93e5e76f-1ecf-4e0f-b4f4-946db88c0439","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 8\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7637"]
[null,"8\"x1 1/2\"","CPNS_W_OF","1.9","0.875","8.625","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","0d8e0033-8f74-50ee-90a7-d84c514c15fe","S1","8","in","8.625","BV",{"$nulls":4},"3000",null,null,"0","in","6e477c96-d5aa-4335-a43c-e329f1e4b011","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 8\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7641"]
[null,"8\"x2\"","CPNS_W_OF","2.375","0.875","8.625","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","51e735ad-0606-52c5-b53e-1ab3936e54cf","S1","8","in","8.625","BV",{"$nulls":4},"3000",null,null,"0","in","0571b634-e8a2-4e28-9252-5641992bbc3a","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 8\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7643"]
[null,"10\"x1/2\"","CPNS_W_OF","0.84","0.625","10.75","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","eee682e3-3d21-5802-b246-2c27518e5296","S1","10","in","10.75","BV",{"$nulls":4},"3000",null,null,"0","in","fbab96a7-f70a-489a-863d-192c7935b74d","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 10\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7657"]
[null,"10\"x3/4\"","CPNS_W_OF","1.05","0.5625","10.75","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","c15b06ce-cacc-59b5-8d0c-fb959387136d","S1","10","in","10.75","BV",{"$nulls":4},"3000",null,null,"0","in","d07f5ca7-26db-4677-a365-dc01b95047dd","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 10\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7659"]
[null,"10\"x1\"","CPNS_W_OF","1.315","0.8125","10.75","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","298eb045-7230-51e9-92fc-da661d858996","S1","10","in","10.75","BV",{"$nulls":4},"3000",null,null,"0","in","3c8e3e4a-dbcf-4bb2-9927-75aff2537605","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 10\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7661"]
[null,"10\"x1 1/2\"","CPNS_W_OF","1.9","0.875","10.75","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","2d9911da-5979-570c-852e-bbf5d3395e4c","S1","10","in","10.75","BV",{"$nulls":4},"3000",null,null,"0","in","e35c61a1-9655-473d-bfd4-2e104ea53e08","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 10\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7665"]
[null,"10\"x2\"","CPNS_W_OF","2.375","0.875","10.75","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","44794930-8464-5236-bbee-b1561942c66b","S1","10","in","10.75","BV",{"$nulls":4},"3000",null,null,"0","in","108a5e53-5456-462f-8703-e79ee32c5bfd","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 10\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7667"]
[null,"12\"x1/2\"","CPNS_W_OF","0.84","0.625","12.75","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","51751404-946e-58d5-b8b2-19e04a5e1436","S1","12","in","12.75","BV",{"$nulls":4},"3000",null,null,"0","in","a17a6477-7093-4240-af2e-8499b2fb5775","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 12\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7681"]
[null,"12\"x3/4\"","CPNS_W_OF","1.05","0.5625","12.75","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","c63eceb6-1462-54f0-b1f9-1c034966ae99","S1","12","in","12.75","BV",{"$nulls":4},"3000",null,null,"0","in","828ce5eb-7b7f-4baa-a363-9751e06edc81","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 12\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7683"]
[null,"12\"x1\"","CPNS_W_OF","1.315","0.8125","12.75","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","511fc4ef-44e7-5dcf-9966-d5ee61b10020","S1","12","in","12.75","BV",{"$nulls":4},"3000",null,null,"0","in","fa2162e4-dc2a-45e1-abae-23b9c91c8aef","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 12\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7685"]
[null,"12\"x1 1/2\"","CPNS_W_OF","1.9","0.875","12.75","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","6b1f84ab-0cff-5211-9f1e-becd07f41ed3","S1","12","in","12.75","BV",{"$nulls":4},"3000",null,null,"0","in","61faad76-fb49-4fbd-98a4-9412c291fe6d","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 12\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7689"]
[null,"12\"x2\"","CPNS_W_OF","2.375","0.875","12.75","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","3345ee08-0e67-5982-acea-569095721dea","S1","12","in","12.75","BV",{"$nulls":4},"3000",null,null,"0","in","cc8c5c53-c574-4a38-8dd0-f8c7299f014e","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 12\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7691"]
[null,"14\"x1/2\"","CPNS_W_OF","0.84","0.625","14","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","ed09f9c1-6942-5acf-a92a-490daaae5947","S1","14","in","14","BV",{"$nulls":4},"3000",null,null,"0","in","94ea2ff8-1e5f-4ad0-a014-5c9d58d0b4ef","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 14\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7706"]
[null,"14\"x3/4\"","CPNS_W_OF","1.05","0.5625","14","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","83e64441-306e-50ee-8e85-f2d96cfad671","S1","14","in","14","BV",{"$nulls":4},"3000",null,null,"0","in","91cb9895-b5d1-4ba3-9e73-5d6c0a3f5ab5","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 14\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7708"]
[null,"14\"x1\"","CPNS_W_OF","1.315","0.8125","14","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","9c627c78-721b-5e68-b99d-eca94ac84c79","S1","14","in","14","BV",{"$nulls":4},"3000",null,null,"0","in","0fbbe86c-e521-41f5-a908-fafd3c7fb82b","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 14\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7710"]
[null,"14\"x1 1/2\"","CPNS_W_OF","1.9","0.875","14","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","8f2ee6f8-0d7d-5dce-ab6c-cda928a1380e","S1","14","in","14","BV",{"$nulls":4},"3000",null,null,"0","in","bc2b04db-d1a7-4903-bbd3-aa0ec596adac","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 14\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7714"]
[null,"14\"x2\"","CPNS_W_OF","2.375","0.875","14","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","776925f4-4955-5a26-a5f2-05c53caf7ad0","S1","14","in","14","BV",{"$nulls":4},"3000",null,null,"0","in","dfcdddb7-9861-4a5d-9ac2-3773fd0f6ef6","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 14\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7716"]
[null,"16\"x1/2\"","CPNS_W_OF","0.84","0.625","16","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","4b11b0ff-eaf0-5a0f-b55d-dd8169c9b4ed","S1","16","in","16","BV",{"$nulls":4},"3000",null,null,"0","in","8af6e584-8914-43b5-a874-0fb0a66b5a54","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 16\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7730"]
[null,"16\"x3/4\"","CPNS_W_OF","1.05","0.5625","16","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","9f3d2aaf-96df-5766-9579-b46af7ef6faf","S1","16","in","16","BV",{"$nulls":4},"3000",null,null,"0","in","3d16d623-4587-4007-8b8e-c8093e0d0861","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 16\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7732"]
[null,"16\"x1\"","CPNS_W_OF","1.315","0.8125","16","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","e2d61112-b79b-5a79-8841-757573ec6292","S1","16","in","16","BV",{"$nulls":4},"3000",null,null,"0","in","f9f3ea7c-805c-450a-8a51-9774a48155b2","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 16\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7734"]
[null,"16\"x1 1/2\"","CPNS_W_OF","1.9","0.875","16","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","b7c149e0-2fd7-500f-9684-6307b2199422","S1","16","in","16","BV",{"$nulls":4},"3000",null,null,"0","in","35d99b12-88d7-43fb-b52d-8d7749c78137","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 16\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7738"]
[null,"16\"x2\"","CPNS_W_OF","2.375","0.875","16","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","d0c89257-5b98-5bb7-a31d-8987f011412a","S1","16","in","16","BV",{"$nulls":4},"3000",null,null,"0","in","89473f6a-3f10-4505-bc9c-8b240cb124c0","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 16\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7740"]
[null,"18\"x1/2\"","CPNS_W_OF","0.84","0.625","18","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","7a407a73-9d8c-535c-ad69-45a699d9a63c","S1","18","in","18","BV",{"$nulls":4},"3000",null,null,"0","in","b738b6ff-d9b1-42a0-ad84-9e809cfaca33","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 18\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7754"]
[null,"18\"x3/4\"","CPNS_W_OF","1.05","0.5625","18","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","608f52ef-9962-53ed-9fbf-cda5e54bdbd1","S1","18","in","18","BV",{"$nulls":4},"3000",null,null,"0","in","1c5aef74-4438-4d93-a9d2-c7c3d1fb0147","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 18\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7756"]
[null,"18\"x1\"","CPNS_W_OF","1.315","0.8125","18","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","cdf7165a-5b31-5abe-8c06-3a185c3b25b5","S1","18","in","18","BV",{"$nulls":4},"3000",null,null,"0","in","cea3435d-e61c-4500-b7bc-db2219f74054","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 18\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7758"]
[null,"18\"x1 1/2\"","CPNS_W_OF","1.9","0.875","18","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","d4c02ab3-e2ed-5065-bbbc-52b8622ad5bb","S1","18","in","18","BV",{"$nulls":4},"3000",null,null,"0","in","b39fecff-cbb4-4530-8781-77d9f60a77eb","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 18\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7762"]
[null,"18\"x2\"","CPNS_W_OF","2.375","0.875","18","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","f963c237-3133-5d68-a581-9cd608fa1de1","S1","18","in","18","BV",{"$nulls":4},"3000",null,null,"0","in","01de2816-a346-4b63-99ce-9f3fe03d49f1","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 18\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7764"]
[null,"20\"x1/2\"","CPNS_W_OF","0.84","0.625","20","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","0358c00f-88ae-5887-8d96-4e1a2e2a4bdc","S1","20","in","20","BV",{"$nulls":4},"3000",null,null,"0","in","d5ccc23e-2e73-42ed-87dc-3d1b3175a4b5","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 20\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7778"]
[null,"20\"x3/4\"","CPNS_W_OF","1.05","0.5625","20","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","d24420b1-705a-5f1d-a9a9-7349f24d87a1","S1","20","in","20","BV",{"$nulls":4},"3000",null,null,"0","in","bb5eb894-6f3d-4b0e-a620-697c8f6a70cf","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 20\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7780"]
[null,"20\"x1\"","CPNS_W_OF","1.315","0.8125","20","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","609ec1ea-6981-5b9d-aca1-931ba4275390","S1","20","in","20","BV",{"$nulls":4},"3000",null,null,"0","in","e0dbae43-62aa-4d1e-b287-0c1220ddd989","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 20\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7782"]
[null,"20\"x1 1/2\"","CPNS_W_OF","1.9","0.875","20","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","4d5eeaf5-029e-569c-a60d-660710979ebb","S1","20","in","20","BV",{"$nulls":4},"3000",null,null,"0","in","b34d319a-5361-4fdd-8854-7c046e676192","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 20\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7786"]
[null,"20\"x2\"","CPNS_W_OF","2.375","0.875","20","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","a543a49e-edd0-5a37-8801-c7d4b827e460","S1","20","in","20","BV",{"$nulls":4},"3000",null,null,"0","in","0ea37777-9d70-4ddc-995b-42aa2f3121e2","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 20\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7788"]
[null,"24\"x1/2\"","CPNS_W_OF","0.84","0.625","24","1.40625","90","0.375","0.375","0","D,L,D2,W,A,L1,I,OF,","b31265e3-06b9-575e-b51b-7b890f949238","S1","24","in","24","BV",{"$nulls":4},"3000",null,null,"0","in","6c7e5079-1306-4ce4-9f8f-020600084f0d","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.375","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 24\"X1/2\" ND, 3000 LB, BWXSW, 5/8\" LG, ASME B16.11",null,null,"0.26","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.625",null,"Olet",null,"7827"]
[null,"24\"x3/4\"","CPNS_W_OF","1.05","0.5625","24","1.71875","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","34a78e97-a93a-5889-9946-ba3848cafe34","S1","24","in","24","BV",{"$nulls":4},"3000",null,null,"0","in","0301942b-fb28-420d-9033-21490bd0fb1c","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 24\"X3/4\" ND, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11",null,null,"0.3","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.5625",null,"Olet",null,"7829"]
[null,"24\"x1\"","CPNS_W_OF","1.315","0.8125","24","2","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","d12e2a1c-899b-5eb5-b856-f963cb52cb90","S1","24","in","24","BV",{"$nulls":4},"3000",null,null,"0","in","07bf110e-e41c-4106-b247-f112915e3eaf","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 24\"X1\" ND, 3000 LB, BWXSW, 13/16\" LG, ASME B16.11",null,null,"0.54","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.8125",null,"Olet",null,"7831"]
[null,"24\"x1 1/2\"","CPNS_W_OF","1.9","0.875","24","2.84375","90","0.5","0.5","0","D,L,D2,W,A,L1,I,OF,","6f1030e0-1d4f-5568-b382-d710fe7a8823","S1","24","in","24","BV",{"$nulls":4},"3000",null,null,"0","in","9a849041-e77c-4c6b-b629-65e0b7a36070","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 24\"X1 1/2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"0.96","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7835"]
[null,"24\"x2\"","CPNS_W_OF","2.375","0.875","24","3.46875","90","0.625","0.625","0","D,L,D2,W,A,L1,I,OF,","e44fb039-f259-5c9f-a061-ba91ee0e5434","S1","24","in","24","BV",{"$nulls":4},"3000",null,null,"0","in","c80451b2-9ca6-4212-9095-6a776122aa63","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.625","in","SOCKOLET","ASME B16.11",null,"SOCKOLET, 3000 LB, BWXSW, 9/16\" LG, ASME B16.11, ASTM A105","SOCKOLET, 24\"X2\" ND, 3000 LB, BWXSW, 7/8\" LG, ASME B16.11",null,null,"1.49","LB","SKSW","OLET","fd5b02eb-e3bd-4696-a593-a0e3ae9c8343","5be2661a-6271-4fd5-9c1a-5c835a60b21c",{"$nulls":4},"2",null,"Olet","TYPE=OLET,SKEY=SKSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Sockolet","0.875",null,"Olet",null,"7837"]

{"sheet":"GASKET","index":30,"n_rows":18,"n_cols":51,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPMGP","1.38","0.84","0.0625","D1,D2,L,","575abaea-a28b-5fa7-a317-3d2b95c8ea3c","ALL","0.5","in","0.84","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 1/2\" ND, 150 LB",null,null,"0","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1409"]
[null,"3/4\"","CPMGP","1.69","1.05","0.0625","D1,D2,L,","07c109a1-1397-59ec-8934-42a513207289","ALL","0.75","in","1.05","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 3/4\" ND, 150 LB",null,null,"0.01","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1411"]
[null,"1\"","CPMGP","2","1.315","0.0625","D1,D2,L,","30ec2726-d1bd-500a-b8c8-ff24f797a505","ALL","1","in","1.315","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 1\" ND, 150 LB",null,null,"0.01","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1413"]
[null,"1 1/2\"","CPMGP","2.88","1.9","0.0625","D1,D2,L,","7a3ace45-a9c6-535b-8d18-129ffddf9afc","ALL","1.5","in","1.9","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 1 1/2\" ND, 150 LB",null,null,"0.02","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1415"]
[null,"2\"","CPMGP","3.62","2.375","0.0625","D1,D2,L,","3734d3e6-51ba-5a4d-bb51-868acd5fb0db","ALL","2","in","2.375","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 2\" ND, 150 LB",null,null,"0.03","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1417"]
[null,"3\"","CPMGP","5","3.5","0.0625","D1,D2,L,","3e3bbbef-d8c0-5de2-a84e-d0f3ff43275a","ALL","3","in","3.5","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 3\" ND, 150 LB",null,null,"0.04","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1419"]
[null,"4\"","CPMGP","6.19","4.5","0.0625","D1,D2,L,","153c977f-4897-597b-834c-8468c1f83e3d","ALL","4","in","4.5","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 4\" ND, 150 LB",null,null,"0.06","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1421"]
[null,"6\"","CPMGP","8.5","6.625","0.0625","D1,D2,L,","8f40accc-76d1-5217-b041-b35c9cf705dc","ALL","6","in","6.625","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 6\" ND, 150 LB",null,null,"0.1","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1423"]
[null,"8\"","CPMGP","10.62","8.625","0.0625","D1,D2,L,","7e193faf-65c7-5c81-bc57-3083164e29dc","ALL","8","in","8.625","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 8\" ND, 150 LB",null,null,"0.13","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1425"]
[null,"10\"","CPMGP","12.75","10.75","0.0625","D1,D2,L,","c148c0b7-13a5-55ff-92a0-2ff20b670638","ALL","10","in","10.75","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 10\" ND, 150 LB",null,null,"0.16","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1427"]
[null,"12\"","CPMGP","15","12.75","0.0625","D1,D2,L,","9791adec-4eef-529c-9c66-ebb084f05cb6","ALL","12","in","12.75","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 12\" ND, 150 LB",null,null,"0.21","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1429"]
[null,"14\"","CPMGP","16.25","14","0.0625","D1,D2,L,","87aaa668-9b0d-5af7-aec5-e332d874b011","ALL","14","in","14","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 14\" ND, 150 LB",null,null,"0.23","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1431"]
[null,"16\"","CPMGP","18.5","16","0.0625","D1,D2,L,","3563be77-7f22-5fef-a85c-94fe6be9ac88","ALL","16","in","16","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 16\" ND, 150 LB",null,null,"0.3","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1433"]
[null,"18\"","CPMGP","21","18","0.0625","D1,D2,L,","d2fe8258-1328-52a2-9e85-43fd822238b5","ALL","18","in","18","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 18\" ND, 150 LB",null,null,"0.4","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1435"]
[null,"20\"","CPMGP","23","20","0.0625","D1,D2,L,","9b86b309-c2cd-5c49-b712-3bc30630f022","ALL","20","in","20","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 20\" ND, 150 LB",null,null,"0.44","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1437"]
[null,"24\"","CPMGP","27.25","24","0.0625","D1,D2,L,","0842a52e-244a-55d3-bff9-05009501f5dd","ALL","24","in","24","Undefined_ET",{"$nulls":4},"150",null,"0","0","in","GASKET",null,null,"GASKET, 150 LB, CS/PTFE","GASKET, 24\" ND, 150 LB",null,null,"0.57","LB",null,"GASKET","bdaf03b4-64ed-485d-8bf3-7332b829a847","3dd31140-b6d1-463f-88b8-e4696eec1f64",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1439"]

{"sheet":"GASKET, SWG","index":31,"n_rows":21,"n_cols":51,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D1","D2","L","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D1","D2","L","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPMGP","1.8800","0.5600","0.1250","D1,D2,L,","479af779-1431-5624-913c-4a0af67569ba","ALL","0.5","in","0.84","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 1/2\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.06","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1370"]
[null,"3/4\"","CPMGP","2.2500","0.8100","0.1250","D1,D2,L,","7a1e8848-793b-59c6-9c55-eaae57cd41eb","ALL","0.75","in","1.05","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 3/4\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.08","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1372"]
[null,"1\"","CPMGP","2.6300","1.0600","0.1250","D1,D2,L,","592cc95d-f015-5a1a-b604-8d8a6fc6b5bb","ALL","1","in","1.315","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 1\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.11","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1374"]
[null,"1 1/4\"","CPMGP","3.0000","1.5000","0.1250","D1,D2,L,","3d3500dc-9478-5cc9-b715-ce38450904d6","ALL","1.25","in","1.66","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 1 1/4\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.13","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1376"]
[null,"1 1/2\"","CPMGP","3.3800","1.7500","0.1250","D1,D2,L,","7174d646-5be2-5837-89e5-341b75e48e9c","ALL","1.5","in","1.9","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 1 1/2\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.17","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1378"]
[null,"2\"","CPMGP","4.1300","2.1900","0.1250","D1,D2,L,","3f0bb1b9-373e-5402-9bfe-004d035ba9fe","ALL","2","in","2.375","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 2\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.24","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1380"]
[null,"2 1/2\"","CPMGP","4.8800","2.6200","0.1250","D1,D2,L,","101fcde4-525d-5cb7-85ab-e0f2a26fed7a","ALL","2.5","in","2.875","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 2 1/2\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.33","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1382"]
[null,"3\"","CPMGP","5.3800","3.1900","0.1250","D1,D2,L,","f988cb4f-d06e-5871-b8c5-24b52ee518dc","ALL","3","in","3.5","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 3\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.41","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1384"]
[null,"4\"","CPMGP","6.8800","4.1900","0.1250","D1,D2,L,","0e40527b-b867-5e7a-895a-f24f2d84f001","ALL","4","in","4.5","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 4\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"0.7","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1386"]
[null,"5\"","CPMGP","7.7500","5.1900","0.1250","D1,D2,L,","a8739c7e-f120-5052-9c6c-51ba90c1e32f","ALL","5","in","5.5625","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 5\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"1.1","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1388"]
[null,"6\"","CPMGP","8.7500","6.1900","0.1250","D1,D2,L,","2d95cbc4-4094-56a5-abfa-354cf531b9f5","ALL","6","in","6.625","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 6\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"1.23","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1390"]
[null,"8\"","CPMGP","11.0000","8.5000","0.1250","D1,D2,L,","1a0e9463-7984-506b-af17-b13aa28232bd","ALL","8","in","8.625","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 8\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"1.6","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1392"]
[null,"10\"","CPMGP","13.3800","10.5600","0.1250","D1,D2,L,","a57993ea-afe7-5f04-934f-475bb8e7f7c9","ALL","10","in","10.75","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 10\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"2.51","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1394"]
[null,"12\"","CPMGP","16.1300","12.5000","0.1250","D1,D2,L,","cffd1300-3a18-5914-8782-8a7e45052cf9","ALL","12","in","12.75","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 12\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"3.1","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1396"]
[null,"14\"","CPMGP","17.7500","13.7500","0.1250","D1,D2,L,","b0eb96e7-aba3-5e6a-a43e-57a4419f57cb","ALL","14","in","14","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 14\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"3.46","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1398"]
[null,"16\"","CPMGP","20.2500","15.7500","0.1250","D1,D2,L,","a647aa56-1576-522e-bc8f-0f8a7d9b1591","ALL","16","in","16","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 16\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"4.62","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1401"]
[null,"18\"","CPMGP","21.6300","17.6900","0.1250","D1,D2,L,","be1e1877-e026-5e5f-a701-840f7c53bd27","ALL","18","in","18","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 18\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"5.09","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1403"]
[null,"20\"","CPMGP","23.8800","19.6900","0.1250","D1,D2,L,","ff5d18a5-3a7e-55f7-a9b5-868d237ec9c8","ALL","20","in","20","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 20\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"6.32","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1405"]
[null,"24\"","CPMGP","28.2500","23.7500","0.1250","D1,D2,L,","c84e2643-b9bd-5b90-86c1-990406504cde","ALL","24","in","24","Undefined_ET",null,null,"RF",null,"150",null,null,null,"in","Gasket, SWG","ASME B16.20",null,"GASKET, SWG, 1/8\" THK, RF, 150 LB, ASME B16.20, CS/PTFE","GASKET, SWG, 24\" ND, 1/8\" THK, 150 LB, RF, ASME B16.20",null,null,"7.84","LB",null,"GASKET","6a0fb215-91a6-43c8-a8a2-102ae912484a","2f57173b-d74a-44c4-a9db-e8c166b63da8",{"$nulls":4},"2",null,"Fasteners","TYPE=GASKET",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Gasket",null,"1407"]

{"sheet":"FLANGE WN","index":32,"n_rows":13,"n_cols":68,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","L","B","D1","D2","D3","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","L","B","D1","D2","D3","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPFWR","2.75","0.94","7.5","3.5","4.25","L,B,D1,D2,D3,","48fc6c21-d39b-59cc-9611-ea8367376331","S1","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,null,"in","155ade0d-ce53-4c36-9108-e2cbfdb20f27","S2","3","in","3.5","BV",null,null,null,"0.94",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 3\" ND, 150 LB, RF, ASME B16.5",null,null,"11.5","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1308"]
[null,"4\"","CPFWR","3","0.94","9","4.5","5.31","L,B,D1,D2,D3,","6f58ecf1-f454-5a40-9780-c8552300e99f","S1","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,null,"in","a7968d29-de0c-432d-ac14-b695f09478ed","S2","4","in","4.5","BV",null,null,null,"0.94",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 4\" ND, 150 LB, RF, ASME B16.5",null,null,"16.5","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1312"]
[null,"6\"","CPFWR","3.5","1","11","6.625","7.56","L,B,D1,D2,D3,","db1313e4-fe7d-55f8-adb3-6158e31cb6ff","S1","6","in","6.625","FL",null,null,"RF","1","150",null,null,null,"in","916c6c79-1eb0-4880-9c70-c41c0c750d39","S2","6","in","6.625","BV",null,null,null,"1",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 6\" ND, 150 LB, RF, ASME B16.5",null,null,"26","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1316"]
[null,"8\"","CPFWR","4","1.12","13.5","8.625","9.69","L,B,D1,D2,D3,","0ce98db6-74cc-582f-8ee3-a5d335c24593","S1","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,null,"in","37386977-2a5e-4a68-8840-b6941a9370cf","S2","8","in","8.625","BV",null,null,null,"1.12",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 8\" ND, 150 LB, RF, ASME B16.5",null,null,"42","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1318"]
[null,"10\"","CPFWR","4","1.18","16","10.75","12","L,B,D1,D2,D3,","087d0ed2-4096-5827-a4e2-76f89ad7f090","S1","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,null,"in","1cdbe745-1c97-4294-a6c6-bfd710dcd056","S2","10","in","10.75","BV",null,null,null,"1.18",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 10\" ND, 150 LB, RF, ASME B16.5",null,null,"54","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1320"]
[null,"12\"","CPFWR","4.5","1.25","19","12.75","14.38","L,B,D1,D2,D3,","91d3349a-3b42-5736-a2f9-dc8d9c198e05","S1","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,null,"in","c94701a8-9630-47c3-9ada-e3b49a5d1275","S2","12","in","12.75","BV",null,null,null,"1.25",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 12\" ND, 150 LB, RF, ASME B16.5",null,null,"88","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1322"]
[null,"14\"","CPFWR","5","1.37","21","14","15.75","L,B,D1,D2,D3,","5665fe4b-cd96-5e8d-bdee-263a5a9a1f15","S1","14","in","14","FL",null,null,"RF","1.37","150",null,null,null,"in","94985f1b-eded-4db1-ae90-d97cdce528dc","S2","14","in","14","BV",null,null,null,"1.37",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 14\" ND, 150 LB, RF, ASME B16.5",null,null,"114","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1324"]
[null,"16\"","CPFWR","5","1.44","23.5","16","18","L,B,D1,D2,D3,","fb7612ab-6bec-5718-93f5-512b82b26f8c","S1","16","in","16","FL",null,null,"RF","1.44","150",null,null,null,"in","b41bf308-3f90-4200-b320-3cc507fde90f","S2","16","in","16","BV",null,null,null,"1.44",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 16\" ND, 150 LB, RF, ASME B16.5",null,null,"142","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1326"]
[null,"18\"","CPFWR","5.5","1.56","25","18","19.88","L,B,D1,D2,D3,","2dcbeb1c-b7e3-5877-9871-c5d3cf4f490b","S1","18","in","18","FL",null,null,"RF","1.56","150",null,null,null,"in","7868d898-1fe4-4bb7-8b78-2e4329f018e8","S2","18","in","18","BV",null,null,null,"1.56",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 18\" ND, 150 LB, RF, ASME B16.5",null,null,"165","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1328"]
[null,"20\"","CPFWR","5.68","1.68","27.5","20","22","L,B,D1,D2,D3,","37092852-c1f6-56c5-8230-297e1ce87d57","S1","20","in","20","FL",null,null,"RF","1.68","150",null,null,null,"in","40d46757-b273-42ea-9f3f-4890bce5ac46","S2","20","in","20","BV",null,null,null,"1.68",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 20\" ND, 150 LB, RF, ASME B16.5",null,null,"197","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1330"]
[null,"24\"","CPFWR","6","1.87","32","24","26.12","L,B,D1,D2,D3,","439a734d-bcaf-5ac6-a47d-54f773fdcbd2","S1","24","in","24","FL",null,null,"RF","1.87","150",null,null,null,"in","7c16fc15-cc03-42b5-94ab-73199e81abed","S2","24","in","24","BV",null,null,null,"1.87",{"$nulls":4},"in","FLANGE WN","ASME B16.5",null,"FLANGE WN, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE WN, 24\" ND, 150 LB, RF, ASME B16.5",null,null,"268","LB","FLWN","FLANGE","853382a2-04dc-465f-a748-e4548ecec2e2","fb7a3964-3646-4054-9c65-5065f3bdd36b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLWN",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1332"]

{"sheet":"FLANGE SW","index":33,"n_rows":7,"n_cols":69,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","L","B","D1","D2","D3","I","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","L","B","D1","D2","D3","I","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPFWR_F_SF","0.62","0.44","3.5","0.88","1.19","0.38","L,B,D1,D2,D3,I,","5a7a0ea3-8779-5edd-b0af-929fb6cb8e2d","S1","0.5","in","0.84","FL",null,null,"RF","0.44","150",null,null,null,"in","6649a455-22f6-47e4-89f0-ea9b349142fa","S2","0.5","in","0.84","SW",null,null,null,"0.44","150",null,null,"0.38","in","FLANGE SW","ASME B16.5",null,"FLANGE SW, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE SW, 1/2\" ND, 150 LB, RF, ASME B16.5",null,null,"2","LB","FLSI","FLANGE","9db3621a-ad69-49a1-ac30-7e0d267548a5","83bee4cc-87b8-4dd1-942b-72563e46b15b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLSI",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1277"]
[null,"3/4\"","CPFWR_F_SF","0.62","0.5","3.88","1.09","1.5","0.44","L,B,D1,D2,D3,I,","8a4646eb-3f59-5bd5-b780-ff22b79859dc","S1","0.75","in","1.05","FL",null,null,"RF","0.5","150",null,null,null,"in","208d581b-1260-434d-9ac7-d3cc5dac71af","S2","0.75","in","1.05","SW",null,null,null,"0.5","150",null,null,"0.44","in","FLANGE SW","ASME B16.5",null,"FLANGE SW, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE SW, 3/4\" ND, 150 LB, RF, ASME B16.5",null,null,"2","LB","FLSI","FLANGE","9db3621a-ad69-49a1-ac30-7e0d267548a5","83bee4cc-87b8-4dd1-942b-72563e46b15b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLSI",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1279"]
[null,"1\"","CPFWR_F_SF","0.68","0.56","4.25","1.36","1.94","0.5","L,B,D1,D2,D3,I,","91a8c8f4-cbae-544f-8113-f119b9564ce9","S1","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,null,"in","ebde45c1-601b-45d2-807b-1ea52a19598a","S2","1","in","1.315","SW",null,null,null,"0.56","150",null,null,"0.5","in","FLANGE SW","ASME B16.5",null,"FLANGE SW, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE SW, 1\" ND, 150 LB, RF, ASME B16.5",null,null,"2","LB","FLSI","FLANGE","9db3621a-ad69-49a1-ac30-7e0d267548a5","83bee4cc-87b8-4dd1-942b-72563e46b15b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLSI",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1281"]
[null,"1 1/2\"","CPFWR_F_SF","0.87","0.68","5","1.95","2.56","0.62","L,B,D1,D2,D3,I,","b6870630-9ab4-505c-a72b-85a13687da64","S1","1.5","in","1.9","FL",null,null,"RF","0.68","150",null,null,null,"in","0732347a-8521-46d0-ba79-17e469f301c8","S2","1.5","in","1.9","SW",null,null,null,"0.68","150",null,null,"0.62","in","FLANGE SW","ASME B16.5",null,"FLANGE SW, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE SW, 1 1/2\" ND, 150 LB, RF, ASME B16.5",null,null,"3","LB","FLSI","FLANGE","9db3621a-ad69-49a1-ac30-7e0d267548a5","83bee4cc-87b8-4dd1-942b-72563e46b15b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLSI",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1285"]
[null,"2\"","CPFWR_F_SF","1","0.75","6","2.44","3.06","0.69","L,B,D1,D2,D3,I,","685231cb-bf3d-504a-8cfd-8d433e819f5d","S1","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,null,"in","86eabb0e-a35a-494f-946f-3860ad4136df","S2","2","in","2.375","SW",null,null,null,"0.75","150",null,null,"0.69","in","FLANGE SW","ASME B16.5",null,"FLANGE SW, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE SW, 2\" ND, 150 LB, RF, ASME B16.5",null,null,"5","LB","FLSI","FLANGE","9db3621a-ad69-49a1-ac30-7e0d267548a5","83bee4cc-87b8-4dd1-942b-72563e46b15b",{"$nulls":4},"2",null,"Flanges","TYPE=FLANGE,SKEY=FLSI",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Flange",null,"1287"]

{"sheet":"ELL 45","index":34,"n_rows":7,"n_cols":61,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","D2","R","A","OF","L1","I1","L2","I2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PathAngle","CurveRadius","SegmentCount","CutbackAngle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","D2","R","A","OF","L1","I1","L2","I2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Path Angle","Curve Radius","Segment Count","Cutback Angle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPB_OFOF","0.84","0","1.06","45","-1","0.82","0.38","0.82","0.38","D,D2,R,A,OF,L1,I1,L2,I2,","b94c8228-e86b-5f6b-9799-5d24065abe0d","ALL","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.38","in","ELL 45","ASME B16.11",null,"ELL 45, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 45, 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.4375","LB","ELSW","ELBOW","350a6fd1-8340-419c-90e6-195f339987ed","7894da3c-5104-4765-8c0e-974deb88a24d",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","1.06",null,null,"Elbow",null,"1091"]
[null,"3/4\"","CPB_OFOF","1.05","0","1.21","45","-1","1","0.5","1","0.5","D,D2,R,A,OF,L1,I1,L2,I2,","fdb16fe4-b728-5948-9a13-c49ba9e2d14a","ALL","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","ELL 45","ASME B16.11",null,"ELL 45, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 45, 3/4\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.5","LB","ELSW","ELBOW","350a6fd1-8340-419c-90e6-195f339987ed","7894da3c-5104-4765-8c0e-974deb88a24d",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","1.21",null,null,"Elbow",null,"1093"]
[null,"1\"","CPB_OFOF","1.315","0","1.35","45","-1","1.06","0.5","1.06","0.5","D,D2,R,A,OF,L1,I1,L2,I2,","1b963042-322d-584b-aef6-d9c511c067ed","ALL","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","ELL 45","ASME B16.11",null,"ELL 45, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 45, 1\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.875","LB","ELSW","ELBOW","350a6fd1-8340-419c-90e6-195f339987ed","7894da3c-5104-4765-8c0e-974deb88a24d",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","1.35",null,null,"Elbow",null,"1095"]
[null,"1 1/2\"","CPB_OFOF","1.9","0","1.96","45","-1","1.31","0.5","1.31","0.5","D,D2,R,A,OF,L1,I1,L2,I2,","895d4b92-d200-58bc-8f02-9c70c3b44da4","ALL","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","ELL 45","ASME B16.11",null,"ELL 45, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 45, 1 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"1.75","LB","ELSW","ELBOW","350a6fd1-8340-419c-90e6-195f339987ed","7894da3c-5104-4765-8c0e-974deb88a24d",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","1.96",null,null,"Elbow",null,"1099"]
[null,"2\"","CPB_OFOF","2.375","0","2.41","45","-1","1.62","0.62","1.62","0.62","D,D2,R,A,OF,L1,I1,L2,I2,","e97b788b-45c6-5b61-8d0c-5cd76ca6b542","ALL","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.62","in","ELL 45","ASME B16.11",null,"ELL 45, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 45, 2\" ND, 3000 LB, SW, ASME B16.11",null,null,"2.875","LB","ELSW","ELBOW","350a6fd1-8340-419c-90e6-195f339987ed","7894da3c-5104-4765-8c0e-974deb88a24d",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","2.41",null,null,"Elbow",null,"1102"]

{"sheet":"ELL 45 LR","index":35,"n_rows":13,"n_cols":59,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","D2","R","A","L1","L2","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PathAngle","CurveRadius","SegmentCount","CutbackAngle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","D2","R","A","L1","L2","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Path Angle","Curve Radius","Segment Count","Cutback Angle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPB","3.5","0","4.8284","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","8f1448fd-57ad-5384-bc9f-7cecbbf9b686","ALL","3","in","3.5","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 3\" ND, BW, ASME B16.9",null,null,"2.24","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","4.8284",null,null,"Elbow",null,"4848"]
[null,"4\"","CPB","4.5","0","6.0355","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","2b1250a3-01ed-5ee3-ab1c-228e7d03d41e","ALL","4","in","4.5","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 4\" ND, BW, ASME B16.9",null,null,"4.29","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","6.0355",null,null,"Elbow",null,"4852"]
[null,"6\"","CPB","6.625","0","9.0533","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","72bb588b-1694-5912-8cc0-79c493ea2ee2","ALL","6","in","6.625","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 6\" ND, BW, ASME B16.9",null,null,"11.24","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","9.0533",null,null,"Elbow",null,"4856"]
[null,"8\"","CPB","8.625","0","12.0711","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","9f36acdd-d6d1-5a32-945f-38232b1a55ec","ALL","8","in","8.625","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 8\" ND, BW, ASME B16.9",null,null,"24.58","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","12.0711",null,null,"Elbow",null,"4858"]
[null,"10\"","CPB","10.75","0","15.0888","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","7f5302d0-c2f7-54e6-98ac-d43fd337a695","ALL","10","in","10.75","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 10\" ND, BW, ASME B16.9",null,null,"45.19","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","15.0888",null,null,"Elbow",null,"4860"]
[null,"12\"","CPB","12.75","0","18.1066","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","63835e1d-dc5c-514d-baf9-a162c6c6cb68","ALL","12","in","12.75","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 12\" ND, BW, ASME B16.9",null,null,"59.52","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","18.1066",null,null,"Elbow",null,"4862"]
[null,"14\"","CPB","14","0","21.1244","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","6f9a0ffe-81be-54c2-aa7e-f7325440b137","ALL","14","in","14","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 14\" ND, BW, ASME B16.9",null,null,"74.95","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","21.1244",null,null,"Elbow",null,"4864"]
[null,"16\"","CPB","16","0","24.1421","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","aa39d495-957b-5d70-9611-4cec728def3c","ALL","16","in","16","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 16\" ND, BW, ASME B16.9",null,null,"105.82","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","24.1421",null,null,"Elbow",null,"4866"]
[null,"18\"","CPB","18","0","27.1599","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","6f6b7e39-a821-5b6a-8c6e-fcd44d06aadd","ALL","18","in","18","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 18\" ND, BW, ASME B16.9",null,null,"132.27","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","27.1599",null,null,"Elbow",null,"4868"]
[null,"20\"","CPB","20","0","30.1777","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","696f3dd2-8308-575e-8fd8-6fa5df920ff6","ALL","20","in","20","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 20\" ND, BW, ASME B16.9",null,null,"156.96","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","30.1777",null,null,"Elbow",null,"4870"]
[null,"24\"","CPB","24","0","36.2132","45",null,null,"-1","D,D2,R,A,L1,L2,OF,","2fc14ed8-4f10-5b4c-8fc4-44cdedd63c1c","ALL","24","in","24","BV",{"$nulls":7},"0","in","ELL 45 LR","ASME B16.9",null,"ELL 45 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 45 LR, 24\" ND, BW, ASME B16.9",null,null,"226.96","LB","ELBW","ELBOW","3d1ea5b5-23c3-4981-81f1-9f8891159ee7","d4b7bd00-b6ed-4a42-ba1c-9ab58ff4a96a",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"45","36.2132",null,null,"Elbow",null,"4874"]

{"sheet":"ELL 90","index":36,"n_rows":7,"n_cols":61,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","D2","R","A","OF","L1","I1","L2","I2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PathAngle","CurveRadius","SegmentCount","CutbackAngle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","D2","R","A","OF","L1","I1","L2","I2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Path Angle","Curve Radius","Segment Count","Cutback Angle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPB_OFOF","0.84","0","0.62","90","-1","1","0.38","1","0.38","D,D2,R,A,OF,L1,I1,L2,I2,","8646a48c-6940-5a43-91eb-003ad1ba01bf","ALL","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.38","in","ELL 90","ASME B16.11",null,"ELL 90, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 90, 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.5","LB","ELSW","ELBOW","799163aa-18f6-4061-8377-1e2ee9f25801","f3dde5df-cada-4fac-936b-9d3a258f66fe",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0.62",null,null,"Elbow",null,"1116"]
[null,"3/4\"","CPB_OFOF","1.05","0","0.75","90","-1","1.25","0.5","1.25","0.5","D,D2,R,A,OF,L1,I1,L2,I2,","4f242f7f-f4c1-5d67-bbf5-952dfcb17f65","ALL","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","ELL 90","ASME B16.11",null,"ELL 90, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 90, 3/4\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.6875","LB","ELSW","ELBOW","799163aa-18f6-4061-8377-1e2ee9f25801","f3dde5df-cada-4fac-936b-9d3a258f66fe",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0.75",null,null,"Elbow",null,"1118"]
[null,"1\"","CPB_OFOF","1.315","0","0.88","90","-1","1.38","0.5","1.38","0.5","D,D2,R,A,OF,L1,I1,L2,I2,","22053427-24a3-577e-94f5-2ecb88019515","ALL","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","ELL 90","ASME B16.11",null,"ELL 90, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 90, 1\" ND, 3000 LB, SW, ASME B16.11",null,null,"1.0625","LB","ELSW","ELBOW","799163aa-18f6-4061-8377-1e2ee9f25801","f3dde5df-cada-4fac-936b-9d3a258f66fe",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0.88",null,null,"Elbow",null,"1120"]
[null,"1 1/2\"","CPB_OFOF","1.9","0","1.25","90","-1","1.75","0.5","1.75","0.5","D,D2,R,A,OF,L1,I1,L2,I2,","156dcfa7-4594-5564-ac9e-2a40de8b4e38","ALL","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","ELL 90","ASME B16.11",null,"ELL 90, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 90, 1 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"2.125","LB","ELSW","ELBOW","799163aa-18f6-4061-8377-1e2ee9f25801","f3dde5df-cada-4fac-936b-9d3a258f66fe",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","1.25",null,null,"Elbow",null,"1124"]
[null,"2\"","CPB_OFOF","2.375","0","1.5","90","-1","2.12","0.62","2.12","0.62","D,D2,R,A,OF,L1,I1,L2,I2,","fb94be3e-9361-5b9d-adab-c05a33ff4e15","ALL","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.62","in","ELL 90","ASME B16.11",null,"ELL 90, 3000 LB, SW, ASME B16.11, ASTM A105","ELL 90, 2\" ND, 3000 LB, SW, ASME B16.11",null,null,"3.5625","LB","ELSW","ELBOW","799163aa-18f6-4061-8377-1e2ee9f25801","f3dde5df-cada-4fac-936b-9d3a258f66fe",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","1.5",null,null,"Elbow",null,"1126"]

{"sheet":"ELL 90 LR","index":37,"n_rows":13,"n_cols":59,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","D2","R","A","L1","L2","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PathAngle","CurveRadius","SegmentCount","CutbackAngle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","D2","R","A","L1","L2","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Path Angle","Curve Radius","Segment Count","Cutback Angle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPB","3.5","0","4.5","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","9e4112c9-c142-563c-9324-64fa76c8379e","ALL","3","in","3.5","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 3\" ND, BW, ASME B16.9",null,null,"4.47","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","4.5",null,null,"Elbow",null,"4915"]
[null,"4\"","CPB","4.5","0","6","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","e0da85c3-4545-5032-84a1-9355a782146e","ALL","4","in","4.5","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 4\" ND, BW, ASME B16.9",null,null,"8.59","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","6",null,null,"Elbow",null,"4919"]
[null,"6\"","CPB","6.625","0","9","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","640bb295-f9ad-5237-970c-709fb71a06b3","ALL","6","in","6.625","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 6\" ND, BW, ASME B16.9",null,null,"22.48","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","9",null,null,"Elbow",null,"4923"]
[null,"8\"","CPB","8.625","0","12","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","da71d197-181e-5f2d-8d28-3aabd74169b5","ALL","8","in","8.625","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 8\" ND, BW, ASME B16.9",null,null,"44.75","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","12",null,null,"Elbow",null,"4925"]
[null,"10\"","CPB","10.75","0","15","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","e9350052-0edf-5ce1-8690-e5d441783347","ALL","10","in","10.75","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 10\" ND, BW, ASME B16.9",null,null,"81.57","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","15",null,null,"Elbow",null,"4927"]
[null,"12\"","CPB","12.75","0","18","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","38c2179c-8ce1-55eb-beee-2095d6bb5e03","ALL","12","in","12.75","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 12\" ND, BW, ASME B16.9",null,null,"119.04","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","18",null,null,"Elbow",null,"4929"]
[null,"14\"","CPB","14","0","21","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","93be68ca-3286-5e0d-8a1b-309d7c796a2c","ALL","14","in","14","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 14\" ND, BW, ASME B16.9",null,null,"149.91","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","21",null,null,"Elbow",null,"4931"]
[null,"16\"","CPB","16","0","24","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","4782e0c9-3660-5f14-acf1-6b6b20a11c58","ALL","16","in","16","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 16\" ND, BW, ASME B16.9",null,null,"196.65","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","24",null,null,"Elbow",null,"4933"]
[null,"18\"","CPB","18","0","27","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","d45ebcf7-32c6-56c3-afbd-39a85adfedad","ALL","18","in","18","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 18\" ND, BW, ASME B16.9",null,null,"248.9","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","27",null,null,"Elbow",null,"4935"]
[null,"20\"","CPB","20","0","30","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","b59d2871-fb9d-5984-a18d-b951ea395599","ALL","20","in","20","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 20\" ND, BW, ASME B16.9",null,null,"313.93","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","30",null,null,"Elbow",null,"4937"]
[null,"24\"","CPB","24","0","36","90",null,null,"-1","D,D2,R,A,L1,L2,OF,","582e895b-e1f6-59d8-880b-6340bd83505c","ALL","24","in","24","BV",{"$nulls":7},"0","in","ELL 90 LR","ASME B16.9",null,"ELL 90 LR, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","ELL 90 LR, 24\" ND, BW, ASME B16.9",null,null,"445.33","LB","ELBW","ELBOW","f4268140-c2b8-4fd1-8436-16cf14618ce6","1661262b-21d0-4091-a1df-40034cd94bba",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELBW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","36",null,null,"Elbow",null,"4941"]

{"sheet":"STREET ELL","index":38,"n_rows":7,"n_cols":75,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","D2","R","A","OF","L1","L2","I","ContentGeometryParamDefinition","SizeRecordId_S1","PortName_S1","NominalDiameter_S1","NominalUnit_S1","MatchingPipeOd_S1","EndType_S1","FlangeStd_S1","GasketStd_S1","Facing_S1","FlangeThickness_S1","PressureClass_S1","Schedule_S1","WallThickness_S1","EngagementLength_S1","LengthUnit_S1","SizeRecordId_S2","PortName_S2","NominalDiameter_S2","NominalUnit_S2","MatchingPipeOd_S2","EndType_S2","FlangeStd_S2","GasketStd_S2","Facing_S2","FlangeThickness_S2","PressureClass_S2","Schedule_S2","WallThickness_S2","EngagementLength_S2","LengthUnit_S2","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PathAngle","CurveRadius","SegmentCount","CutbackAngle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","D2","R","A","OF","L1","L2","I","ContentGeometryParamDefinition","Size Record Id_S1","Port Name_S1","Nominal Diameter_S1","Nominal Unit_S1","Matching Pipe OD_S1","End Type_S1","Flange Std_S1","Gasket Std_S1","Facing_S1","Flange Thickness_S1","Pressure Class_S1","Schedule_S1","Wall Thickness_S1","Engagement Length_S1","Port Unit_S1","Size Record Id_S2","Port Name_S2","Nominal Diameter_S2","Nominal Unit_S2","Matching Pipe OD_S2","End Type_S2","Flange Std_S2","Gasket Std_S2","Facing_S2","Flange Thickness_S2","Pressure Class_S2","Schedule_S2","Wall Thickness_S2","Engagement Length_S2","Port Unit_S2","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Path Angle","Curve Radius","Segment Count","Cutback Angle","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPB_OMOF","0.84","0","0","90","-1","1.625","1.125","0.3125","D,D2,R,A,OF,L1,L2,I,","72512015-ecee-56d7-b706-3a2b582648a6","S1","0.5","in","0.84","PL",{"$nulls":4},"3000",null,null,"0","in","c623a500-1e3f-4df2-8de3-4485bc8e5ec7","S2","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.3125","in","STREET ELL","ASME B16.11",null,"STREET ELL, 3000 LB, PEXSW, ASME B16.11, ASTM A105","STREET ELL, 1/2\" ND, 3000 LB, PEXSW, ASME B16.11",null,null,"0.595","LB","ELSC","ELBOW","1f304d0b-00dd-4485-8c78-a7d35ede5dcd","f69853f5-82f1-4ccf-a68e-17b51d6ac87e",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSC",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0",null,null,"Elbow",null,"1267"]
[null,"3/4\"","CPB_OMOF","1.05","0","0","90","-1","1.875","1.375","0.4375","D,D2,R,A,OF,L1,L2,I,","c98ac377-20f3-5d13-9490-9fa8ef611220","S1","0.75","in","1.05","PL",{"$nulls":4},"3000",null,null,"0","in","0fdd4225-fb98-4e4b-8916-e5c190334a99","S2","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.4375","in","STREET ELL","ASME B16.11",null,"STREET ELL, 3000 LB, PEXSW, ASME B16.11, ASTM A105","STREET ELL, 3/4\" ND, 3000 LB, PEXSW, ASME B16.11",null,null,"1.048","LB","ELSC","ELBOW","1f304d0b-00dd-4485-8c78-a7d35ede5dcd","f69853f5-82f1-4ccf-a68e-17b51d6ac87e",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSC",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0",null,null,"Elbow",null,"1269"]
[null,"1\"","CPB_OMOF","1.315","0","0","90","-1","2.25","1.75","0.4375","D,D2,R,A,OF,L1,L2,I,","ba63654f-4724-5ab2-83f7-b08b209bdbe3","S1","1","in","1.315","PL",{"$nulls":4},"3000",null,null,"0","in","74e106bf-7f0a-408f-89e3-4093a8c831f8","S2","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.4375","in","STREET ELL","ASME B16.11",null,"STREET ELL, 3000 LB, PEXSW, ASME B16.11, ASTM A105","STREET ELL, 1\" ND, 3000 LB, PEXSW, ASME B16.11",null,null,"1.438","LB","ELSC","ELBOW","1f304d0b-00dd-4485-8c78-a7d35ede5dcd","f69853f5-82f1-4ccf-a68e-17b51d6ac87e",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSC",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0",null,null,"Elbow",null,"1271"]
[null,"1 1/2\"","CPB_OMOF","1.9","0","0","90","-1","2.9375","2.125","0.4375","D,D2,R,A,OF,L1,L2,I,","7a827233-851b-5c93-9c37-11b1a6508ee6","S1","1.5","in","1.9","PL",{"$nulls":4},"3000",null,null,"0","in","923453d7-2cab-40db-8a59-6614f496746a","S2","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.4375","in","STREET ELL","ASME B16.11",null,"STREET ELL, 3000 LB, PEXSW, ASME B16.11, ASTM A105","STREET ELL, 1 1/2\" ND, 3000 LB, PEXSW, ASME B16.11",null,null,"2.34","LB","ELSC","ELBOW","1f304d0b-00dd-4485-8c78-a7d35ede5dcd","f69853f5-82f1-4ccf-a68e-17b51d6ac87e",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSC",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0",null,null,"Elbow",null,"1273"]
[null,"2\"","CPB_OMOF","2.375","0","0","90","-1","3.3125","2.5","0.5625","D,D2,R,A,OF,L1,L2,I,","d96b4d92-ed2a-557e-a2ec-7041dc4efb2c","S1","2","in","2.375","PL",{"$nulls":4},"3000",null,null,"0","in","a0e659d7-17da-4681-b2db-db23ee5406a7","S2","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.5625","in","STREET ELL","ASME B16.11",null,"STREET ELL, 3000 LB, PEXSW, ASME B16.11, ASTM A105","STREET ELL, 2\" ND, 3000 LB, PEXSW, ASME B16.11",null,null,"3","LB","ELSC","ELBOW","1f304d0b-00dd-4485-8c78-a7d35ede5dcd","f69853f5-82f1-4ccf-a68e-17b51d6ac87e",{"$nulls":4},"2",null,"Fittings","TYPE=ELBOW,SKEY=ELSC",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"90","0",null,null,"Elbow",null,"1275"]

{"sheet":"COUPLING","index":39,"n_rows":9,"n_cols":56,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","L","OF","L1","I1","L2","I2","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","Length","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","L","OF","L1","I1","L2","I2","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Length","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPP_OFOF","0.84","0.5","-1","0.5","0.5","0.5","0.5","D,L,OF,L1,I1,L2,I2,","f2058019-fde0-50a6-9f1b-c650e1774fc1","ALL","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.5","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 1/2\"X1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.25","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1.140625","Coupling",null,"1067"]
[null,"3/4\"","CPP_OFOF","1.05","0.5","-1","0.5625","0.5625","0.5625","0.5625","D,L,OF,L1,I1,L2,I2,","63d3ec6a-3c1a-5204-8bcc-200d78e61be5","ALL","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5625","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 3/4\"X3/4\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.375","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1.40625","Coupling",null,"1069"]
[null,"1\"","CPP_OFOF","1.315","0.625","-1","0.625","0.625","0.625","0.625","D,L,OF,L1,I1,L2,I2,","6ba5fb9f-4426-56a1-ab04-ab57ee78159d","ALL","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.625","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 1\"X1\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.75","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1.515625","Coupling",null,"1071"]
[null,"1 1/2\"","CPP_OFOF","1.9","0.625","-1","0.75","0.75","0.75","0.75","D,L,OF,L1,I1,L2,I2,","bb632f7e-2287-5d06-b14a-3f6103e6e89d","ALL","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.75","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 1 1/2\"X1 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"1.3125","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1.515625","Coupling",null,"1075"]
[null,"2\"","CPP_OFOF","2.375","0.875","-1","1","0.875","1","0.875","D,L,OF,L1,I1,L2,I2,","779b36f9-3046-5f47-9b19-b48730b88bec","ALL","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.875","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 2\"X2\" ND, 3000 LB, SW, ASME B16.11",null,null,"2","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"2.015625","Coupling",null,"1077"]
[null,"3\"","CPP_OFOF","3.5","1","0.125","1","0.9375","1","0.9375","D,L,OF,L1,I1,L2,I2,","b8c03399-21f1-5185-9d83-a79d51354ac8","ALL","3","in","3.5","SW",{"$nulls":4},"3000",null,null,"0.9375","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 3\"X3\" ND, 3000 LB, SW, ASME B16.11",null,null,"4.5625","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"2.015625","Coupling",null,"1081"]
[null,"4\"","CPP_OFOF","4.5","1","0.125","1.125","1.0625","1.125","1.0625","D,L,OF,L1,I1,L2,I2,","0f5cf9a9-c39d-59e7-88d8-eca494c79dea","ALL","4","in","4.5","SW",{"$nulls":4},"3000",null,null,"1.0625","in","COUPLING","ASME B16.11",null,"COUPLING, 3000 LB, SW, ASME B16.11, ASTM A105","COUPLING, 4\"X4\" ND, 3000 LB, SW, ASME B16.11",null,null,"8.625","LB","COSW","COUPLING","8e21676d-8fe5-42c7-8e69-c26092c3c324","49dbdcc4-83e6-4160-b521-65b41e31798c",{"$nulls":4},"2",null,"Fittings","TYPE=COUPLING,SKEY=COSW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"2.265625","Coupling",null,"1083"]

{"sheet":"CAP_1","index":40,"n_rows":7,"n_cols":53,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","L","I","DISP","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","L","I","DISP","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPC_OF","0.84","0.63","0.38","2","-1","D,L,I,DISP,OF,","77c27537-4fc7-51fd-a348-a3fd515be0cc","ALL","0.5","in","0.84","SW",{"$nulls":4},"3000",null,null,"0.38","in","CAP","ASME B16.11",null,"CAP, 3000 LB, SW, ASME B16.11, ASTM A105","CAP, 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.25","LB","KASW","CAP","ce6164c4-3d6c-4e92-b547-cdf239b835b0","10a92c6e-6a67-482f-b63a-374543bb06da",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KASW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"1019"]
[null,"3/4\"","CPC_OF","1.05","0.75","0.5","2","-1","D,L,I,DISP,OF,","96aa2e56-127e-522c-b703-b0dc2d7959d9","ALL","0.75","in","1.05","SW",{"$nulls":4},"3000",null,null,"0.5","in","CAP","ASME B16.11",null,"CAP, 3000 LB, SW, ASME B16.11, ASTM A105","CAP, 3/4\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.375","LB","KASW","CAP","ce6164c4-3d6c-4e92-b547-cdf239b835b0","10a92c6e-6a67-482f-b63a-374543bb06da",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KASW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"1020"]
[null,"1\"","CPC_OF","1.315","0.88","0.5","2","-1","D,L,I,DISP,OF,","4af173f9-add9-5cb6-9f8b-34d9a11ecc05","ALL","1","in","1.315","SW",{"$nulls":4},"3000",null,null,"0.5","in","CAP","ASME B16.11",null,"CAP, 3000 LB, SW, ASME B16.11, ASTM A105","CAP, 1\" ND, 3000 LB, SW, ASME B16.11",null,null,"0.4375","LB","KASW","CAP","ce6164c4-3d6c-4e92-b547-cdf239b835b0","10a92c6e-6a67-482f-b63a-374543bb06da",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KASW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"1021"]
[null,"1 1/2\"","CPC_OF","1.9","0.94","0.5","2","-1","D,L,I,DISP,OF,","a568e834-b2ab-5be8-84db-7a60b7263abc","ALL","1.5","in","1.9","SW",{"$nulls":4},"3000",null,null,"0.5","in","CAP","ASME B16.11",null,"CAP, 3000 LB, SW, ASME B16.11, ASTM A105","CAP, 1 1/2\" ND, 3000 LB, SW, ASME B16.11",null,null,"1.1875","LB","KASW","CAP","ce6164c4-3d6c-4e92-b547-cdf239b835b0","10a92c6e-6a67-482f-b63a-374543bb06da",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KASW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"1023"]
[null,"2\"","CPC_OF","2.375","1.12","0.62","2","-1","D,L,I,DISP,OF,","8af195ea-e4a1-5480-a79a-1b737c3fc747","ALL","2","in","2.375","SW",{"$nulls":4},"3000",null,null,"0.62","in","CAP","ASME B16.11",null,"CAP, 3000 LB, SW, ASME B16.11, ASTM A105","CAP, 2\" ND, 3000 LB, SW, ASME B16.11",null,null,"2","LB","KASW","CAP","ce6164c4-3d6c-4e92-b547-cdf239b835b0","10a92c6e-6a67-482f-b63a-374543bb06da",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KASW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"1024"]

{"sheet":"CAP","index":41,"n_rows":13,"n_cols":52,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","D","L","DISP","OF","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","D","L","DISP","OF","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"3\"","CPC","3.5","2","0","0","D,L,DISP,OF,","95a78321-f4bd-59be-be32-281acc8a448c","ALL","3","in","3.5","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 3\" ND, BW, ASME B16.9",null,null,"1.54","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4808"]
[null,"4\"","CPC","4.5","2.5","0","0","D,L,DISP,OF,","b05396af-cfaa-519e-a241-5819ac20c831","ALL","4","in","4.5","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 4\" ND, BW, ASME B16.9",null,null,"3.52","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4810"]
[null,"6\"","CPC","6.625","3.5","0","0","D,L,DISP,OF,","a62127f0-7156-5fbe-8918-2e1d0aef6eac","ALL","6","in","6.625","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 6\" ND, BW, ASME B16.9",null,null,"7.93","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4812"]
[null,"8\"","CPC","8.625","4","0","0","D,L,DISP,OF,","824a4934-a70e-5185-8522-2a1b34483dfa","ALL","8","in","8.625","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 8\" ND, BW, ASME B16.9",null,null,"12.12","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4813"]
[null,"10\"","CPC","10.75","5","0","0","D,L,DISP,OF,","1b40357d-7e14-5998-84ca-d69a64157f22","ALL","10","in","10.75","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 10\" ND, BW, ASME B16.9",null,null,"22.04","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4814"]
[null,"12\"","CPC","12.75","6","0","0","D,L,DISP,OF,","796ee910-9a49-505f-a33e-9d76787a91ec","ALL","12","in","12.75","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 12\" ND, BW, ASME B16.9",null,null,"33.06","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4815"]
[null,"14\"","CPC","14","6.5","0","0","D,L,DISP,OF,","00576f73-168a-5d57-9ba3-fcb73f715aa3","ALL","14","in","14","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 14\" ND, BW, ASME B16.9",null,null,"37.47","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4816"]
[null,"16\"","CPC","16","7","0","0","D,L,DISP,OF,","9f9ac072-9a6d-51de-818c-bbb8eee6d8ab","ALL","16","in","16","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 16\" ND, BW, ASME B16.9",null,null,"50.7","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4817"]
[null,"18\"","CPC","18","8","0","0","D,L,DISP,OF,","48af8ca4-3d9c-5a07-96b1-177b7fddb39b","ALL","18","in","18","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 18\" ND, BW, ASME B16.9",null,null,"63.93","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4818"]
[null,"20\"","CPC","20","9","0","0","D,L,DISP,OF,","acfd2f71-22eb-5ddc-a116-f9e39f0fecad","ALL","20","in","20","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 20\" ND, BW, ASME B16.9",null,null,"79.36","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4819"]
[null,"24\"","CPC","24","10.5","0","0","D,L,DISP,OF,","6f07f37f-aed8-5661-b1e3-329ba0e9e1d7","ALL","24","in","24","BV",{"$nulls":7},"0","in","CAP","ASME B16.9",null,"CAP, BW, ASME B16.9, ASTM A234 Gr WPB SMLS, Sch 40","CAP, 24\" ND, BW, ASME B16.9",null,null,"114.64","LB","KABW","CAP","82c0c6b2-4213-4f48-8489-d5e51455d760","57202da2-ad84-4416-b8cd-451ccb25219c",{"$nulls":4},"1",null,"Miscellaneous","TYPE=CAP,SKEY=KABW",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"Cap",null,"4821"]

{"sheet":"BOLT SET_1","index":42,"n_rows":22,"n_cols":55,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","BoltSize","NumberInSet","IsLugSet","Length","StudTypeDescription","StudDescription","BoltCompatibleStd","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Bolt Size","Number In Set","Is Lug Set","Length","Stud Type Description","Stud Description","Bolt Compatible Standard","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"",null,null,"a73c3378-c2ee-5f6b-b9ed-5c411d5a3fc7","ALL","0.5","in",{"$nulls":4},"RF","0.44","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1/2\", ASTM A194, GR 2, 2 WASHER 1/2\", ASTM F436",null,null,"1.03","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","False","2.25","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"995"]
[null,"3/4\"",null,null,"3e775837-f34b-53fa-8d44-77f030b90f9c","ALL","0.75","in",{"$nulls":4},"RF","0.5","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1/2\", ASTM A194, GR 2, 2 WASHER 1/2\", ASTM F436",null,null,"1.1","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","False","2.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"996"]
[null,"1\"",null,null,"d52e1e45-df33-5c89-8bfa-0cd7788f2bd1","ALL","1","in",{"$nulls":4},"RF","0.56","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1/2\", ASTM A194, GR 2, 2 WASHER 1/2\", ASTM F436",null,null,"1.14","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","False","2.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"997"]
[null,"1 1/4\"",null,null,"e9198310-e773-51b8-b3fb-fbaacff4b4c9","ALL","1.25","in",{"$nulls":4},"RF","0.62","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1/2\", ASTM A194, GR 2, 2 WASHER 1/2\", ASTM F436",null,null,"1.14","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","False","2.75","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"998"]
[null,"1 1/2\"",null,null,"34f9c8d8-7201-59ed-939e-93ab6613f4a1","ALL","1.5","in",{"$nulls":4},"RF","0.68","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1/2\", ASTM A194, GR 2, 2 WASHER 1/2\", ASTM F436",null,null,"1.19","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","False","2.75","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"999"]
[null,"2\"",null,null,"4218249d-8beb-559c-9c67-79e86dcef9c7","ALL","2","in",{"$nulls":4},"RF","0.75","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 5/8\", ASTM A194, GR 2, 2 WASHER 5/8\", ASTM F436",null,null,"1.67","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","4","False","3.25","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1001"]
[null,"2 1/2\"",null,null,"f4371f0e-35c5-586c-ab63-4fa9a532f188","ALL","2.5","in",{"$nulls":4},"RF","0.87","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 5/8\", ASTM A194, GR 2, 2 WASHER 5/8\", ASTM F436",null,null,"1.71","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","4","False","3.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1002"]
[null,"3\"",null,null,"7259d54c-8a36-52a3-86d0-db1ac977f9e6","ALL","3","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 5/8\", ASTM A194, GR 2, 2 WASHER 5/8\", ASTM F436",null,null,"1.71","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","4","False","3.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1003"]
[null,"3 1/2\"",null,null,"873278e7-ff19-5f2d-b7d3-ddd7adc06014","ALL","3.5","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 5/8\", ASTM A194, GR 2, 2 WASHER 5/8\", ASTM F436",null,null,"3.43","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","8","False","3.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1004"]
[null,"4\"",null,null,"b882eab6-3249-558d-9d37-7c8e1052d792","ALL","4","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 5/8\", ASTM A194, GR 2, 2 WASHER 5/8\", ASTM F436",null,null,"3.43","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","8","False","3.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1005"]
[null,"5\"",null,null,"cc753025-cc21-5931-bdc3-2d422acf460f","ALL","5","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 3/4\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 3/4\", ASTM A194, GR 2, 2 WASHER 3/4\", ASTM F436",null,null,"6.81","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3/4\"","8","False","3.75","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1006"]
[null,"6\"",null,null,"e068d5c2-0f95-5801-a922-acbdc44fda4e","ALL","6","in",{"$nulls":4},"RF","1","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 3/4\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 3/4\", ASTM A194, GR 2, 2 WASHER 3/4\", ASTM F436",null,null,"6.81","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3/4\"","8","False","4","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1007"]
[null,"8\"",null,null,"45b1af22-9398-53ad-a569-e1bb720c5c5f","ALL","8","in",{"$nulls":4},"RF","1.12","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 3/4\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 3/4\", ASTM A194, GR 2, 2 WASHER 3/4\", ASTM F436",null,null,"7.18","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3/4\"","8","False","4.25","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1008"]
[null,"10\"",null,null,"5748f3b5-c91c-5847-baf2-43efcbdaacda","ALL","10","in",{"$nulls":4},"RF","1.18","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 7/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 7/8\", ASTM A194, GR 2, 2 WASHER 7/8\", ASTM F436",null,null,"16.71","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7/8\"","12","False","4.5","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1009"]
[null,"12\"",null,null,"1ad2e9eb-f978-5e0c-a30f-12564950a80e","ALL","12","in",{"$nulls":4},"RF","1.25","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 7/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 7/8\", ASTM A194, GR 2, 2 WASHER 7/8\", ASTM F436",null,null,"16.71","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7/8\"","12","False","4.75","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1010"]
[null,"14\"",null,null,"7ff6a31b-be6a-52be-b4c8-75db19c38892","ALL","14","in",{"$nulls":4},"RF","1.37","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1\", ASTM A194, GR 2, 2 WASHER 1\", ASTM F436",null,null,"24.51","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1\"","12","False","5.25","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1011"]
[null,"16\"",null,null,"2799e6e8-5201-5684-a91c-c49689185317","ALL","16","in",{"$nulls":4},"RF","1.44","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1\", ASTM A194, GR 2, 2 WASHER 1\", ASTM F436",null,null,"32.69","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1\"","16","False","5.25","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1012"]
[null,"18\"",null,null,"a8da20e4-10d8-570d-99ad-3d93f43c5d86","ALL","18","in",{"$nulls":4},"RF","1.56","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1 1/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1 1/8\", ASTM A194, GR 2, 2 WASHER 1 1/8\", ASTM F436",null,null,"44.44","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1 1/8\"","16","False","5.75","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1013"]
[null,"20\"",null,null,"8140b0a7-6e83-533a-a2da-4e7560668800","ALL","20","in",{"$nulls":4},"RF","1.68","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1 1/8\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1 1/8\", ASTM A194, GR 2, 2 WASHER 1 1/8\", ASTM F436",null,null,"57.32","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1 1/8\"","20","False","6.25","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1014"]
[null,"24\"",null,null,"34de67dc-ee1f-5170-b0e5-cd03637199c3","ALL","24","in",{"$nulls":4},"RF","1.87","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, STUD BOLT","STUD BOLT 1 1/4\" X @@@ LG, ASTM A193, B7 W/2 HEX. NUT 1 1/4\", ASTM A194, GR 2, 2 WASHER 1 1/4\", ASTM F436",null,null,"77.6","LB",null,"BOLT","8328946d-8e40-4cf1-995c-9718d7359a8c","2b3d948f-b6cf-4b72-a06c-1c13eec72585",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1 1/4\"","20","False","6.75","Stud Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"1015"]

{"sheet":"BOLT SET","index":43,"n_rows":22,"n_cols":55,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","BoltSize","NumberInSet","IsLugSet","Length","StudTypeDescription","StudDescription","BoltCompatibleStd","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","Bolt Size","Number In Set","Is Lug Set","Length","Stud Type Description","Stud Description","Bolt Compatible Standard","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"",null,null,"1d114cdb-f375-5427-ae91-5fcd3c003ee6","ALL","0.5","in",{"$nulls":4},"RF","0.44","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1/2\", ASTM A194, GR 2, 1 WASHER 1/2\", ASTM F436",null,null,"0.8","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","True","2.091488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"282"]
[null,"3/4\"",null,null,"a71f67a6-3433-51ad-ba95-8da44765b5d1","ALL","0.75","in",{"$nulls":4},"RF","0.5","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1/2\", ASTM A194, GR 2, 1 WASHER 1/2\", ASTM F436",null,null,"0.8","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","True","2.211488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"382"]
[null,"1\"",null,null,"80e9544f-6327-5e52-890b-c5e4d6c73c33","ALL","1","in",{"$nulls":4},"RF","0.56","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1/2\", ASTM A194, GR 2, 1 WASHER 1/2\", ASTM F436",null,null,"0.9","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","True","2.331488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"383"]
[null,"1 1/4\"",null,null,"42957c81-2611-57de-a579-84a025f80325","ALL","1.25","in",{"$nulls":4},"RF","0.62","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1/2\", ASTM A194, GR 2, 1 WASHER 1/2\", ASTM F436",null,null,"0.9","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","True","2.451488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"384"]
[null,"1 1/2\"",null,null,"d10c9be4-4275-561e-bc07-b0c5c661e542","ALL","1.5","in",{"$nulls":4},"RF","0.68","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1/2\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1/2\", ASTM A194, GR 2, 1 WASHER 1/2\", ASTM F436",null,null,"0.9","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1/2\"","4","True","2.571488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"385"]
[null,"2\"",null,null,"1b68a4fe-12b1-5412-ab5b-41eb56c12842","ALL","2","in",{"$nulls":4},"RF","0.75","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 5/8\", ASTM A194, GR 2, 1 WASHER 5/8\", ASTM F436",null,null,"1.7","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","4","True","2.990488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"386"]
[null,"2 1/2\"",null,null,"d6a3126c-7005-5039-a3ee-a0ec0639da37","ALL","2.5","in",{"$nulls":4},"RF","0.87","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 5/8\", ASTM A194, GR 2, 1 WASHER 5/8\", ASTM F436",null,null,"1.8","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","4","True","3.230488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"486"]
[null,"3\"",null,null,"dc4690a4-4d1d-51f6-945d-922ba51b6eb1","ALL","3","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 5/8\", ASTM A194, GR 2, 1 WASHER 5/8\", ASTM F436",null,null,"1.8","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","4","True","3.370488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"487"]
[null,"3 1/2\"",null,null,"32e840fa-7f95-5643-b234-a8642428bad7","ALL","3.5","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 5/8\", ASTM A194, GR 2, 1 WASHER 5/8\", ASTM F436",null,null,"3.7","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","8","True","3.370488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"488"]
[null,"4\"",null,null,"91113e05-a315-552c-934b-53b9608c82bb","ALL","4","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 5/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 5/8\", ASTM A194, GR 2, 1 WASHER 5/8\", ASTM F436",null,null,"3.7","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"5/8\"","8","True","3.370488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"489"]
[null,"5\"",null,null,"b1a1a19d-5e19-52ba-ab3d-57cfe33e4933","ALL","5","in",{"$nulls":4},"RF","0.94","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 3/4\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 3/4\", ASTM A194, GR 2, 1 WASHER 3/4\", ASTM F436",null,null,"5.7","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3/4\"","8","True","3.638488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"490"]
[null,"6\"",null,null,"ae8298cc-a7c8-5214-bb41-1985a1acc7fe","ALL","6","in",{"$nulls":4},"RF","1","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 3/4\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 3/4\", ASTM A194, GR 2, 1 WASHER 3/4\", ASTM F436",null,null,"5.9","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3/4\"","8","True","3.758488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"590"]
[null,"8\"",null,null,"c5a5a9c1-6882-5150-a539-b27933698a0f","ALL","8","in",{"$nulls":4},"RF","1.12","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 3/4\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 3/4\", ASTM A194, GR 2, 1 WASHER 3/4\", ASTM F436",null,null,"6.1","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"3/4\"","8","True","3.998488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"591"]
[null,"10\"",null,null,"814a12c4-2c4c-5b47-a346-a044e96470a6","ALL","10","in",{"$nulls":4},"RF","1.18","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 7/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 7/8\", ASTM A194, GR 2, 1 WASHER 7/8\", ASTM F436",null,null,"13.7","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7/8\"","12","True","4.389488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"592"]
[null,"12\"",null,null,"6bedbaf7-a828-567f-854b-62d0fb7a60e5","ALL","12","in",{"$nulls":4},"RF","1.25","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 7/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 7/8\", ASTM A194, GR 2, 1 WASHER 7/8\", ASTM F436",null,null,"14","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"7/8\"","12","True","4.529488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"692"]
[null,"14\"",null,null,"7493c8b5-44f0-5291-9b39-5b478324eb16","ALL","14","in",{"$nulls":4},"RF","1.37","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1\", ASTM A194, GR 2, 1 WASHER 1\", ASTM F436",null,null,"20","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1\"","12","True","5.023488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"693"]
[null,"16\"",null,null,"2c9e5ad6-50b4-57a1-9d83-fce9b8c00dc6","ALL","16","in",{"$nulls":4},"RF","1.44","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1\", ASTM A194, GR 2, 1 WASHER 1\", ASTM F436",null,null,"27.1","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1\"","16","True","5.163488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"793"]
[null,"18\"",null,null,"799c91a7-3149-50ff-8c08-201328f33a08","ALL","18","in",{"$nulls":4},"RF","1.56","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1 1/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1 1/8\", ASTM A194, GR 2, 1 WASHER 1 1/8\", ASTM F436",null,null,"37.3","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1 1/8\"","16","True","5.657488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"794"]
[null,"20\"",null,null,"f4888211-2db6-5e9a-8548-f5739819e935","ALL","20","in",{"$nulls":4},"RF","1.68","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1 1/8\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1 1/8\", ASTM A194, GR 2, 1 WASHER 1 1/8\", ASTM F436",null,null,"48","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1 1/8\"","20","True","5.897488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"894"]
[null,"24\"",null,null,"437e38ed-794e-5262-a89f-2f124048e43f","ALL","24","in",{"$nulls":4},"RF","1.87","150",null,null,null,"in","Bolt set",null,null,"BOLT SET, RF, 150 LB, LUG BOLT","LUG BOLT 1 1/4\" X @@@ LG, ASTM A193, B7 W/1 HEX. NUT 1 1/4\", ASTM A194, GR 2, 1 WASHER 1 1/4\", ASTM F436",null,null,"64.4","LB",null,"BOLT","3b3c3450-918e-4d27-87f5-2ee2057bd735","a805dbfe-7cc8-4b31-844e-997cbd368740",{"$nulls":4},"1",null,"Fasteners","TYPE=BOLT",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"1 1/4\"","20","True","6.501488","Lug Bolt","Lg, ASTM A193, B7","ASTM A193","BoltSet",null,"895"]

{"sheet":"FLANGE BLIND","index":44,"n_rows":18,"n_cols":50,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Previews","Sizes","ShapeName","L","D","ContentGeometryParamDefinition","SizeRecordId_S-ALL","PortName_S-ALL","NominalDiameter_S-ALL","NominalUnit_S-ALL","MatchingPipeOd_S-ALL","EndType_S-ALL","FlangeStd_S-ALL","GasketStd_S-ALL","Facing_S-ALL","FlangeThickness_S-ALL","PressureClass_S-ALL","Schedule_S-ALL","WallThickness_S-ALL","EngagementLength_S-ALL","LengthUnit_S-ALL","ShortDescription","CompatibleStandard","DesignStd","PartFamilyLongDesc","PartSizeLongDesc","Material","MaterialCode","Weight","WeightUnit","SKEY","TYPE","PartFamilyId","CatalogPartFamilyId","PartStatus","Manufacturer","ItemCode","DesignPressureFactor","ConnectionPortCount","ComponentDesignation","PartCategory","ContentIsoSymbolDefinition","CatalogPartId","CatalogId","PartVersion","Status","Shop_Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
["Preview","Sizes","Shape Name","L","D","ContentGeometryParamDefinition","Size Record Id_S-ALL","Port Name_S-ALL","Nominal Diameter_S-ALL","Nominal Unit_S-ALL","Matching Pipe OD_S-ALL","End Type_S-ALL","Flange Std_S-ALL","Gasket Std_S-ALL","Facing_S-ALL","Flange Thickness_S-ALL","Pressure Class_S-ALL","Schedule_S-ALL","Wall Thickness_S-ALL","Engagement Length_S-ALL","Port Unit_S-ALL","Short Description","Compatible Standard","Design Std","Long Description (Family)","Long Description (Size)","Material","Material Code","Weight","Weight Unit","SKEY","TYPE","Part Family Id","CatalogPartFamilyId","PartStatus","Manufacturer","Item Code","Design Pressure Factor","Connection Port Count","Component Designation","Part Category","Content Iso Symbol Definition","CatalogPartId","CatalogId","PartVersion","Status","Shop/Field","PnPClassName","ExcelFormatVersion_2.0","PnPID"]
[null,"1/2\"","CPFBR","0.44","3.5","L,D,","bc1f6ae8-5975-5d9f-b35a-5d04b16e8ef9","ALL","0.5","in","0.84","FL",null,null,"RF","0.44","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 1/2\" ND, 150 LB, RF, ASME B16.5",null,null,"2","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"262"]
[null,"3/4\"","CPFBR","0.5","3.88","L,D,","d5367c0e-5bda-5a30-ae6e-77130aff84d9","ALL","0.75","in","1.05","FL",null,null,"RF","0.5","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 3/4\" ND, 150 LB, RF, ASME B16.5",null,null,"2","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"263"]
[null,"1\"","CPFBR","0.56","4.25","L,D,","1161e211-487c-56a1-8e5e-1f5e9f82ccc3","ALL","1","in","1.315","FL",null,null,"RF","0.56","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 1\" ND, 150 LB, RF, ASME B16.5",null,null,"2","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"264"]
[null,"1 1/2\"","CPFBR","0.68","5","L,D,","1cce77cc-7153-599e-9ca8-b4d66ac4c055","ALL","1.5","in","1.9","FL",null,null,"RF","0.68","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 1 1/2\" ND, 150 LB, RF, ASME B16.5",null,null,"3","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"266"]
[null,"2\"","CPFBR","0.75","6","L,D,","6368e87c-8545-528b-bfcd-496837f57cf3","ALL","2","in","2.375","FL",null,null,"RF","0.75","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 2\" ND, 150 LB, RF, ASME B16.5",null,null,"4","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"267"]
[null,"3\"","CPFBR","0.94","7.5","L,D,","439fff21-bb61-5293-975c-6d613e69ceb2","ALL","3","in","3.5","FL",null,null,"RF","0.94","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 3\" ND, 150 LB, RF, ASME B16.5",null,null,"9","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"269"]
[null,"4\"","CPFBR","0.94","9","L,D,","219a40ce-88aa-5bcc-88e3-aeda308798e6","ALL","4","in","4.5","FL",null,null,"RF","0.94","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 4\" ND, 150 LB, RF, ASME B16.5",null,null,"17","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"271"]
[null,"6\"","CPFBR","1","11","L,D,","0695e62d-2986-51f1-afbb-61a9aadce329","ALL","6","in","6.625","FL",null,null,"RF","1","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 6\" ND, 150 LB, RF, ASME B16.5",null,null,"27","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"273"]
[null,"8\"","CPFBR","1.12","13.5","L,D,","d6b787b0-ca17-5098-be75-a6fa4d17f1b6","ALL","8","in","8.625","FL",null,null,"RF","1.12","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 8\" ND, 150 LB, RF, ASME B16.5",null,null,"47","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"274"]
[null,"10\"","CPFBR","1.18","16","L,D,","f1dffd5b-19cc-5d48-8fd5-2f8c0a545214","ALL","10","in","10.75","FL",null,null,"RF","1.18","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 10\" ND, 150 LB, RF, ASME B16.5",null,null,"67","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"275"]
[null,"12\"","CPFBR","1.25","19","L,D,","afeaabd8-53ad-5c80-97ad-b8969ab2f728","ALL","12","in","12.75","FL",null,null,"RF","1.25","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 12\" ND, 150 LB, RF, ASME B16.5",null,null,"123","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"276"]
[null,"14\"","CPFBR","1.37","21","L,D,","cf4777c1-fa2f-5eb2-b8ac-7a9d0d9319ab","ALL","14","in","14","FL",null,null,"RF","1.37","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 14\" ND, 150 LB, RF, ASME B16.5",null,null,"139","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"277"]
[null,"16\"","CPFBR","1.44","23.5","L,D,","31b4b021-993d-5ff2-b289-d33a362d2d4e","ALL","16","in","16","FL",null,null,"RF","1.44","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 16\" ND, 150 LB, RF, ASME B16.5",null,null,"187","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"278"]
[null,"18\"","CPFBR","1.56","25","L,D,","426af44e-e3d9-5242-8fdf-08b180be700c","ALL","18","in","18","FL",null,null,"RF","1.56","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 18\" ND, 150 LB, RF, ASME B16.5",null,null,"217","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"279"]
[null,"20\"","CPFBR","1.68","27.5","L,D,","7d306b7b-1eed-5b55-a04d-9648ff7bd5da","ALL","20","in","20","FL",null,null,"RF","1.68","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 20\" ND, 150 LB, RF, ASME B16.5",null,null,"283","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"280"]
[null,"24\"","CPFBR","1.87","32","L,D,","36cb7f9d-b283-5ec5-8995-b261b6a157f4","ALL","24","in","24","FL",null,null,"RF","1.87","150",null,null,null,"in","FLANGE BLIND","ASME B16.5",null,"FLANGE BLIND, 150 LB, RF, ASME B16.5, ASTM A234 Gr WPB","FLANGE BLIND, 24\" ND, 150 LB, RF, ASME B16.5",null,null,"415","LB","FLBL","FLANGE","04510c5e-136b-44a3-a1df-98046f4332e1","a8b3501d-30a7-4154-ad89-3cf0e928743a",{"$nulls":4},"1",null,"Flanges","TYPE=FLANGE-BLIND,SKEY=FLBL",null,"ASME Pipes and Fittings Catalog","4_0",null,null,"BlindFlange",null,"281"]